;
; VAG-COM Labelfile
;
; VW Golf/Jetta (1K) / VW Passat (3C)
;
; Component: J745 - Cornering Lights Headlight Range Control (#55)
;
; P/N: 5M0-907-357-???
;
; includes measuring blocks, security access, adaptation and coding
;
; created on 17/Dec/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 17/Dec/2005
;
; requires VAG-COM 505.1 or higher
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,1,Voltage,(Terminal 15)
001,2,Light Status,(Terminal 56b),Display Range: ON/OFF
001,3,Vehicle Speed
001,4,Steering Angle,Sensor (G85)
;
002,1,Sensor Signal,Front (G78/G289)
002,2,Sensor Signal,Rear (G76/G77)
;
080,0,Advanced Control Module Identification I
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Brake Electronics,(J104),Specification: ABS 1\nDisplay Range: ABS 1/ABS 0
125,2,CAN-Gateway,(J533),Specification: Gateway 1\nDisplay Range: Gateway 1/Gateway 0
125,3,Power Steering,(J500),Specification: Steer. ang. 1\nDisplay Range: Steer. ang. 1/Steer. ang. 0
125,4,Engine,Electronics,Specification: Engine 1\Display Range: Engine 1/Engine 0
;
127,0,CAN-Databus Communication (Light)
127,1,Left Output,Stage (J667),Specification: LeiMo Left 1\nDisplay Range: LeiMo Left 1/LeiMo Left 0
127,2,Right Output,Stage (J668),Specification: LeiMo Right 1\nDisplay Range: LeiMo Right 1/LeiMo Right 0
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Cornering Lights Headlight Range Control (J745) Coding
C01,0000001 - VW Passat (3C) Left-Hand-Drive / Rest of World
C02,0000004 - VW Golf/Jetta (1K/5M) Left-Hand-Drive / Rest of World
C03,0000006 - VW Passat (3C) Right-Hand-Drive / Rest of World
C04,0000007 - VW Passat (3C) Left-Hand-Drive / North America
C05,0000012 - VW Golf/Jetta (1K/5M) Right-Hand-Drive / Rest of World
C06,0000013 - VW Golf/Jetta (1K/5M) Left-Hand-Drive / North America
;
;
;---------------------------------------------------
;
; security access information
;
;---------------------------------------------------
;
;
S00,Cornering Lights Headlight Range Control (J745) Security Access
S01,15284 - General Adaptation "Enabling"
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A016,0,Tourist Solution
A016,5,Tourist Solution
A016,6,When driving in countries where driving is performed on the
A016,7,opposite side as in the native country the headlights must
A016,8,be changed over to avoid blinding the oncoming traffic.
A016,9, 
A016,10,0 = Disabled
A016,11,1 = Enabled
;
