;
; VAG-COM Labelfile
;
; VW Passat (3C)
;
; Component: J393 - Central Module Comfort System (#46)
;
; P/N: 3C0-959-433-???
;
; includes measuring blocks, adaptation and selective output test
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 3C-46.LBL
; 3C0-959-433-46.LBL
;
; created on 30/Oct/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 08/Nov/2005
;
; requires VAG-COM 505.1 or higher
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Door Contact Switches
001,1,Driver Door,Door Contact (F2),Display Range: Door Closed/Door Open
001,2,Passenger Door,Door Contact (F3),Display Range: Door Closed/Door Open
001,3,Rear Left Door,Door Contact (F10),Display Range: Door Closed/Door Open
001,4,Rear Right Door,Door Contact (F11),Display Range: Door Closed/Door Open
;
002,0,Central Locking Units
002,1,Driver Door,Status (F220),Display Range: Locked/Unlocked/Safe/Implausible
002,2,Passenger Door,Status (F221),Display Range: Locked/Unlocked/Safe/Implausible
002,3,Rear Left Door,Status (F222),Display Range: Locked/Unlocked/Safe/Implausible
002,4,Rear Right Door,Status (F223),Display Range: Locked/Unlocked/Safe/Implausible
;
003,0,Key Switches && Interior Lock Buttons
003,1,Driver Door,Key Switch,Display Range: Not Oper./Open/Close/Implausible
003,2,Passenger Door,Key Switch,Display Range: Not Oper./Open/Close/Implausible
003,3,Driver Door,Lock Butt. (E308),Display Range: Not Oper./Locking/Unlocking/Implausible
003,4,Passenger Door,Lock Butt. (E308),Display Range: Not Oper./Locking/Unlocking/Implausible
;
004,0,Rear Lid
004,1,Rear Lid,Key Switch,Display Range: Open/Close/Not Oper.
004,2,Rear Lid Handle,Unlock Sw. (E234),Display Range: Not Oper./Operated
004,3,Rear Lid Lock Unit,(F256) Main Latch,Display Range: Open/Closed
004,4,Rear Lid Lock Unit,(F256) Pre-Latch,Display Range: Open/Closed
;
005,0,Power Supply
005,1,Voltage,(Terminal 30),Specification: 9.0...14.0 V
005,2,Voltage Status,,?x = Terminal 30\nx? = Terminal 30a
005,3,Terminal 15,Status,Display Range: Term 15 On/Term 15 Off
005,4,S-Contact,Status,Display Range: Activated/Inactive
;
006,1,Vehicle Speed
006,2,Crash Signal,,Display Range: Yes/No
006,3,Request to,Open Tank Lid,Display Range: Yes/No
;
007,1,Enabling Sunroof,,Display Range: Yes/No
007,2,Sunroof Control,,Display Range: Not Oper./Open/Closed
007,3,Comfort Function,,Display Range: Not Installed
;
008,1,Terminal 58d,Request,Display Range: 0.0...100.0 %
008,2,Terminal 58s,Signal,Display Range: 0.0...100.0 %
008,3,Door Handle,Illum. Request,Display Range: Not Installed
008,4,Door Handle,Illum. Signal,Display Range: Not Installed
;
009,1,Central Locking,Thermal Protection,Display Range: Yes/No
009,2,Signal:,Doors not Closed,Display Range: Open/Closed
009,3,Rear Left,Entry Light (W33),Display Range: ON/OFF/Not Installed
009,4,Rear Right,Entry Light (W34),Display Range: ON/OFF/Not Installed
;
010,0,Remote Control
010,1,Remote Control,Key Number,0 = No Key recognized\n1 = Key 1\n2 = Key 2\n3 = Key 3\n4 = Key 4	
010,2,Remote Control,Buttons,Display Range: 0 = Not Operated / 1 = Operated\n\n?xxx = Open\nx?xx = Close\nxx?x = Rear Lid\nxxx? = Panic (USA only)
;
011,0,Immobilizer
011,1,Fixed Code,,Display Range: No Value/OK/Not OK
011,2,Code in,Catch Area,Display Range: No Value/OK/Not OK
011,3,Algorithm,,Display Range: No Value/OK/Not OK
;
012,1,Immobilizer,Key Recognition,Display Range: Yes/No
012,2,Rear Lid Remote,Lock Sw. (E233),Display Range: Not Oper./Operated
012,3,Rear Lid Handle,Unlock Sw. (E234),Display Range: Yes/No
012,4,Front Hood,Switch (F266),Display Range: Open/Closed
;
013,1,Telematics,,Display Range: Open/Closed/Not Oper./Not Installed
013,2,Interior Monitoring,Sensor (G273),Display Range: Not Installed
;
014,0,Interior Monitoring Sensor (G273)
014,1,Interior Monitoring,Status,Display Range: Active/Inactive/Not Installed
014,2,Interior Monitoring,Alarm Recognized,Display Range: Yes/No/Not Installed
014,3,Interior Monitoring,Output Active,Display Range: ON/OFF/Not Installed
014,4,Interior Monitoring,Output Active,Display Range: ON/OFF/Not Installed
;
015,0,Vehicle Inclination Sensor (G384)
015,1,Incl. Sensor (G384),Status,Display Range: Active/Inactive/Not Installed
015,2,Incl. Sensor (G384),Alarm Recognized,Display Range: Yes/No/Not Installed
015,3,Incl. Sensor (G384),Output Active,Display Range: ON/OFF/Not Installed
015,4,Incl. Sensor (G384),Indic. Lamp (K188),Display Range: Operated/Not Operated/Not Installed
;
016,0,Alarm Horn (H12)
016,1,Alarm Horn (H12),Status,Display Range: Active/Inactive/Not Installed
016,2,Alarm Horn (H12),Alarm Recognized,Display Range: Yes/No/Not Installed
016,3,Alarm Horn (H12),Output Active,Display Range: ON/OFF/Not Installed
;
017,0,Vehicle Inclination Sensor (G384)
017,1,X-Reference,Angle,Specification: -25.2...+25.4 °\nDisplay Range: No Value/Not Installed
017,2,Current,X-Delta Angle,Specification: -12.6...+12.7 °\nDisplay Range: No Value/Not Installed
017,3,Y-Reference,Angle,Specification: -25.2...+25.4 °\nDisplay Range: No Value/Not Installed
017,4,Current,Y-Delta Angle,Specification: -12.6...+12.7 °\nDisplay Range: No Value/Not Installed
;
018,0,Alarm Horn (H12) Trigger
; 0 = No Alarm Trigger
; 1 = Comfort Control Module
; 2 = Open Circuit on Ground
; 3 = Open Circuit on Plus
; 4 = Intelligent Battery Analysis
018,1,1st Alarm Trigger,,0 = No Alarm Trigger\n1 = Comfort Control Module\n2 = Open Circuit on Ground\n3 = Open Circuit on Plus\n4 = Intelligent Battery
018,2,2nd Alarm Trigger,,0 = No Alarm Trigger\n1 = Comfort Control Module\n2 = Open Circuit on Ground\n3 = Open Circuit on Plus\n4 = Intelligent Battery
018,3,3rd Alarm Trigger,,0 = No Alarm Trigger\n1 = Comfort Control Module\n2 = Open Circuit on Ground\n3 = Open Circuit on Plus\n4 = Intelligent Battery
018,4,Alarm Trigger,Counter
;
019,0,Interior Monitoring Sensor (G273) Trigger
019,1,1st Alarm Trigger
019,2,2nd Alarm Trigger
019,3,3rd Alarm Trigger
019,4,4th Alarm Trigger
;
020,0,Alarm Sources
020,1,1st Alarm Source
020,2,2nd Alarm Source
020,3,3rd Alarm Source
020,4,4th Alarm Source
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A000,0,Remote Control Erasing
A000,5,Remote Control Erasing
A000,6,0 - Erase all keys
;
A001,0,Remote Control Adaptation
A001,1,Key
A001,2,Adaptation
A001,3,Current Number,of Keys
A001,5,Remote Control Adaptation
A001,6,Enter the number of keys that should be adapted. Save.
A001,7, 
A001,8,Now press button 1 or 2 on every remote that
A001,9,should be adapted for at least 1 second.
A001,10, 
A001,11,Note #1: All keys must be adapted in one procedure.
A001,12,Note #2: Adaptation of all keys must not exceed 15 seconds.
;
A003,0,Selective (Single) Door Locking
A003,3,Current Status
A003,5,Selective (Single) Door Locking
A003,6,Display Range: 0 = OFF / 1 = ON
;
A004,0,Auto-Lock
A004,1,Auto-Lock
A004,3,Current Status
A004,5,Auto-Lock
A004,6,The doors will lock automatically when the
A004,7,vehicle reaches a speed of 15 km/h or 10 mph.
A004,8, 
A004,9,Specification: 0 = OFF / 1 = ON
;
A005,0,Auto-Unlock
A005,1,Auto-Unlock
A005,3,Current Status
A005,5,Auto-Unlock
A005,6,The doors will unlock automatically when
A005,7,the key is removed from the ignition switch.
A005,8, 
A005,9,Specification: 0 = OFF / 1 = ON
;
A007,0,Unlocking Confirmation (Remote Control)
A007,1,Unlocking,Confirmation
A007,2,via,Remote Control
A007,3,Current Status
A007,5,Unlocking Confirmation (Remote Control)
A007,6,Type of confirmation when unlocking
A007,7,the car via remote control.
A007,8, 
A007,9,0 = OFF
A007,10,1 = Blink
A007,11,2 = Beep (Horn)
A007,12,3 = Beep (Horn) & Blink
;
A008,0,Unlocking Confirmation (Key Switch)
A008,1,Unlocking,Confirmation
A008,2,via,Key Switch
A008,3,Current Status
A008,5,Unlocking Confirmation (Key Switch)
A008,6,Type of confirmation when unlocking
A008,7,the car via key switch.
A008,8, 
A008,9,0 = OFF
A008,10,1 = Blink
A008,11,2 = Beep (Horn)
A008,12,3 = Beep (Horn) & Blink
;
A010,0,Locking Confirmation (Remote Control)
A010,1,Locking,Confirmation
A010,2,via,Remote Control
A010,3,Current Status
A010,5,Locking Confirmation (Remote Control)
A010,6,Type of confirmation when locking
A010,7,the car via remote control.
A010,8, 
A010,9,0 = OFF
A010,10,1 = Blink
A010,11,2 = Beep (Horn)
A010,12,3 = Beep (Horn) & Blink
;
A011,0,Locking Confirmation (Key Switch)
A011,1,Locking,Confirmation
A011,2,via,Key Switch
A011,3,Current Status
A011,5,Locking Confirmation (Key Switch)
A011,6,Type of confirmation when locking
A011,7,the car via key switch.
A011,8, 
A011,9,0 = OFF
A011,10,1 = Blink
A011,11,2 = Beep (Horn)
A011,12,3 = Beep (Horn) & Blink
;
A012,0,Safe Confirmation
A012,1,Safe,Confirmation
A012,3,Current Status
A012,5,Safe Confirmation
A011,6,Type of confirmation when
A011,7,the car is beeing safed.
A011,8, 
A011,9,0 = OFF
A011,10,1 = Blink
A011,11,2 = Beep (Horn)
A011,12,3 = Beep (Horn) & Blink
;
A013,0,Alarm Horn Adjustment
A013,5,Alarm Horn Adjustment
A013,6,Country setting for alarm horn. This changes length
A013,7,and volume of the alarm horn sounding.
A013,8, 
A013,9,0 - Great Britain (Frequency Modulated - 10 Tamper Alarms)
A013,10,1 - Great Britain (Frequency Modulated - 1 Tamper Alarm)
A013,11,2 - Rest of World (Discontinuous - 10 Tamper Alarms)
A013,12,3 - Rest of World (Discontinuous - 1 Tamper Alarm)
;
A017,0,Comfort Function (Remote Control)
A017,1,Comfort Function
A017,2,Remote Control
A017,3,Current Status
A017,5,Comfort Function
A017,6,Display Range: 0 = OFF / 1 = ON
A017,7, 
A017,8,NOTE: See long coding for more details/options.
;
A018,0,Alarm Delay
A018,1,Alarm Delay
A018,2,Driver Door
A018,3,Current Status
A018,5,Alarm Delay
A018,6,Deactivation of the anti theft warning delay
A018,7,when opening drivers door before the anti theft
A018,8,warning system is beeing activated.
A018,9, 
A018,10,Display Range: 0 = OFF / 1 = ON
;
A019,0,Factory Mode
A019,3,Current Status
A019,5,Factory Mode
;
;
;---------------------------------------------------
;
; selective output test information
;
;---------------------------------------------------
;
;
T94,Rear Left Central Locking Motor (V214)
T95,Rear Right Central Locking Motor (V215)
T327,Open Sliding Sunroof
T948,Close Sliding Roof
T379,Activate Terminal 58s
T1134,Alarm Horn (H12)
T1338,Signal: Doors Not Closed
T332,Open Tank Flap
T1699,Hatch/Trunk Central Locking Motor (V53)
T2483,Rear Lid Locking Module (F327)
;
