;
; VAG-COM labelfile
;
; component: R - Radio (#56) - GAMMA
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1C-56.LBL
; 1J-56.LBL
; 1J0-035-15x.LBL
; 1J0-035-18x.LBL
;
; created on 02/Jun/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 02/Jun/2005
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,GALA-Signal
001,2,Supply Voltage,(Terminal 30)
001,3,Illumination,(Terminal 58d)
001,4,Status,S-Contact
;
002,0,Speakers
002,1,Speakers,front
002,2,Status,,Specification: OK/short/open
002,3,Speakers,rear
002,4,Status,,Specification: OK/short/open
;
003,0,Antenna
003,1,Antenna Type,,Specification: active/passive
003,2,Antenna
003,3,Status,,Specification: OK/short/open
;
004,0,Amplifier / Telephone-Mute
004,1,Amplifier,Output,Specification:\n0 = OK\n1 = Short to ground
004,3,Telephone,Mute
004,4,Status,,Specification: on/off
;
005,0,CD-Player/Changer
005,1,CD-Drive
005,2,Status,,Specification: OK/n.OK
;
006,0,External Display
006,1,External Display
006,2,Status,,Specification: OK/n.OK
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,Radio (R) Coding
C1,??xxx: Sound-Adjustment
C2,00 - Grundkurve / 01 - Golf (1J) / 02 - Bora (1J)
C3,03 - Golf/Bora Variant (1J) / 04 - Passat Limousine (3B/3BG)
C4,05 - Passat Variant (3B/3BG) / 06 - Lupo/Polo / 07 - Golf-Cabriolet (1E)
C5,08 - Sharan (7M) / New Beetle (1C) / 09 - Transporter/Caravelle (7D)
C6,xx?xx: Speakers
C7,0 - no passive Speakers (DSP)
C8,2 - 2 passive Speakers (front)
C9,3 - 2 passive Speakers (rear)
C10,4 - 4 passive Speakers (front and rear)
C11,xxx?x: Soundsystem-Correction
C12,0 - no Correction (w/o DSP)
C13,1 - with Bose-Soundsystem
C14,2 - Sound-System (DSP)
C15,xxxx?: Radio-Configuration
C16,+0 - Radio with passiver Antenna
C17,+1 - Active/Remote Supplied Antenna
C18,+2 - CD-Player/Changer
C19,+4 - External Display in Instrument Cluster
;
