;
; VAG-COM label file
;
; Audi A4 (8EC/8ED)
;
; component: J285 - Instrument cluster (#17)
;
; p/n: 8E0-920-9??-??
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8E-17.LBL
; 8E0-920-9xx-8E2.LBL
; 8E0-920-9xx-8ED.LBL
;
; created on 07/Sep/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 07/Sep/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Display range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,Basic Functions
002,1,Odometer
002,2,Remote Clock,Receiver Status,Display range: OK/not OK
002,3,Comfort-CAN,Information,xx0 - Left-Hand-Drive (LHD)\nxx1 - Right-Hand-Drive (RHD)\nx1x - Four-Door\n1xx - Temperature Display in °F
002,4,Outside,Temperature
;
003,0,Basic Functions
003,1,Coolant,Temperature
003,2,Standing Time
003,3,Dimming Signal,(Terminal 58d)
003,4,Dimming Signal,(Terminal 58s)
;
004,0,Fuel Level Sensor
004,1,Fuel Display,(1st Sensor)
004,2,Fuel Sensor,(1st Sensor)
004,3,Fuel Display,(2nd sensor),All wheel drive only
004,4,Fuel Sensor,(2nd sensor),All wheel drive only
;
005,0,Service Reminder
005,1,Distance,before/after Service,Unit: 100 km
005,2,Time,before/after Service,Unit: 1 day(s)
005,3,Engine Hood,Contact,Display Range: Open/Closed
005,4,Calculated,Service Interval
;
006,0,Oil Level I
006,1,Min. Oil Level,in Service Interval
006,2,Max. Oil Level,in Service Interval
006,3,100 km Average,Oil Level Dif.
;
007,0,Oil Level II
007,1,Current,Oil Level
007,2,Oil Level,Threshold,Current Value from ECU
;
022,0,Immobilizer I
022,1,Engine Start,permitted,Specification: 1 = Yes\nDisplay Range: 0 = No / 1 = Yes
022,2,Engine (ECU),responds,Specification: 1 = Yes\nDisplay Range: 0 = No / 1 = Yes
022,3,Key Status,,Specification: 1 = Key OK\nDisplay Range: 0 = Key not OK / 1 = Key OK
022,4,Number of,adapted Keys,Specification: 1...8
;
023,0,Immobilizer II
023,1,Variable Code,authorized,Specification: 1 = Yes\nDisplay Range: 0 = No / 1 = Yes
023,2,Key Status,(Transponder),Display Range: 0 = not locked / 1 = locked
023,3,Fixed Code,authorized,Specification: 1 = Yes\nDisplay Range: 0 = No / 1 = Yes
023,4,Immobilizer,Status,Specification: 6 (Immobilizer adapted)
; 4 - New Customer Service / Delivery Condition (Replacement Instrument Cluster)
; 5 - Customer Service locked / Adaptation Data Programmed in Customer Service
; 6 - Immobilizer adapted / Normal Function Condition
; 7 - Key Adaptation active
;
024,0,Immobilizer II
024,1,Lock-Time,Instrument Cluster
024,2,Lock-Time,Engine (ECU)
024,3,Lock-Time,Emergency Unlock
024,4,Lock-Time,Transponder
;
050,0,Misc Functions
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Identification Number (VIN) & Serial Number
;
082,0,Advanced Control Module Identification III
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine,,Specification: Engine 1\nDisplay Range: Engine 0/Engine 1
125,2,Transmission
125,3,Brake Electronics,(J104),Specification: ABS 1\nDisplay Range: ABS 0/ABS 1
;
126,0,CAN-Databus Communication (Powertrain)
126,1,Airbag,(J234),Specification: Airbag 1\nDisplay Range: Airbag 0/Airbag 1
126,2,Headlight Range,,Specification: HdLtRange 1\nDisplay Range: HdLtRange 0/HdLtRange 1
;
130,0,CAN-Databus Communication (Comfort)
130,3,Comfort System,(J393),Specification: Central 1\nDisplay Range: Central 0/Central 1
;
131,0,CAN-Databus Communication (Comfort)
131,1,Central Electronics,(J519),Specification: Cent Elec 1\nDisplay Range: Cent Elec 0/Cent Elec 1
131,2,Steering Column,Electronics (J527),Specification: St. Wheel 1\nDisplay Range: St. Wheel 0/St. Wheel 1
131,3,Climate Control,(J255),Specification: A/C 1\nDisplay Range: A/C 0/A/C 1
131,4,Status,CAN-Comfort,Specification: 2-Wire\nDisplay Range: 1-Wire/2-Wire
;
132,0,CAN-Databus Communication (Comfort)
132,1,Convertible Top
;
140,0,CAN-Databus Communication (Infotainment)
140,1,Radio,,Specification: Radio 1\nDisplay Range: Radio 0/Radio 1
;
141,0,CAN-Databus Communication (Infotainment)
141,4,Status,CAN-Infotainment,Specification: 2-Wire\nDisplay Range: 1-Wire/2-Wire
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,Instrument Cluster (J285) Coding
C1,??xx1:  Extra Options
C2,+00 - 1. K-Number (Europe/USA/Rest of World)
C3,+01 - Smaller Fuel Tank Volume (All wheel drive)
C4,+02 - Side Marker Lights Indicator Lamp inactive
C5,+04 - 3. K-Number (Rental Cars)
C6,+08 - 2. K-Number (Australia)
C7,+16 - Clutch Pedal Switch Operation in FIS Display
C8,xx?x1: Country
C9,0 - Germany (D) / 1 - Rest of World (RoW) / 2 - USA (US)
C10,3 - Canada (CAN) / 4 - Great Britain (GB) / 5 - Japan (JP)
C11,6 - Saudi Arabia / 7 - Australia (AUS)
C12,xxx?1: Seatbelt Warning
C13,0 - No Seatbelt Warning
C14,1	- Seatbelt Warning Europe-NCAP
C15,2 - Seatbelt Warning USA and Canada old
C16,3 - Seatbelt Warning USA and Canada NAR neu
C17,4 - Seatbelt Warning Europe-NCAP (incl. passenger)
C18,5 - Seatbelt Warning USA and Canada old (incl. passenger)
C19,6 - Seatbelt Warning USA and Canada NAR new (incl. passenger)
;
;
;---------------------------------------------------
;
; security access informations
;
;---------------------------------------------------
;
;
S0,Instrument Cluster (J285) Security Access
S1,13861 - General Adaptation "Enabling"
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 - Service NOT Due
A002,7,1 - Service Due
A002,8, 
A002,9,To reset the service reminder save 00000 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 5 %
;
A004,0,Language
A004,5,Language
A004,6,1 - German
A004,7,2 - English
A004,8,3 - French
A004,9,4 - Italian
A004,10,5 - Spanish
A004,11,6 - Portuguese
A004,12,8 - Chinese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km/62 mi.
A009,11, 
A009,12,NOTE: Perform Security Access with "13861" first.
;
A018,0,Auxiliary Heating
A018,5,Auxiliary Heating
A018,6,000?x: Engine pre-warm-up
A018,7,0 - without Engine pre-warm-up
A018,8,1 - with Engine pre-warm-up
A018,9, 
A018,10,000x?: Auxiliary Heating
A018,11,0 - No Auxiliary Heating installed
A018,12,1 - Auxiliary Heating installed
A018,13,2 - Auxiliary Heating installed and goes out when turning Engine OFF
A018,14,3 - Only Auxiliary Ventilation
A018,15,4 - Only Auxiliary Ventilation and goes out when turning engine OFF
;
A019,0,Additional Features
A019,5,Additional Features
A019,6,?xxxx: Illumination
A019,7,0 - Needle and Scale only active at "Light ON"
A019,8,1 - Needle already active at "Ignition ON"
A019,9,2 - Scale already active at "Ignition ON"
A019,10,3 - Scale (2nd Map) and Needle at "Ignition ON" active
A019,11,x?xxx: Board computer
A019,12,0 - only Level 2 (Long Time Memory)
A019,13,1 - Level 1 and 2
A019,14,xx?xx: Driver Information System (DIS)
A019,15,0 - DIS / 1 - Highline without DIS
A019,16,2 - DIS with Menu Guide / 3 - DIS with Menu Guide and Unit Changing
A019,17,xxx?x: Outside Temperature
A019,18,0 - No Display/Illumination inactive
A019,19,1 - Display and Illumination active
A019,20,xxxx?: Remote Clock
A019,21,0 - Remote Clock not active / 1 - Remote Clock active
;
A029,0,Tank Characteristic (Fuel Level Sensor 2)
A029,5,Tank Characteristic (Fuel Level Sensor 2)
A029,6,Parallel shift of tank characteristic by +/- 32 Ohm
A029,7,Value Range: 96...160
;
A030,0,Tank Characteristic (Fuel Level Sensor 1)
A030,5,Tank Characteristic (Fuel Level Sensor 1)
A030,6,Parallel shift of tank characteristic by +/- 32 Ohm
A030,7,Value Range: 96...160
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A038,0,Oil Minimum Detection
A038,5,Oil Minimum Detection
A038,6,With this function the oil-minimum-warning at
A038,7,low oil level can be deactivated or activated.
A038,8,0 - Oil Minimum Detection not activated
A038,9,1 - Oil Minimum Detection activated
A038,10, 
A038,11,NOTE: Perform Security Access with "13861" first.
;
A039,0,Oil Level Sensor Adaptation
A039,5,Oil Level Sensor Adaptation
A039,6,Determines if the TOG Sensor is installed or not.
A039,7,0 - TOG Evaluation from the Instrument Cluster not activated
A039,8,1 - TOG Evaluation from the Instrument Cluster activated
A039,9, 
A039,10,NOTE: Perform Security Access with "13861" first.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km
A040,7, 
A040,8,NOTE: Adaptation channels 40-49 must be
A040,9,entered and stored in the following order:
A040,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
A041,7, 
A041,8,NOTE: Adaptation channels 40-49 must be
A041,9,entered and stored in the following order:
A041,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 100 km
A042,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A042,8,00150 - flexible Service Intervals (15.000 km - with Longlife)
A042,9,or (if coded to miles)
A042,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A042,11,00090 - flexible Service Intervals (9.000 mi - with Longlife)
A042,12, 
A042,13,NOTE: Adaptation channels 40-49 must be
A042,14,entered and stored in the following order:
A042,15,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 100 km
A043,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A043,8,00300 - flexible Service Intervals (30.000 km - with Longlife)
A043,9,or (if coded to miles)
A043,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A043,11,00190 - flexible Service Intervals (19.000 mi - with Longlife)
A043,12, 
A043,13,NOTE: Adaptation channels 40-49 must be
A043,14,entered and stored in the following order:
A043,15,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 - fixed Service Intervals (w/o Longlife)
A044,8,00730 - flexible Service Intervals (with Longlife)
A044,9, 
A044,10,NOTE: Adaptation channels 40-49 must be
A044,11,entered and stored in the following order:
A044,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 - fixed Service Intervals (w/o Longlife)
A045,7,2 - flexible Service Intervals (with Longlife)
A045,8,3 - Diesel Engines with Immobilizer III
A045,9, 
A045,10,NOTE: Adaptation channels 40-49 must be
A045,11,entered and stored in the following order:
A045,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display
A046,8, 
A046,9,NOTE: Adaptation channels 40-49 must be
A046,10,entered and stored in the following order:
A046,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
A047,9, 
A047,10,NOTE: Adaptation channels 40-49 must be
A047,11,entered and stored in the following order:
A047,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
A048,9, 
A048,10,NOTE: Adaptation channels 40-49 must be
A048,11,entered and stored in the following order:
A048,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A049,0,Minimum Time to Service
A049,5,Minimum Time to Service
A049,6,Increments: 1 = 1 day(s)
A049,7,00365 - fixed Service Intervals (w/o Longlife)
A049,8,00365 - flexible Service Intervals (Gasoline Engines with Longlife)
A049,9,00730 - flexible Service Intervals (Diesel Engines with Longlife)
A049,10, 
A049,11,NOTE: Adaptation channels 40-49 must be
A049,12,entered and stored in the following order:
A049,13,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A060,0,CAN-Databus Powertrain (Installation List)
A060,5,CAN-Databus Powertrain (Installation List)
A060,6,+00001 - Engine (Standard)
A060,7,+00002 - Automatic Transmission (Optional)
A060,8,+00004 - Brake (Standard)
A060,9,+00008 - Airbag (Standard)
A060,10,+01024 - Instrument Cluster (Standard)
;
A061,0,CAN-Databus Comfort (Installation List)
A061,5,CAN-Databus Comfort (Installation List)
A061,6,+00001 - Central Electronics (Standard)
A061,7,+00002 - Comfort System (Standard)
A061,8,+00064 - Trailer (Optional)
A061,9,+00128 - Convertible Top (Optional)
A061,10,+00256 - Instrument Cluster (Standard)
A061,11,+00512 - Tire Pressure Control (Optional)
A061,12,+01024 - Steering Column Electronics (Standard)
A061,13,+02048 - Climate Control (Standard)
A061,14,+32768 - Auxiliary Heating (Optional)
;
A062,0,CAN-Databus Infotainment (Installation List)
A062,5,CAN-Databus Infotainment (Installation List)
A062,6,+00001 - Radio (Optional)
A062,7,+00002 - Telephone (Optional)
A062,8,+00004 - Navigation (Optional)
A062,9,+00008 - Telematics (Optional)
A062,10,+00016 - Intrument Cluster (Standard - only coded with 2nd Component)
;
A099,0,Transport Mode
A099,5,Transport Mode
A099,6,0 - inactive
A099,7,1 - active
A099,8, 
A099,9,Some Head units require a seperate transport mode
A099,10,deactivation (Adress 56 - Adaptation channel 099).
;
