;
; VAG-COM Labelfile
;
; VW Golf/Jetta (1J/9M) / VW Lupo (6E/6X) / VW Passat (3B) / VW Polo (6N)
;
; Component: A/C Heating Electronics (J255) (#01) - Climatronic
;
; P/N: 3B?-907-044-???
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 3B-08.LBL
; 3Bx-907-044.LBL
;
; created on 27/Aug/2001 by Jens Ulmer
; updated/enhanced on 15/Apr/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
000,0,Basic Setting (Specified Value: 0)
000,1,Temperature Regulator Flap Motor (V68),Specified Value: 0
000,2,Central Air Flap Motor (V70),Specified Value: 0
000,3,Footwell/Defroster Flap Motor (V85),Specified Value: 0
000,4,Air Flow Flap Motor (V71),Specified Value: 0
;
001,0,General Values
1,1,A/C clutch,sw-off cond. 1-12 
001,2,Engine Speed,recognized,Display Range: 0 = no/1 = yes
001,3,Vehicle Speed,,Display Range: 0...255 km/h
001,4,Standing Time,,Specification: 0...240 Min | 250 = Battery disconnected | 255 = Transfer Malfunction
;
002,0,Temperature Regulator Flap Motor (V68)
002,1,Measured Value,,Display Range: 0...255
002,2,Specified Value,,Display Range: 0...255
002,3,Flap Position,(air supply cooled),Specification: 150...250
002,4,Flap Position,(air supply heated),Specification: 5...100
;
003,0,Central Air Flap Motor (V70)
003,1,Measured Value,,Display Range: 0...255
003,2,Specified Value,,Display Range: 0...255
003,3,Flap Position,(air flow to panel),Specification: 150...250
003,4,Flap Position,(air flow to footwell),Specification: 5...100
;
004,0,Footwell/Defroster Flap Motor (V85)
004,1,Measured Value,,Display Range: 0...255
004,2,Specified Value,,Display Range: 0...255
004,3,Flap Position,(air flow to footwell),Specification: 150...250
004,4,Flap Position,(air flow to defrost.),Specification: 5...100
;
005,0,Air Flow Flap Motor (V71)
005,1,Measured Value,,Display Range: 0...255
005,2,Specified Value,,Display Range: 0...255
005,3,Flap Position,(fresh air flow),Specification: 150...250
005,4,Flap Position,(recirculating),Specification: 5...100
;
006,0,Temperatures I && Photo Sensor
006,1,Calculated,Temperature,Calculated from temperature sensor (G89) and outside air temperature sensor (G17)
006,2,Fresh Air Duct,Temperature (G89)
006,3,Outside Air,Temperature (G17)
006,4,Sunlight Photo,Sensor (G107),Display Range: 0...120 %
; 
007,0,Temperatures II
007,1,Temperature at,Center Outl. (G191)
007,2,Temperature at,Floor Outlet (G192)
007,3,Temperature at,A/C Panel (G56)
;
008,0,Voltages
008,1,Fresh Air Blower,(V2 - specified),Display Range: 0 V = Blower Off / 3.6 V = Blower Speed 1 / 12 V = Blower Speed 7
008,2,Fresh Air Blower,(V2 - actual),Specification: ± 0.8 V to Specification (in Field 1)
008,3,Voltage,(Terminal 15)
008,4,Voltage,A/C Clutch (N25)
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,A/C Heating Electronics (J255) Coding
C1,?xxxx - Compressor Version
C2,0 - Internally regulated
C3,1 - Internally regulated with temp. sensor behind evaporator
C4,2 - Externally regulated
C5,x?xxx - Vehicle Type
C6,1 - Golf/Jetta (1J/9M) / 2 - VW Passat (3B - < MY 1999)
C7,3 - VW New Beetle (1C/9C) / 4 - VW Polo (6N)
C8,5 - VW Passat mit L-Klappe (3BG - MY 2000 >)
C9,6 - VW Lupo (6E/6X) / 7 - VW Passat W8 (3BG) / 8 - VW Golf Cabrio (1E)
C10,xx?xx - Country
C11,0 - Rest of World / 1 - Japan / 2 - USA
C12,xxx?x - Engine Cooling
C13,0 - w/o characteristic map cooling
C14,1 - with characteristic map cooling
C15,xxxx? - Equipment
C16,0 - with outside temperature indication
C17,1 - w/o outside temperature indication
;
