;
; VAG-COM label file
;
; VW Golf (1K) / VW Touran (1T) / VW Caddy (2K) / Seat Altea (5P)
; Skoda Octavia (1Z)
;
; component: J285 - instrument cluster (#17)
;
; p/n: 1K0-920-???-???
;
; tested with: 1K0 920 870 F
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-17.LBL
; 1T-17.LBL
; 1Z-17.LBL
; 2K-17.LBL
; 5P-17.LBL
; 1K-25.LBL
; 1T-25.LBL
; 1Z-25.LBL
; 2K-25.LBL
; 5P-25.LBL
; 1K0-920-xxx-17.LBL
; 1K0-920-xxx-25.LBL
;
; created on 19/Oct/2004 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 29/Sep/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,0,Speed / Engine speed / Oil pressure / Time
001,1,Speed
001,2,Engine Speed
001,3,Oil pressure, 0.9 bar
001,4,Time
;
002,0,Distance / Fuel / Ambient temperature
002,1,Odometer
002,2,Fuel level (l)
002,3,Fuel Sender,Resistance
002,4,Ambient,temperature
;
003,0,Coolant and Oil
003,1,Coolant Temp
003,2,Oil level,(Ok/n.Ok)
003,3,Oil,temperature
003,4,[N/A]
;
004,0,Voltage supply
004,1,Voltage
004,2,[N/A]
004,3,[N/A]
004,4,[N/A]
;
005,0,Service reminder informations
005,1,Service,timeout
005,2,Service,timeout
005,3,Remaining,distance
005,4,Remaining,time
;
006,0,Service reminder informations (oil) [SI = service interval]
006,1,Min. oil,in last SI
006,2,Max. oil,in last SI
006,3,Long time,avarage,Oil level difference
006,4,[N/A]
;
007,0,Unknown
;
012,0,Mileage/Days since last service
012,1,Adaptation,channel
012,2,Mileage,since service
012,3,Adaptation,channel
012,4,Days,since service
;
013,0,Mileage minimum/maximum (Service reminder limit)
013,1,Adaptation,channel
013,2,Mileage,minimum
013,3,Adaptation,channel
013,4,Mileage,maximum
;
014,0,Days minimum/maximum (Service reminder limit)
014,1,Adaptation,channel
014,2,Maximum,in days
014,3,Adaptation,channel
014,4,Minimum,in days
;
015,0,Oil quality
015,1,Adaptation,channel
015,2,Oil quality
;
016,0,Soot quantity && thermal load
016,1,Adaptation,channel
016,2,Soot quantity
016,3,Adaptation,channel
016,4,Thermal,load
;
50,0,Misc
50,1,Odometer
50,2,Engine Speed
50,3,Oil,temperature
50,4,Coolant,temperature
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test numbers
;
082,0,FTC/Serial number
;
125,0,CAN-Databus Powertrain
125,1,Engine,electronics,no Display/0/1/S
125,2,[N/A]
125,3,Brake,electronics,no Display/0/1/S
125,4,[N/A]
;
126,0,CAN-Databus Powertrain
126,1,CAN-Gateway,,no Display/0/1/S
126,2,Airbag,,no Display/0/1
126,3,Steering,Assistant,no Display/0/1/S
126,4,[N/A]
;
201,1,Distance,impulse number
201,2,[Unknown]
201,3,[N/A]
201,4,[N/A]
;
202,1,[N/A]
202,2,Wheel,circumference
202,3,[N/A]
202,4,[N/A]
;
;
;---------------------------------------------------
;
; Adaptation informations
;
;---------------------------------------------------
;
;
A2,0,Service reminder
A2,5,Service reminder reset
A2,6,displayed values:
A2,7,0 - no service
A2,8,1 - service
A2,9, 
A2,10,reset:
A2,11,0 - Service reminder reset
;
A3,0,Consumption display
A3,5,consumption display adaptation
A3,6,Basic value: 100
A3,7,Range: 85 - 115
A3,8,Unit: 1 % (percent)
;
A4,0,Language for error messages and navigation (MFD only)
A4,5,Language for error messages and navigation
A4,6,1 - German
A4,7,2 - English
A4,8,3 - French
A4,9,4 - Italian
A4,10,5 - Spanish
A4,11,6 - Portuguese
A4,12,7 - No Text
A4,13,8 - Czech
;
A22,0,Production Mode
;
A25,0,Unknown
;
A30,0,Fuel gauge adaptation
A30,1,Current,value
A30,5,Fuel gauge adaptation
A30,6,Basic value: 100
A30,7,Range: 120 - 136
A30,8,Unit: 1 Ohm
;
A35,0,Engine speed threshold
A35,5,Engine speed threshold adaptation
A35,6,Basic value: 0
A35,7,Range: 0 - 1000
A35,8,Unit: 250 U/min
;
A38,0,Oil minimum detection
;
A39,0,TOG-Sensor
A39,5,Temperatur and Oil Level Sensor (TOG)
A39,6,Deactivation of the temperatur and oil level sensor (TOG)
A39,7, 
A39,8,0 - inactive
A39,9,1 - active
;
A40,0,Distance from inspection
A40,5,Distance from inspection
A40,6,Resolution: 1 = 100 km
A40,7, 
A40,8,NOTE: Adaptation channels 40-48 must be
A40,9,entered and stored in the following order:
A40,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A41,0,Time from inspection
A41,5,Time from inspection
A41,6, 
A41,7,NOTE: Adaptation channels 40-48 must be
A41,8,entered and stored in the following order:
A41,9,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A42,0,Minimum value mileage
A42,5,Minimum value mileage
A42,6,Resolution: 1 = 1000 km
A42,7, 
A42,8,NOTE: Adaptation channels 40-48 must be
A42,9,entered and stored in the following order:
A42,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A43,0,Maximum value mileage
A43,5,Maximum value mileage
A43,6,Resolution: 1 = 1000 km
A43,7, 
A43,8,NOTE: Adaptation channels 40-48 must be
A43,9,entered and stored in the following order:
A43,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A44,0,Maximum time interval
A44,5,Maximum time interval
A44,6, 
A44,7,NOTE: Adaptation channels 40-48 must be
A44,8,entered and stored in the following order:
A44,9,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A45,0,Oil quality
A45,5,Oil quality
A45,6,Value range: 0.5 - 2.0
A45,7, 
A45,8,NOTE: Adaptation channels 40-48 must be
A45,9,entered and stored in the following order:
A45,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A46,0,Total consumption amount (Gas only)
A46,0,Total consumption amount (Gas only)
A46,6, 
A46,7,NOTE: Adaptation channels 40-48 must be
A46,8,entered and stored in the following order:
A46,9,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A47,0,Soot entry (Diesel only)
A47,5,Soot entry (Diesel only)
A47,6,Resolution: 1 = 100 km
A47,7, 
A47,8,NOTE: Adaptation channels 40-48 must be
A47,9,entered and stored in the following order:
A47,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A48,0,Thermal load (Diesel only)
A48,5,Thermal load (Diesel only)
A48,6,Resolution: 1 = 100 km
A48,7, 
A48,8,NOTE: Adaptation channels 40-48 must be
A48,9,entered and stored in the following order:
A48,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A49,0,minimum time interval
A49,5,minimum time interval
A49,6,365 - fixed service interval (12 month)
A49,7,730 - flexible service interval (24 month)
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,Instrument Cluster (J285) Coding
C1,00??x0x: Options
C2,+00 - No Options
C3,+01 - Brake Pad Warning
C4,+02 - Seatbelt Warning
C5,+04 - Washer Fluid Warning
C6,+16 - Sedan (Jetta)
C7, 
C8,00xx?0x: Country
C9,1 - Europe (EU) / 2 - USA (US) / 3 - Canada (CDN) / 4 - Great Britain (GB)
C10,5 - Japan (JP) / 6 - Saudi Arabia (SA) / 7 - Australia (AUS)
C11, 
C12,00xxx0?: Distance Impulse Number
C13,1 - 22188 / 2 - 22076 / 3 - 21960 / 4 - 21848
C14,5 - 22304 / 6 - 22420 / 7 - 22532
;
