;
; VAG-COM Labelfile
;
; Audi A3 (8P) / VW Caddy (2K) / VW Golf V (1K) / VW Touran (1T)
; Seat Altea/Toledo (5P) / Seat Leon (1P) / Skoda Octavia II (1Z)
;
; Component: J533 - Diagnostic Interface for Databus (#19)
;
; P/N: 1K0 907 530 ?
;
; includes measuring blocks and selective output tests
;
; created on 24/Jun/2004 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 11/Oct/2005
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Line Status
001,1,Wake-Up Line,,Display Range: Passive/Active
001,2,CAN-Comfort,Static,Display Range: [No Value]/CmfCAN Stat
001,3,CAN-Infotainment,Static,Display Range: [No Value]/InfCAN Stat
001,4,CAN-Powertrain,Static,Display Range: [No Value]/PwrCAN Stat
;
002,0,Transport Mode
002,1,Unlearn Counter
002,2,Transport Mode,,Display Range: Active/Deactivated
;
010,0,CAN-Gateway Status
010,1,CAN-Gateway,Status,0 = No Error\n1 = RAM-Error\n2 = ROM-Error\n3 = EEPROM-Error
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine Electronics,,Specification: Engine 1\nDisplay Range: Engine 1/Engine 0
125,2,Transmission,Electronics,Specification: Transm. 1\nDisplay Range: Transm. 1/Transm. 0
125,3,Brake Electronics,(J104),Specification: ABS 1\nDisplay Range: ABS 1/ABS 0
125,4,Instrument Cluster,(J285),Specification: Instruments 1\nDisplay Range: Instruments 1/Instruments 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nDisplay Range: Steer. ang. 1/Steer. ang. 0
126,2,Airbag System,(J255),Specification: Airbag 1\nDisplay Range: Airbag 1/Airbag 0
126,3,Steering Aid,(J500),Specification: Steering 1\nDisplay Range: Steering 1/Steering 0
126,4,Headlight Range,(J431),Specification: HdLtRange 1\nDisplay Range: HdLtRange 1/HdLtRange 0
;
127,0,CAN-Databus Powertrain (Communication)
127,1,All-Wheel-Drive,Electronics (J492),Specification: AWD 1\nDisplay Range: AWD 1/AWD 0
127,3,Immobilizer,,Specification: Immobilizer 1\nDisplay Range: Immobilizer 1/Immobilizer 0
;
130,0,CAN-Databus Comfort (Communication)
130,1,CAN-Comfort,Status,Specification: 2-Wire\nDisplay Range: 2-Wire/1-Wire
130,2,Central Electronics,(J519),Specification: E.Load.Crtl 1\nDisplay Range: E.Load.Crtl 1/E.Load.Crtl 0
130,3,Comfort System,(J393),Specification: Central 1\nDisplay Range: Central 1/Central 0s
130,4,Door Electronics,Driver (J386),Specification: Dr. Door 1\nDisplay Range: Dr. Door 1/Dr. Door 0
;
131,0,CAN-Databus Comfort (Communication)
131,1,Door Electronics,Passenger (J387),Specification: Pas. Door 1\nDisplay Range: Pas. Door 1/Pas. Door 0
131,2,Door Electronics,Rear Left (J388),Specification: RL Door 1\nDisplay Range: RL Door 1/RL Door 0
131,3,Door Electronics,Rear Right (J389),Specification: RR Door 1\nDisplay Range: RR Door 1/RR Door 0
131,4,Seat Memory,Driver (J521),Specification: Memory 1\nDisplay Range: Memory 1/Memory 0
;
132,0,CAN-Databus Comfort (Communication)
132,1,Tire Pressure,Monitoring (J502),Specification: Tire 1\nDisplay Range: Tire 1/Tire 0
132,2,Steering Wheel,Electronics (J527),Specification: St. Wheel 1\nDisplay Range: St. Wheel 1/St. Wheel 0
132,3,Heating/Air,Condition (J255),Specification: A/C 1\nDisplay Range: A/C 1/A/C 0
132,4,Parking Aid,Electronics (J446),Specification: Parking 1\nDisplay Range: Parking 1/Parking 0
;
133,0,CAN-Databus Comfort (Communication)
133,1,Auxiliary,Heating (J604),Specification: Aux. Htg 1\nDisplay Range: Aux. Htg 1/Aux. Htg 0
133,2,Convertible Top,,Specification: Conv. Top 1\nDisplay Range: Conv. Top 1/Conv. Top 0
133,3,Trailer,Electronics (J345),Specification: Trailer 1\nDisplay Range: Trailer 1/Trailer 0
133,4,Seat Memory,Passenger (J136),Specification: Memory Pax 1\nDisplay Range: Memory Pax 1/Memory Pax 0
;
134,0,CAN-Databus Comfort (Communication)
134,1,Special Vehicle,Electronics (J608),Specification: Special Veh 1\nDisplay Range: Special Veh 1/Special Veh 0
;
140,0,CAN-Databus Infotainment (Communication)
140,1,CAN-Infotainment,Status,Specification: 2-Wire\nDisplay Range: 2-Wire/1-Wire
140,2,Digital,Soundsystem,Specification: Dig.Soundp. 1\nDisplay Range: Dig.Soundp. 1/Dig.Soundp. 0
140,3,Telematic,,Specification: Telemat 1\nDisplay Range: Telemat 1/Telemat 0
140,4,Navigation,,Specification: Navigation 1\nDisplay Range: Navigation 1/Navigation 0
;
141,0,CAN-Databus Infotainment (Communication)
141,1,TV-Tuner,(J415),Specification: TV-Tuner 1\nDisplay Range: TV-Tuner 1/TV-Tuner 0
141,2,Digital Radio,,Specification: DigitRadio 1\nDisplay Range: DigitRadio 1/DigitRadio 0
141,3,Analog Radio,,Specification: Radio 1\nDisplay Range: Radio 1/Radio 0
141,4,Telephone,Electronics,Specification: Telephone 1\nDisplay Range: Telephone 1/Telephone 0
;
142,0,CAN-Databus Infotainment (Communication)
142,1,Auxiliary,Heater (J364),Specification: Aux. Heater 1\nDisplay Range: Aux. Heater 1/Aux. Heater 0
;
200,0,Voltage Supply
200,2,Voltage,(Terminal 30)
200,3,Voltage,(Terminal 15)
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1178,Powertrain Databus: Static
;
