;
; VAG-COM Measuring Block Labels Template file.
;   Updated 24. November 2005 to specify new features
;   in latest VAG-COM version 505.1
;
; Lines beginning with a semi-colon(;) are comments.
;
; Please always put the part number of the controller
; in the comment in a file.  For example:
; AG4 TRansmission, ECU p/n 01M-927-733-xx
;
; Also please your name and e-mail address in a comment 
; in the file:  This template was made by:
;
;    Eric Maurier, Chief of Carrot Cake Consumption
;    Andy Smith, Chief Assistant to the Assistant Chief 
;    Uwe Ross, Chief Cook and Bottle Washer
;    Sebastian Stange, Chief Fumbler on Duty
;    www.Ross-Tech.com  Support@Ross-Tech.com
;
;******************************************************************
; ***** New in VAG-COM version 401.2:  
; ****** Labels for Adapatation
;
; The format of the data-lines is for adaptation block labels is:
; nnn,n,xxxxxx,xxxxxxx
; 
; Ann is the Adaptation Channel Number (A0 - A255 with leading 0's optional)
; n is the Field Number 1 numeric digit, 
;   0-4 (conventional labels) or
;   5-25 (balloon data)
; xxxxxxx are the displayed text fields.
; fields must be separated by commas
; commas cannot be used within text fields
;
A1,0,This is the header for Adaptation channel 01
A1,1,Field 1,Field 2
A1,2,This is just,like in meas. blocks
A1,3,you only have,2 fields
A1,4,Max field leng., is 13-17 chars
;
;
; ***** New in VAG-COM version 402.3 
; ***** Ballon to help user figure out a value to put in an Adaptation Channel
;
A1,5,This is the header of the Adaptation Value Balloon which starts at 5.
A1,6,This is the first line of the ADP balloon text
A1,7,Your are allowed to up to 128 chars per line
A1,8,One can put up to 20 lines of info in the ballon in addition to the header.
A1,9,There can be one Adaptation Value Balloon per Adaptation channel.
A1,10,Only one "Field" per line.
A1,11,6th line of the Adaptation Value Balloon
A1,12,7th line of the Adaptation Value Balloon
A1,13,8th line of the Adaptation Value Balloon
A1,14,9th line of the Adaptation Value Balloon
A1,15,10th line of the Adaptation Value Balloon
A1,16,11th line of the Adaptation Value Balloon
A1,17,12th line of the Adaptation Value Balloon
A1,18,13th line of the Adaptation Value Balloon
A1,19,14th line of the Adaptation Value Balloon
A1,20,If you want a blank line in a balloon
A1,21, 
A1,22,You should have a blank line in the file
A1,23,as shown for Line 21.
A1,24,19th line of the Adaptation Value Balloon
A1,25,20th line of the Adaptation Value Balloon
;
;  Another Adaptation Channel
;
A2,0,This is the header for Adaptation channel 02
A2,1,Max field leng., is 13-17 chars
;
;  There are 255 possible Adaptation channels
;  Each can have complete labels and it's own Balloon
;  as shown for channel 01.
;
A255,0,This is the header for Adaptation channel 255
A255,1,Max field leng., is 13-17 chars
;
;
; **************************************************************
; ***** New in VAG-COM version 401.2:  
; ***** Coding *******
;
;  Ballon to help user figure out a value to put in Coding for the ECU
; 
:  The format of the data-lines for the Coding Balloon is
;  Cn,xxxxxx
; 
;  C stands for Coding
;  n is the line Number for the text in the Balloon 
;  xxxxx is the text displayed on that line
;
C0,This is the header for the Coding Balloon
C1,This is the first line of the coding balloon.
C2,There can be 20 lines in addition to the header
C3,Your are allowed to up to 128 chars per line
C4,One can put up to 20 lines of coding in the coding table
C5,There is only one coding ballon per control module
C6,6th line of the coding table
C7,7th line of the coding table
C8,8th line of the coding table
C9,9th line of the coding table
C10,10th line of the coding table
C11,11th line of the coding table
C12,12th line of the coding table
C13,13th line of the coding table
C14,14th line of the coding table
C15,15th line of the coding table
C16,16th line of the coding table
C17,17th line of the coding table
C18,18th line of the coding table
C19,19th line of the coding table
C20,20th line of the coding table
;
;  It's OK to have fewer than 20 lines in a balloon.  
;  Just delete some of the lines.
;
;
; ***************************************************************
; ***** New in VAG-COM version 401.2:  
; ***** Balloon Labels for Measuring Block Group 000
;       Since there is no room on the screen for these,
;       all except the Header pop up in Balloons when
;       the user clicks on a field.
;       It's probably a good idea to put
;       "Click on fields for details"  in the header
;
0,0,Header for the Group - displayed conventionally. Click on fields for details.
0,1,Heading,Condition1:Value1...Value2(meaning1-meaning2),Condition2:Value1...Value2(meaning1-meaning2)
0,2,Each Field can be up to 128 Characters,0,0
0,3,Heading shows parameter being measured,0,0
0,4,Condition1 describes a running condition ,Idle for example,0
0,5,Condition2 describes a different condition ,Full load for example,0
0,6,Value1 and Value2 are the raw displayed data,0,0
0,7,Meaning1 and Meaning2 are the real interpretations of the raw values,0,0
0,8,The popup window will expand in size to fit this text as long as you keep under 128 characters,0,0
0,9,0,0
0,10,0,0
;
; You can add any other bits of wisdom to these comment fields, 
; like how long EGR runs after engine start
;
;Real example for for one of the above fields
;0,7,Engine Coolant Temp.,Idle:80...35(80-110*C),Full load:80...35(80-110*C)
;
;
; **************************************************************
; ***** Now the traditional Measuring Block Labels
; ***** New in version 401.2:  A third field for each label
:       which is displayed in a ballon when the user clicks
;       on the data.
;
; The format of the data-lines is for measuring block labels isalways:
; nnn,n,xxxxxx,xxxxxxx
; 
; nnn is the Group Number (1-3 numeric digits, 0-255, leading 0's optional
; n is the Field Number (1 numeric digit, 0-4)
; xxxxxxx are the displayed text fields.
; fields must be separated by commas
; commas cannot be used within text fields
;
1,0,This is the Group Heading. 
1,1,Line 1,Line 2,Balloon Info
1,2,Just Line 1
1,3,,Just Line 2
1,4,,;nothing at all
;
; If you leave line 1 blank, VAG-COM will display the "default" label
; which is based on a "best guess" from the data-type being sent by
; control module
; line 3 will pop up when user clicks on the corresponding field.
;
2,0,Group Heading: One Line, Maximum 70 Characters!
2,1,123456789012345,ABCDEFGHIJKLM,This is the Third Field which is displayed in a balloon
2,2,Max field leng., is 13-17 chars,except for the third field that can be 80 chars long.
2,3,Depends on size, of characters
2,4,ABCDEFGHIJKLM,abcdefghijklmnopq
;
; VAG-COM won't die if you exceed the maxumum field lengths,
; but won't display it all.  Sometimes you'll have to use
; abbreviations. 
;
; A group heading is not required
;
3,1,Group 3,Field 1
3,2,This is way too long and won't be displayed properly,See?
;
4,0,This is an example of a Group Heading that is somewhat too long and won't be displayed properly.
;
5,0,Group 5
5,5,This won't display, the Field Number is Invalid
05,1,This is OK,Field 1
005,2,This is OK too,Field 2,Field 3
0005,3,This won't display, Group Number too long
5,04,This won't display, Field Number is too long
;
;
; There is no specific order in which you must put adaptations, coding and measuring 
; blocks. for instance you could theoretically put coding info in the middle of a
; measuring block label, all this being surrounded by adaptation labels. 
; VAG-Com bases itself on the first char of each line
; (digit,'A', or 'C' to decide which kind of info is contained in the line.
;
; The file should end with a comment line 
; (or at least a blank line after the last line of Data)
; 
; Any additional info you want to put in the file
; such as assorted notes should be in Comment lines
; which start with a semi-colon like these.
;
;
; **************************************************************
; ***** New in VAG-COM version 505.1 ******
; ***** Balloon labels for Login/Coding-II *******
;
;  Ballon to help user figure out a value for Login/Coding-II
; 
:  The format of the data-lines for the login Balloon is
;  Ln,xxxxxx
; 
;  L stands for Login
;  n is the line Number for the text in the Balloon 
;  xxxxx is the text displayed on that line
;
L0,This is the header for the Login Balloon
L1,This is the first line of the Login balloon.
L2,There can be 20 lines in addition to the header
L3,Your are allowed to up to 128 chars per line
L4,One can put up to 20 lines of logins in the login table
L5,There is only one login ballon per control module
L6,6th line of the login table
L7,7th line of the login table
L8,8th line of the login table
L9,9th line of the login table
L10,10th line of the login table
L11,11th line of the login table
L12,12th line of the login table
L13,13th line of the login table
L14,14th line of the login table
L15,15th line of the login table
L16,16th line of the login table
L17,17th line of the login table
L18,18th line of the login table
L19,19th line of the login table
L20,20th line of the login table
;
;  It's OK to have fewer than 20 lines in a balloon.  
;  Just delete some of the lines.
;
;
; **************************************************************
; ***** New in VAG-COM version 505.1 ******
; ***** Balloon labels for Security Access ******
;
;  Ballon to help user figure out a value for Security Access
; 
:  The format of the data-lines for the Security Access Balloon is
;  Sn,xxxxxx
; 
;  S stands for Security Access
;  n is the line Number for the text in the Balloon 
;  xxxxx is the text displayed on that line
;
S0,This is the header for the Security Access Balloon
S1,This is the first line of the Security Access balloon.
S2,There can be 20 lines in addition to the header
S3,Your are allowed to up to 128 chars per line
S4,One can put up to 20 lines of Security Access's in the Security Access table
S5,There is only one Security Access ballon per control module
S6,6th line of the Security Access table
S7,7th line of the Security Access table
S8,8th line of the Security Access table
S9,9th line of the Security Access table
S10,10th line of the Security Access table
S11,11th line of the Security Access table
S12,12th line of the Security Access table
S13,13th line of the Security Access table
S14,14th line of the Security Access table
S15,15th line of the Security Access table
S16,16th line of the Security Access table
S17,17th line of the Security Access table
S18,18th line of the Security Access table
S19,19th line of the Security Access table
S20,20th line of the Security Access table
;
;  It's OK to have fewer than 20 lines in a balloon.  
;  Just delete some of the lines.
;
;
;
; **************************************************************
; ***** New in VAG-COM version 505.1 ******
; ***** Labels for Selective Output Tests *******
;
;  Ballon to display possible Selective Output Tests
; 
:  The format of the data-lines for the Selective Output Tests is
;  Txxxx,yyyyy
; 
;  T stands for Selective Output Test
;  xxxx is the number of the actuator
;  yyyyy is the description for the actuator
;
;
T0111,Actuator #1
T0576,Actuator #2
T6558,Actuator #3
T2554,Actuator #4
;
;
