;
; VAG-COM Label File
;
; Audi A6 (4F)
;
; Component: J518 - Access/Start Authorization (#05)
;
; P/N: 4F0-910-852-???
;
; includes measuring blocks and coding
;
; created on 08/Sep/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 09/Sep/2005
;
; requires VAG-COM 403.2 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Terminal Status
001,1,Status,Terminal 15,Display Range: Term 15 On/Term 15 Off
001,3,Status,Terminal 75X,Display Range: ON/OFF
001,4,Status,Terminal 50,Display Range: Term 50 On/Term 50 Off
;
002,0,Entry and Start Authorisation Buttons
002,1,Start Auth. Button,(E408) ON,Display Range: ON/OFF
002,2,Start Auth. Button,(E408) START,Display Range: ON/OFF
002,3,Start Auth. Button,(E408) STOP,Display Range: ON/OFF
002,4,Door Touch,Sensors,0000xxx? = Front Left\n0000xx?x = Rear Left\n0000x?xx = Front Right\n0000?xxx = Rear Right
;
003,0,Ignition Switch (E415) I
003,1,Status,S-Contact,On Data Wire from Ignition Switch (E415)\nDisplay Range: ON/OFF
003,2,Status,Terminal 15,On Data Wire from Ignition Switch (E415)\nDisplay Range: ON/OFF
003,3,Status,Terminal 50,On Data Wire from Ignition Switch (E415)\nDisplay Range: ON/OFF
;
004,0,Ignition Switch (E415) II
004,1,Start Auth. Button,(E408) ON,On Data Wire from Ignition Switch (E415)\nDisplay Range: ON/OFF
004,2,Start Auth. Button,(E408) START,On Data Wire from Ignition Switch (E415)\nDisplay Range: ON/OFF
004,3,Start Auth. Button,(E408) STOP,On Data Wire from Ignition Switch (E415)\nDisplay Range: ON/OFF
004,4,Brake Light Switch,(F),On Data Wire from Ignition Switch (E415)\nDisplay Range: ON/OFF
;
005,0,Recovery Data
005,1,Current,Recovery Buffer
005,2,Recovery Data 0
005,3,Recovery Data 1
;
006,1,Serial Bus
006,2,Terminal 15R,Relay Circuit,Display Range: ON/OFF
006,3,Terminal 75X,Relay Circuit,Display Range: ON/OFF
006,4,Terminal 50R,Relay Circuit,Display Range: ON/OFF
;
007,0,Voltages
007,1,Supply Voltage
007,2,Output Voltage to,activate Term. 15
007,3,Output Voltage to,activate Term. 75X
007,4,Output Voltage to,activate Term. 50
;
008,0,Ignition Switch (E415)
008,2,Locked 1,,Display Range: Not Oper./Activated
008,3,Locked 2,,Display Range: Not Oper./Activated
008,4,Unlocked,,Display Range: Not Oper./Activated
;
009,1,Switch Motor 1,Relay 1 Term. 15,Display Range: Not Oper./Activated
009,2,Switch Motor 2,Relay 2 Term. 15,Display Range: Not Oper./Activated
009,3,K15/P Wire from,Ignition Sw. (E415),Display Range: ON/OFF
009,4,K15/S Wire from,Ignition Sw. (E415),Display Range: ON/OFF
;
010,1,Jump-Start,Counter
010,2,Unlock Counter
010,4,Wait-Time Preset
;
011,1,Remote Control,Key,0000xxxx = 0 = Sender-ID Unknown\nxxxx1xxx = Battery Low\nxxxxx1xx = Open\nxxxxxx?x = Rear\nxxxxxxx? = Close
011,2,Remote Control,Command,1xxxxxxx = Wrong Response\nx1xxxxxx = No Response\nxx1xxxxx = Carfinder Error\nxxx1xxxx = CAN Carfinder\nxxxx1xxx = CAN Panic\nxxxxx1xx = CAN Rear\nxxxxxx1x = CAN Close\nxxxxxxx1 = CAN Open
011,3,Reception Strength,of Remote Control
;
022,0,Keys I
022,4,Number of,matched Keys
;
023,0,Keys II
023,1,Authentication,,Specification: Yes = OK\nDisplay Range: Yes = OK / No = Not OK
023,2,Engine Control,Unit authorized,Specification: Yes = OK\nDisplay Range: Yes = OK / No = Not OK
023,3,Key-ID,authorized,Specification: Yes = OK\nDisplay Range: Yes = OK / No = Not OK
023,4,Immobilizer Status,,0 = End of Line (Original)\n1 = End of Line (New)\n6 = Immobilizer adapted
;
024,1,Login-Lock,(for Adaptation),in Minutes
024,2,Remaining,Free Starts,Terminal 15 ON Cycles
024,3,Drive Enable
024,4,End of Line,Timeout,
;
025,1,Warning Text,to Instr. Cluster,via CAN
025,2,Warning Message,to Instr. Cluster,via CAN
025,3,Advanced Key,Error Message
;
026,0,Advanced Key
026,4,Total Number of,Authentications
;
027,0,Door Touch Sensors
027,1,Lock-Out Time,Touch Sensors
027,2,False Triggering,Configuration
027,3,Current Counter,False Triggering
;
050,0,CAN-Messages from Central Electronics (J519)
050,1,Tailgate Lock
050,2,Locked,(internal)
050,3,Locked,(external)
050,4,Safed,(external)
;
051,0,CAN-Messages from Driver's Door Control Unit (J386)
051,1,Driver's Door,Opened,Display Range: ON/OFF
051,2,Driver's Door,Locked,Display Range: ON/OFF
051,3,Driver's Door,Safed,Display Range: ON/OFF
;
052,0,CAN-Messages from Passenger Door Control Unit (J387)
052,1,Passenger Door,Opened,Display Range: ON/OFF
052,2,Passenger Door,Locked,Display Range: ON/OFF
052,3,Passenger Door,Safed,Display Range: ON/OFF
;
053,0,CAN-Messages from Rear Left Door Control Unit (J388)
053,1,Door Rear Left,Opened,Display Range: ON/OFF
053,2,Door Rear Left,Locked,Display Range: ON/OFF
053,3,Door Rear Left,Safed,Display Range: ON/OFF
;
054,0,CAN-Messages from Rear Right Door Control Unit (J389)
054,1,Door Rear Right,Opened,Display Range: ON/OFF
054,2,Door Rear Right,Locked,Display Range: ON/OFF
054,3,Door Rear Right,Safed,Display Range: ON/OFF
;
055,0,CAN-Messages from Door Control Units
055,1,Driver's Door,Opening,Display Range: 0.0...100.0 %
055,2,Passenger Door,Opening,Display Range: 0.0...100.0 %
055,3,Door Rear Left,Opening,Display Range: 0.0...100.0 %
055,4,Door Rear Right,Opening,Display Range: 0.0...100.0 %
;
057,1,CAN-Diagnosis 1,Unlearn Counter
057,2,CAN-Diagnosis 1,Error-Bit Mileage
057,3,CAN-Diagnosis 1,Error-Bit Time
;
058,1,CAN-Diagnoses 1
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Identification Number (VIN) & Serial Number
;
082,0,Advanced Control Module Identification III
;
090,0,CAN-Gateway
090,1,Engine 1 Old,,Display Range: ON/OFF
090,2,Clutch Switch,,Display Range: ON/OFF
090,3,Brake Light Switch,,Display Range: ON/OFF
090,4,Brake Test Switch,,Display Range: ON/OFF
;
091,0,CAN-Gateway
091,2,Selector Lever,Position,Display Range: ON/OFF
091,3,Brake 1 Old,,Display Range: ON/OFF
091,4,Gearbox 1 Old,,Display Range: ON/OFF
;
128,0,Terminals
128,1,Status,Terminal S,Display Range: ON/OFF
128,3,Status,Terminal P,Display Range: ON/OFF
;
129,0,Gear Status
129,2,Gear P,,Display Range: ON/OFF
129,3,Gear PN,,Display Range: PN Inactive/PN Active
;
137,1,Locking Voltage,St. Column Lock
137,2,Minimum,Locking Voltage
;
177,0,Intelligent Load Management (ILM)
177,1,ILM Rear 1,Softtouch pressed,Display Range: ON/OFF
;
178,0,CAN-Messages from Driver's Door Control Unit (J386)
178,1,Driver's Door,Keyswitch Close,Display Range: ON/OFF
178,2,Driver's Door,Tag Pressed,Display Range: ON/OFF
178,3,Driver's Door,Lock Button,Display Range: ON/OFF
;
179,0,CAN-Messages from Passenger Door Control Unit (J387)
179,2,Passenger Door,Tag Pressed,Display Range: ON/OFF
179,3,Passenger Door,Lock Button,Display Range: ON/OFF
;
180,0,CAN-Messages from Rear Left Door Control Unit (J388)
180,2,Door Rear Left,Tag Pressed,Display Range: ON/OFF
180,3,Door Rear Left,Lock Button,Display Range: ON/OFF
;
181,0,CAN-Messages from Rear Right Door Control Unit (J389)
181,2,Door Rear Right,Tag Pressed,Display Range: ON/OFF
181,3,Door Rear Right,Lock Button,Display Range: ON/OFF
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,Access/Start Authorization (J518) Coding
C1,+001 - Standard (Coding Check)
C2,+002 - Automatic Transmission
C3,+004 - Advanced Key
C4,+008 - North American Region (USA/Canada)
C5,+016 - Right Hand Steering (RHD)
C6,+032 - Performance Reduction (Japan/South Korea)
C7,+064 - Special Vehicles
C8,+128 - Avant
;
