;
; VAG-COM label file
;
; Bentley Continental GT (3W) / VW Phaeton (3D)
;
; Component: J523 - Front Information Display Control Head (#07)
;
;       P/N: 3D0-035-007-? 
;       P/N: 3D0-035-008-? 
;
;       3D0 035 007 L 0223 Coding: 0500735 German W12 (Daniel)
;       3D0 035 008 M 0223 Coding: 0500305 NAR W12 (Brent)
;       3D0 035 008 Q 0223 Coding: 0500305 NAR W12 (Michael)
;       3D0 035 008 Q 0223 Coding: 0500305 NAR W12 (David)
;       3D0 035 007 P 0223 Coding: 0400525 Swiss V6 TDI MY 2003 (Alex)
;       3D0 035 007 L 0223 Coding: 0500735 German V6 Benzene (Tomasz)
;       3D0 035 008 Q 0223 Coding: 0500205 NAR V8 MY 2005 (Robert)
;       3D0 035 008 M 0188 Coding: 0500305 NAR V8 MY 2004 (Fred)
;       3D0 035 007 P 0223 Coding: 0500525 German W12 MY 2004 (DD AM 2662)
;
; NOTE: A CD ROM is available to flash upgrade the Phaeton controller to 0223 status, 
; VW part number 3D0 919 278, release 136 ZAB. This is suitable for -007 and -008 controllers
; (meaning, NAR and ROW), but do not use this CD ROM flash upgrade on older NAR controllers that have 
; 'MANUAL' and 'NAV SETUP' buttons or the button functions will be reassigned to 'INFO' and 'PHONE'.
;
;       P/N: 3W0-035-007-? (Bentley Continental GT - Rest of World)
;       P/N: 3W0-035-008-? (Bentley Continental GT - North America)
;
; includes coding & measuring blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 3D-07.LBL
; 3W-07.LBL
; 3D0-035-00x-07.LBL
;
; created by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; measuring block information added on 30/Mar/2005 by Sebastian Stange (sebastian@ross-tech.com)
; updated on 04/Sep/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 23/Sep/2005 by Michael Moore - Bentley information added above.
;                    23/Nov/2005 by Michael Moore - Note Added about CD Rom Flash Upgrade 
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
001,0,General Vehicle Information
001,1,Battery Voltage,at J523,Specification: 5.0...18.0 V
;
002,0,Signals
002,1,Status,Terminal 15
002,2,Status,S-Contact
002,4,Close-Request,S-Contact
;
003,0,Screen Illumination and Light Levels Sensed
003,1,Instrument Panel,Illumination,Terminal 58d (Specification: 0...100 %)
003,2,Photocell signal,from J523 Panel
;
004,0,HF Remote Supply (Active Antenna Test)
;
005,0,IF Remote Supply
;
006,0,Stereo Channel Testing - Entertainment Audio (CD, Radio, etc.)
006,1,Stereo channel 1,(left)
006,2,Stereo channel 1,(right)
;
007,0,Cable Testing - Telephone or Telematics Input
007,1,Stereo cable 2,(Tel +)
007,2,Stereo cable 2,(Tel -)
;
007,0,Cable Testing - Voice Guidance from Navigation System
008,1,Mono channel 3,(Nav +)
008,2,Mono channel 3,(Nav -)
; 
009,0,Function Test of Large Knob
009,1,Testing press-in,rotating adjuster
009,2,Testing left,rotating adjuster
009,3,Testing right,rotating adjuster
;
010,0,Function Test of Soft Keys either side of screen
010,1,Testing keypad,,Press buttons to see results
;
011,0,Rear Headphones - Driver Side Jacks
011,1,Headphone,output 1 (left)
011,2,Headphone,output 1 (right)
;
012,0,Rear Headphones - Passenger Side Jacks
012,1,Headphone,output 2 (left)
012,2,Headphone,output 2 (right)
;
013,0, CD Changer Connection and Malfunction Message Status
013,1,Connection,CD-Changer
013,2,Malfunction,CD-Changer
;
014,0,Fibre Optic Cable from Nav CD Reader to J523
014,2,Optical-Bus,Status
;
015,0,*Next Block Used is Block 80
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test numbers
;
082,0,FTC/Serial number
;
083,0,*Next Block Used is Block 141
;
141,0,Unknown
;
142,0,*Next Block Used is Block 240
;
240,0,Unknown
;
241,0,Unknown
;
242,0,Unknown
;
243,0,Unknown
;
244,0,Unknown
;
245,0,Unknown
;
246,0,Unknown
;
247,0,Unknown
;
248,0,Unknown
;
249,0,Unknown
;
250,0,Unknown
;
251,0,Unknown
;
252,0,Unknown
;
253,0,Unknown
;
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Phaeton (3D) - Front Information Display Control Head - CCH - (J523) Coding
C01,xxxxxx?
C02,+1 Navigation Installed (J401 module)
C03,+2 Voice Activation Installed (for cell phone only - not for OnStar)
C04,+4 CD Changer Installed (R41 module)
C05, 
C06,xxxxx?x
C07,+1 TV Tuner Installed
C08,+2 Telephone Installed (cell phone - not OnStar)
C09,+4 Test Mode 1 selected
C10, 
C11,xxxx?xx
C12,+1 Seat Memory Installed
C13,+2 Tire Pressure Monitoring System installed
C14,+4 Parking Heater (Webasto overnight heater) installed
C15, 
C16,x?xxxxx
C17,+0 None of the three configurations below
C18,+1 Rear Air Conditioning Control Head installed (typical)
C19,+2 Rear Central Control Head Installed (very rare)
C20,+4 Byte Coding Valid (always added to the total)
;
; REMARK: It is possible, though unlikely, that a 0 could be used in the first three positions from the right.
;         A 0 would be applicable if none of the three controllers indicated in the group were installed.
;
;
