;
; VAG-COM label file
;
; Audi A6 (4F)
;
; component: J520 - Central Electronics II (#4F)
;
; p/n: 4F0-910-280-???
;
; includes measuring blocks, adaptation, coding, security access and selective output tests
;
; created on 11/Jul/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 11/Jul/2005
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,1,Voltage Supply,(Terminal 30)
001,2,Outside,Temperature
;
002,0,Vehicle Data
002,1,Engine Speed
002,2,Vehicle Speed
002,3,Steering Angle,Sensor
;
003,0,Servotronic
003,2,Servotronic Valve,Adjusted Current
003,3,Servotronic Valve
;
004,0,Sunroof Comfort Function
004,1,Sunroof Comfort,Opening (CAN)
004,2,Sunroof Comfort,Closing (CAN)
004,3,Sunroof Comfort,Opening
004,4,Sunroof Comfort,Closing
;
005,0,Eneryg,
005,1,Terminal 15,Status
005,2,Terminal X,Status
005,3,Energy Manager,Dynamic Shut-Off
005,4,Energy Manager,Static Shut-Off
;
006,0,Inclination Sensor
006,1,X-Value,(absolute)
006,2,X-Value,(difference)
006,3,Y-Value,(absolute)
006,4,Y-Value,(difference)
;
007,0,Sunroof
007,1,Speed Signal,(Sunroof)
007,2,Enabling Sunroof
007,3,Enabling,Comfort Functions
;
008,0,Glove Compartment && Central Locking
008,1,Button for,Glove Compartm.
008,2,Central Locking,Open
008,3,Links of,Pre-Conditions
008,4,Glove Compartm.,Motor
;
020,0,Component Protection
020,1,Component,Protection
020,2,CAN Lock Counter
020,3,SA Lock Counter
;
140,0,CAN-Databus Communication (Comfort)
140,1,Battery Manager,,Specification: Batt.Mgmt 1
140,2,CAN-Gateway,,Specification: Gateway 1
140,3,Electrical,Ignition Lock,Specification: El.Ign.Lock 1
;
141,0,CAN-Databus Communication (Comfort)
141,1,Climate Control,,Specification: A/C 1
141,2,Databus,Status,Display Range: 1-Wire/2-Wire/No Communication 
141,3,Central,Electronics,Specification: Central 1
;
;
;---------------------------------------------------
;
; selective output test informations
;
;---------------------------------------------------
;
;
T2264,Servotronic Steering: Full Assistance
T2265,Servotronic Steering: No Assistance
T2661,Speed Signal (Sunroof)
T2662,Comfort Opening of Sunroof
T2663,Comfort Closing of Sunroof
T2752,Glovebox Unlocking Motor (V327)
;
;
;---------------------------------------------------
;
; security access informations
;
;---------------------------------------------------
;
;
S0,Central Electronics II (J520) Security Access
S1,12151 - General Adaptation "Enabling"
;
;
;---------------------------------------------------
;
; adaptation informations
;
;---------------------------------------------------
;
;
A001,0,Inclination Sensor Threshold
A001,5,Inclination Sensor Threshold
A001,6,Alarm threshold in X and Y direction.
;
A002,0,Glove Compartment Activation Time
A002,5,Glove Compartment Activation Time
A002,6,Time for which the glove compartment opening is
A002,7,permitted after the ignition is switched off.
;
A003,0,Anti-Play Protection Decrease Time
A003,5,Anti-Play Protection Decrease Time
A003,6,Time after the anti-play protection counter is decreased by 1.
;
A004,0,Anti-Play Protection Threshold
A004,5,Anti-Play Protection Threshold
A004,6,Threshold for anti-play protection counter from which an activation is prevented.
;
;
;---------------------------------------------------
;
; coding informations
;
;---------------------------------------------------
;
;
C0,Central Electronics II (J520) Coding
C1,000?xxx: Glove Compartment Unlock (1 - Standard)
C2, 
C3,000x?xx: Inclination Sensor
C4,0 - w/o Inclination Sensor (PR-7AA)
C5,1 - with Inclination Sensor (PR-7AL)
C6, 
C7,000xx?x: Sunroof
C8,0 - w/o Sunroof
C9,1 - with Sunroof
C10, 
C11,000xxx?: Engine
C12,3 - 6-Cylinder Diesel Engine (PR-T41)
C13,4 - Any other Engine
;
