;
; VAG-COM Labelfile
;
; VW Passat (3C)
;
; Component: J104 - Brake Electronics (#03)
;
; P/N: 3C0-614-095-???
;
; includes measuring blocks and coding
;
; created on 27/Oct/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 27/Oct/2005
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left (G47),Display Range: 0.0...255.0 km/h
001,2,Wheel Speed,Front Right (G45),Display Range: 0.0...255.0 km/h
001,3,Wheel Speed,Rear Left (G46),Display Range: 0.0...255.0 km/h
001,4,Wheel Speed,Rear Right (G44),Display Range: 0.0...255.0 km/h
;
003,1,Brake Light,Switch (F),Display Range: BrkSw. Off/BrkSw. On
003,2,Brake (K118),Warning Light,Display Range: Brake._WL off/Brake._WL on
003,3,ABS (K47),Warning Light,Display Range: ABS_warnl off/ABS_warnl on
003,4,ASR/ESP (K155),Warning Light,Display Range: ASR/ESP_WLoff/ASR/ESP_WLon
;
004,1,Steering Angle,Sensor (G85),Specification: ± 4.5 ° (left = positive / right = negative)
004,2,Transverse (G200),Acceleration,Specification: ± 1.5 m/s²
004,3,Rotation Rate,(G202),Specification: ± 2.5 °/s²
004,4,Longitudinal,Acc. Sensor (G251),Specification: ± 2.5 m/s²
;
005,1,Brake Pressure,Sensor,Specification: ± 7.0 bar
005,2,Steering Angle,Sensor Condition,Display Range: initialised/n. initialised/implausible
005,3,ASR Button,,Display Range: ON/OFF
005,4,Brake Light,Switch (F),Display Range: BrkSw. Off/BrkSw. On
;
006,0,Voltages
006,1,Voltage,(Terminal 15)
006,2,Voltage,(Terminal 30)
;
007,0,EDL Condition
007,1,EDL Shut-Off,(Temperature),?xxx = Front Left\nx?xx = Front Right\nxx?x = Rear Left\nxxx? = Rear Right
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine,,Specification: Engine 1\nDisplay Range: Engine 1/Engine 0
125,2,Transmission,,Display Range: Transm. 1/Transm. 0
125,3,Instrument Cluster,,Specification: Instruments 1\nDisplay Range: Instruments 1/Instruments 0
125,4,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nDisplay Range: Steer. ang. 1/Steer. ang. 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,CAN-Gateway,,Specification: Gateway 1\nDisplay Range: Gateway 1/Gateway 0
126,2,Airbag,,Specification: Airbag 1\nDisplay Range: Airbag 1/Airbag 0
126,4,Parking Brake,,Specification: Park Brake 1\nDisplay Range: Park Brake 1/Park Brake 0
;
127,0,CAN-Databus Powertrain (Communication)
127,2,Immobilizer,,Specification: Immobilizer 1\nDisplay Range: Immobilizer 1/Immobilizer 0
;
225,0,CAN-Databus Powertrain (Time-Out)
225,1,Engine
225,2,Transmission
225,3,Instrument Cluster
225,4,Steering Angle,Sensor (G85)
;
226,0,CAN-Databus Powertrain (Time-Out)
226,1,CAN-Gateway
226,2,Airbag
226,4,Parking Brake
;
227,0,CAN-Databus Powertrain (Time-Out)
227,2,Immobilizer
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104) Coding
+0016384 - Trailer Stabilisation
;
