;
; VAG-COM Labelfile
;
; Seat Altea/Toledo (5P) / Skoda Octavia (1Z) / VW Golf/Jetta (1K/5M)
;
; Component: J234 - Airbag (#15) - VW8/VW8R
;
; P/N: 1K0-909-605-???
;
; includes measuring blocks
;
; created on 25/Mar/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 10/Oct/2005
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,0,Ignitiers I (Front Airbags Stage 1 && Front Belt Tensioners)
001,1,Airbag (Stage 1),Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Airbag (Stage 1),Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Belt Tensioner,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Belt Tensioner,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
002,0,Ignitiers II (Rear Belt Tensioners)
002,1,Belt Tensioner,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Belt Tensioner,Rear Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,3,Belt Tensioner,Rear Center,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,0,Voltage && Seat. Occupation && Belt Inquiry I (Front)
003,1,Voltage Supply,,Specification: Correct
003,2,Occupied Seat,Sensor Pass. Side,Display Range: child/child seat/light adult/heavy adult/occupied/not occupied/not installed
003,3,Belt Inquiry,Front Driver Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Front Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry II (Rear)
004,1,Belt Inquiry,Rear Driver Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,3,Belt Inquiry,Rear Center,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
005,0,Igniters III (Side Airbags)
005,1,Side Airbag,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,2,Side Airbag,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,3,Side Airbag,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,4,Side Airbag,Rear Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
006,0,Seat Occupation (Rear)
006,1,Seat Occupation,Rear Driver Side,Display Range: Not Installed
006,2,Seat Occupation,Rear Pass. Side,Display Range: Not Installed
;
007,0,Igniters IV (Head Airbags)
007,1,Head-Level Airbag,Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
007,2,Head-Level Airbag,Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
010,0,Key Switch
010,1,Passenger,Airbag Status,Display Range: ON/OFF
010,2,Key Switch,Logic Contact 1,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
010,3,Key Switch,Logic Contact 2,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
011,0,Ingniters V (Front Airbags Stage 2 && Front Knee Airbags)
011,1,Airbag (Stage 2),Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,2,Airbag (Stage 2),Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,3,Knee Airbag,Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,4,Knee Airbag,Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Instrument Cluster,,Specification: Instruments 1
;
225,0,CAN-Databus Powertrain (TimeOut)
225,1,Instrument Cluster
;
