;
; VAG-COM label file
;
; VW Golf IV / Bora / Jetta IV (1J)
;
; component: J285 - instrument cluster (#17)
;
; p/n: 1J?-920-??6-???
;
; tested with: 1J0 920 906 J
;              1J0 920 826 A
;              1J5 920 846 A
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1J-17.LBL
; 1J0-919-xxx.LBL
; 1J0-920-xx0.LBL
; 1J0-920-xx6.LBL
; 1J0-920-xx7.LBL
;
; created on 10/Aug/2004 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 15/Apr/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; Measuring block informations
;
;---------------------------------------------------
;
;
001,0,Speed / Engine speed / Oil pressure / Time
001,1,Speed
001,2,Engine Speed
001,3,Oil pressure, 0.9 bar
001,4,Time
;
002,0,Distance / Fuel / Ambient temperature
002,1,Odometer
002,2,Fuel level (l)
002,3,Fuel Sender,Resistance
002,4,Ambient,temperature,MFD only
;
003,0,Coolant and Oil
003,1,Coolant Temp
003,2,Oil level,(Ok/n.Ok)
003,3,Oil,temperature
003,4,[N/A]
;
022,0,Immobilizer
022,1,Starting,permitted
022,2,Engine (ECM),responds
022,3,Key condition,OK
022,4,Number of,keys coded
;
023,0,Immobilizer
023,1,Variable code,authorized
023,2,Key status,(transponder)
023,3,Fixed code,authorized
023,4,Immobilizer,status,see labelfile
; 4 - new customer service - delivery condition (replacement part instrument cluster)
; 5 - customer service locked - adaptation data programmed in customer service
; 6 - immobilizer adapted - normal function condition
; 7 - key adaptation active - key adaptation via tester
;
024,0,Immobilizer - locking periods
024,1,Instrument,cluster
024,2,Engine control, module (ECM)
024,3,Emergency,release
024,4,Transponder,recognition
;
025,0,Immobilizer Communication
025,1,Immobilizer,Communication,1 = via CAN-Databus / 2 = via W-Line
025,2,[N/A]
025,3,[N/A]
025,4,[N/A]
;
050,0,Misc
050,1,Odometer
050,2,Engine Speed
050,3,Oil,temperature
050,4,Coolant,temperature
;
125,0,CAN-Databus communication (Powertrain)
125,1,Engine
125,2,Transmission
125,3,ABS
125,4,[N/A]
;
126,0,CAN-Databus communication (Powertrain)
126,1,Steering,sensor
126,2,Airbag
126,3,[N/A]
126,4,[N/A]
;
;
;---------------------------------------------------
;
; Adaptation informations
;
;---------------------------------------------------
;
;
A2,0,Service reminder
A2,5,Service reminder reset
A2,6,displayed values:
A2,7,0 - no service
A2,8,1 - service
A2,9, 
A2,10,reset:
A2,11,0 - Service reminder reset
;
A4,0,Language for error messages and navigation (MFD only)
A4,5,Language for error messages and navigation
A4,6,1 - German
A4,7,2 - English
A4,8,3 - French
A4,9,4 - Italian
A4,10,5 - Spanish
A4,11,6 - Portuguese
A4,12,8 - Czech
;
A9,0,Dinstance (in 10km)
A9,1,Distance
A9,2,in 10
A9,3,km
A9,5,Distance changing
A9,6,The distance can only be changed until
A9,7,the current value is not over 100km.
;
A21,0,Key count (Immobilizer)
A21,1,Old Key
A21,2,count
A21,3,[count]
;
A30,0,Fuel gauge adaption
A30,1,Current,value
A30,5,Fuel gauge adaption
A30,6,Basic value: 100
A30,7,Range: 120 - 136
A30,8,Unit: 1 Ohm
;
A35,0,Engine speed threshold
A35,5,Engine speed threshold adaption
A35,6,Basic value: 0
A35,7,Range: 0 - 1000
A35,8,Unit: 250 U/min
;
A40,0,Distance from inspection
A40,5,Distance from inspection
A40,6,Resolution: 1 = 100 km
A40,7, 
A40,8,NOTE: Adaptation channels 40-44 must be
A40,9,entered and stored in the following order:
A40,10,42 > 43 > 44 > 40 > 41
;
A41,0,Time from inspection
A41,5,Time from inspection
A41,6, 
A41,7,NOTE: Adaptation channels 40-44 must be
A41,8,entered and stored in the following order:
A41,9,42 > 43 > 44 > 40 > 41
;
A42,0,Minimum value mileage
A42,5,Minimum value mileage
A42,6,Resolution: 1 = 1000 km
A42,7, 
A42,8,NOTE: Adaptation channels 40-44 must be
A42,9,entered and stored in the following order:
A42,10,42 > 43 > 44 > 40 > 41
;
A43,0,Maximum value mileage
A43,5,Maximum value mileage
A43,6,Resolution: 1 = 1000 km
A43,7, 
A43,8,NOTE: Adaptation channels 40-44 must be
A43,9,entered and stored in the following order:
A43,10,42 > 43 > 44 > 40 > 41
;
A44,0,Maximum time interval
A44,5,Maximum time interval
A44,6, 
A44,7,NOTE: Adaptation channels 40-44 must be
A44,8,entered and stored in the following order:
A44,9,42 > 43 > 44 > 40 > 41
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,Instrument Cluster (J285) Coding
C1,??xxx - Additional equipment
C2,+00 - Without additional equipment
C3,+01 - Brake pad warning
C4,+02 - Seatbelt warning
C5,+04 - Washer fluid level warning
C6,+16 - Radio/Navigation
C7,xx?xx - Country version
C8,1 - Europe / 2 - USA / 3 - Canada/Mexico/Latin America
C9,4 - England / 5 - Japan / 6 - Saudi Arabia / 7 - Australia
C10,xxx?x - Service intervals
C11,0 - mini-service intervals without oil level/temperature sensor
C12,1 - flexible service intervals with oil level/temperature sensor
C13,2 - fixed service intervals with oil level/temperature sensor
C14,3 - without service intervals (USA/Canada)
C15,xxxx? - Distance impulse number (K-value)
C16,1 - 4358 (1,4l/55kW AHW/AKQ with manual transmission)
C17,2 - 3538 (all other engine  codes and/or automatic transmission)
C18,3 - 4146 (1,6l/74-77kW and 1,9l/50kW-SDI with manual transmission)
C19,4 - 3648 (unknown)
;
;
;---------------------------------------------------
;
; login information
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L00,13861 - General Adaptation "Enabling"
;
