;
; VAG-COM Measuring Block AGU Engine Label file.
; Component number 06A 906 018 CG
;
; Does not work with 06A 906 018 FA (2000 US 2.0L)
;
; Created by James Billings. Thanks to "Dave" the VW tech who
; got me the codes!
;
; Visit http://ds.dial.pipex.com/town/terrace/pp70/golf
;
1,0,Basic Functions - Spec figures at Idle
1,1,Idle speed,800-920 rpm
1,2,Engine load,0.5-1.5 m/s
1,3,Throttle ang,0-5 deg.
1,4,Ignition ang,6-12 BTDC
;
2,0,Basic Functions - Spec figures at Idle
2,1,Idle speed,800-920 rpm
2,2,Engine load,0.5-1.5 m/s
2,3,Inj. period,1.00-3.00 m/s
2,4,Air mass in,1.8-4 g/s
;
3,0,Basic Functions - - Spec figures at Idle
3,1,Idle speed,800-920 rpm
3,2,Supply volts,10-14.5V
3,3,Coolant temp,80-105 d/C
3,4,Intake temp,-45-108.5 d/C
;
4,0,Idle Stabilisation - Spec figures at Idle
4,1,Throttle ang.,0-5 deg.
4,2,Idle mass,-1.7-1.7 A/T
4,3,Idle mass,0 if man/t
4,4,Op. mode,
;
5,0,Idle Stabilisation - Spec figures at Idle
5,1,Idle speed,800-920 rpm
5,2,Spec. idle,860 rpm
5,3,Idle reg,-10-10%
5,4,Air mass in,1.8-4 g/s
;
6,0,Idle Stabilisation - Spec figures at Idle
6,1,Idle speed,800-920 rpm
6,2,Idle reg,-10-10%
6,3,Lambda reg,-10-10%
6,4,Ign angle,6-12 BTDC
;
7,0,Lambda learned values
7,1,Lambda reg,-10-10%
7,2,Probe volts,0-1V
7,3,Valve duty,angle 0-99%
7,4,Correction,0.3-1.25
;
8,0,Lambda learned values
8,1,Inj. period,1-3 m/s
8,2,Idle learned,-10-10%
8,3,Learned,-8-8%
8,4,Vent mode
;
9,0,Lambda learned values
9,1,Idle speed,800-920 rpm
9,2,Lambda reg,-10-10%
9,3,Probe volts,0-1V
9,4,Idle learned,-10-10%
;
10,0,Fuel tank breather
10,1,Valve duty,angle 0-99%
10,2,Correction,0.3-1.25
10,3,Filter state,-3-32
10,4,Purge rate,0-0.3
;
11,0,Fuel Consumption
11,1,Idle speed,800-920 rpm
11,2,Engine load,0.5-1.5 m/s
11,3,Road speed,km/h
11,4,Consumption,l/h
;
12,0,Fuel Consumption [Not verified in manual]
12,1,Engine rpm,0-6800 rpm 
12,2,Voltage,V
12,3,Consumption,l/h 
12,4,Ign degrees,deg
;
13,0,Knock regulation [Not verified in manual]
;
14,0,Knock control
14,1,Engine speed,0-6800 rpm
14,2,Engine load,0-10 m/s
14,3,Cyl 1 retard,0-9 degCA
14,4,Cyl 2 retard,0-9 degCA
;
15,0,Knock control
15,1,Engine speed,0-6800 rpm
15,2,Engine load,0-10 m/s
15,3,Cyl 3 retard,0-9 degCA
15,4,Cyl 4 retard,0-9 degCA
;
16,0,Knock control
16,1,Sens 1 volts,0.4-1.4V
16,2,Sens 2 volts,0.4-1.4V
16,3,Sens 3 volts,0.4-1.4V
16,4,Sens 4 volts,0.4-1.4V
;
17,0,[Not listed in manual - Using default labels]
;
18,0,Altitude adaptation
18,1,Idle speed,800-920 rpm
18,2,Engine load,0.5-1.5 m/s
18,3,Throttle,valve angle
18,4,Alt. correc.,-50-10%
;
19,0,Additional signals
19,1,Engine speed,0-6800 rpm
19,2,Engine load,0-10 m/s
19,3,Additional,signals
19,4,Ign. timing,20Atdc-42Btdc
;
20,0,Operating Modes
20,1,Idle speed,800-920 rpm
20,2,Auto trans,Neutral/ON
20,3,Air cond.,AC High/Low
20,4,A/C Comp.,Compr ON/OFF
;
21,0,Lambda Control
21,1,Idle speed,800-920 rpm
21,2,Engine load,0.5-1.5 m/s
21,3,Coolant temp,-40-125 deg/C
21,4,Lambda mode,
;
23,0,Throttle valve adaptation
23,1,Learning req.,100000
23,2,Min stop,72-95%
23,3,Emerg. stop,60-91%
23,4,Max stop,18-54%
;
24,0,Knock control
24,1,Engine speed,0-6800 rpm
24,2,Engine load,0-10 m/s
24,3,Ign timing,20Atdc-42Btdc
24,4,Sum of ret.,angle 0-36
;
25,0,Charge Pressure control
25,1,Spec. load,3-8 m/s
25,2,Load correc.,0-8 m/s
25,3,Actual load,0.5-8 m/s
25,4,Valve cycle,0-99%
;
26,0,[Not listed in manual - Using default labels]
;
27,0,[Not listed in manual - Using default labels]
;
66,0,Cruise control
66,1,Road speed,km/h
66,2,Switch pos.,xxxx
66,3,Spec. speed
66,4,CCS switch,position
;
95,0,Basic functions
95,1,Idle speed,800-920 rpm
95,2,Engine load,0.5-1.5 m/s
95,3,Ign timing,
95,4,Coolant temp.,80-105 degC
;
97,0,[Not listed in manual - Using default labels]
;
98,0,Throttle Valve Matching/Calibration/Adaptation
98,1,Valve voltage,0-5V
98,2,Sender voltage,0-5V
98,3,Opr. mode,
98,4,Adapt mode,RUN/OK/ERROR
;
99,0,Lambda regulation
99,1,Engine speed,0-6800 rpm
99,2,Coolant temp,-40-125 deg/C
99,3,Lambda reg.,-10-10%
99,4,Lambda mode
;
;End of File