;
; VAG-COM label file 3D0-937-049.lbl
;
; VW Phaeton (3D) - up to and including model year 2005 (fully tested with 2004 W12 Phaeton)
; VW Bentley Continental GT - up to and including model year 2005 (not tested with this vehicle)
;
; component: Central Electronics -J519-  (#09)
;
; p/n: 3D0 937 049 E
;      3D0 937 049 G Component: STG.Bordnetz 5001 Coding: 0000003 (Canada 2004, 2005 W12 & V8 Phaeton)
;      3D0 937 049 G Component: STG.Bordnetz 5001 Coding: 0000003 (Germany 2004 W12 Phaeton)
;      3D0 937 049 H Component: STG.Bordnetz 5101 Coding: 0000105 (Canada 2004 Bentley Continental GT)
;      NOTE: The Touareg is very different, therefore this file is not suitable for the Touareg.
;            Perhaps 50% of the MVB's are the same, but coding is totally different for the Touareg.
;            Use the existing file 7L6-937-049.lbl for the Touareg.
;
; includes measured value blocks, coding, and some (incomplete) information about adaptation.
;
; by Sebastian Stange (sebastian@ross-tech.com)
; modified by Michael Moore (moore99@rogers.com)
;
; last modified: 11/05/2004 (Sebastian)
; last modified: 22/July/2005 (Michael)
; - adaptation channel 1 information added, MVB 17/2 and 3/3 added, note 2 added to coding.
; checked against CSV and PLB October 11 2005, Michael - all blocks documented.
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
001,0,Light SWITCH status (not the status of the lights themselves)
001,1,Parking light,switch,Specified value: off/on
001,2,Low beam,light switch,Specified value: off/on
001,3,Automatic,headlight activation,Specified value: off/on
001,4,Switch for,emergency flasher,Specified value: active/inactive ('active' will only appear when switch is held in depressed position)
;
002,0,Light SWITCH status (not the status of the lights themselves)
002,1,Rear fog light,or VALET button,Specified value: off = not pressed at the moment/on = pressed in/not installed
002,2,Front Fog light,,off = not pressed at the moment/on = pressed in/not installed
002,3,Back-up light,switch,Specified value: off/on
002,4,Not Used
;
003,0,Instrument panel illumination dimming
003,1,Increase,button,Specified value: active/inactive
003,2,Decrease,button,Specified value: active/inactive
003,3,Valet Lockout,button,Specified value: active/inactive
003,4,Not Used
;
004,0,Status of Hood (Bonnet) - open or closed
004,1,Not Used
004,2,Not Used
004,3,Engine hood,switch,Specified value: closed/open
004,4,Not Used
;
005,0,Mirror adjustment switch
005,1,Y-Axis,(minus),Specified value: active/inactive
005,2,Y-Axis,(plus),Specified value: active/inactive
005,3,X-Axis,(minus),Specified value: active/inactive
005,4,X-Axis,(plus),Specified value: active/inactive
;
006,0,Mirror control switch position
006,1,Left mirror,selection,Specified value: active/inactive
006,2,Right mirror,selection,Specified value: active/inactive
006,3,Folding in,function,Specified value: active/inactive
006,4,Mirror Heating,switch,Specified value: active/inactive
;
007,0,Voltages present on the car
007,1,Terminal 15,(Ignition),Specified value: Term. 15 on/Term. 15 off
007,2,Terminal X,(consumers),Specified value: Term. X on/Term. X off
007,3,Power Supply,battery,Specified value: 6...15 V
007,4,Starter,battery,Specified value: 6...15 V
;
008,0,Status of the actual lamps themselves (not the switches for these lamps)
008,1,Left low,beam headlight,Specified value: off/on
008,2,Right low,beam headlight,Specified value: off/on
008,3,Left high beam,,Specified value: off/on
008,4,Right high beam,,Specified value: off/on
;
009,0,Status of the actual lamps themselves (not the switches for these lamps)
009,1,Left,parking light,Specified value: off/on
009,2,Right,parking light,Specified value: off/on
009,3,Not Used
009,4,Not Used
;
010,0,Status of the actual lamps themselves (not the switches for these lamps)
010,1,Turn signal,lights left,Specified value: off/on
010,2,Turn signal,lights right,Specified value: off/on
010,3,Front Fog lights,left/right,Specified value: off/on
010,4,Not Used
;
011,0,Status of the switch position for turn signals or single side parking lights
011,1,Left turn,signal lever,Specified value: off/on
011,2,Right turn,signal lever,Specified value: off/on
011,3,Left parking,light switch,Specified value: off/on
011,4,Right parking,light switch,Specified value: off/on
;
012,0,Status of switch positions
012,1,Headlamp flash,to pass switch,Specified value: off/on
012,2,High beam switch,,Specified value: off/on
012,3,Switch for horn,,Specified value: off/on
012,4,Window washing,switch,Specified value: off/on
;
013,0,Intervention Load Management status
013,1,Intervention,Load management,Specified value: active/inactive
013,2,highest shut-off,priority reached,Specified value: 0 to 14. May be reset to zero via adaptation channel 01.
013,3,Not Used
013,4,Not Used
;
014,0,Heated mirrors status
014,1,Driver door,heated mirror,Specified value: off/on
014,2,Passenger door,heated mirror,Specified value: off/on
014,3,Not Used
014,4,Not Used
;
015,0,Rotary traps (detents in the door latches that indicate the door is closed properly)
015,1,Driver door,rotary trap,Specified value: open/closed
015,2,Passenger door,rotary trap,Specified value: open/closed
015,3,Rotary trap,Left Rear door,Specified value: open/closed
015,4,Rotary trap,Right Rear door,Specified value: open/closed
;
016,0,Footwell light dimming levels, other vehicle conditions
016,1,Footwell light,dimming level,Specified value: 0...100 %
016,2,Terminal DFM,,Specified value: 0...255 %
016,3,Outside air,temperature,Specified value: 0...255 °
016,4,Gear Selector,lever position,Specified value: 0...15
;
017,0,CAN bus signal being sent
017,1,Not Used
017,2,CAN signal,lights on
017,3,Not Used
017,4,Not Used
;
018,0,*Next MVB is 080, there are no others past that.
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,*End of MVB in this controller.
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Phaeton Central Electronics (J519) Coding
C01, 
C02,xxxx? - Choice of Daytime Running Light (DRL) Function
C03,Choose one number only from the list below
C04, 
C05,1 - Scandinavia - all lights illuminated for DRL + rear fog light installed. No DRL icon.
C06,2 - North America - headlights only illuminated for DRL + no rear fog light installed. With DRL icon.
C07,3 - No DRL of any kind (DRL feature disabled) + rear fog light installed.
C08, 
C09,NOTE 1: Interior light functions controlled by 'soft-buttons' such as dome lights illuminating 
C10,when doors are opened may need to be re-set after the DRL function has been changed. 
C11,Re-cycle the push-button(s) on the roof to the setting desired after recoding is done.
C12, 
C13,NOTE 2: Changing DRL selection away from 'North America' will cause loss of the valet
C14,lockout button function - this button will now be assigned to operate the rear fog light,
C15,even though the rear foglight is not functional on NAR Phaetons.
;
;
;
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
A01,0,Load Intervention Management History
A01,6,The number shown is the highest level of load intervention reached since this
A01,7,number was last reset. The range is from zero to fourteen.
A01,8,
A01,9,You may reset this number to zero - for troubleshooting and tracking purposes - 
A01,10,by entering a value of zero in this channel and saving it.
;
;
;
;No adaptation channels available 02 to 80 inclusive, did not check past 80.