;
; VAG-COM Label File
;
; Audi A3 (8P)
;
; component: J393 - Central Module Comfort System (#46)
;
; P/N: 8P0-959-433-???
;
; includes measuring blocks and adaptation
;
; created on 13/Sep/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 13/Sep/2005
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Rotary Switches
001,1,Driver Door,Rotary Switch,Display Range: Door open/Door closed
001,2,Passenger Door,Rotary Switch,Display Range: Door open/Door closed
001,3,Rear Left Door,Rotary Switch,Display Range: Door open/Door closed
001,4,Rear Right Door,Rotary Switch,Display Range: Door open/Door closed
;
002,0,Central Locking Return Messages
002,1,Driver Door,,Display Range: implausible/locked/unlocked/safe
002,2,Passenger Door,,Display Range: implausible/locked/unlocked/safe
002,3,Rear Left Door,,Display Range: implausible/locked/unlocked/safe/not installed
002,4,Rear Right Door,,Display Range: implausible/locked/unlocked/safe/not installed
;
003,1,Driver Door,Key Switch,Display Range: implausible/open/closed/not operated
003,2,Passenger Door,Key Switch,Display Range: implausible/open/closed/not operated
003,3,Lock/Unlock,Button Driver Door,Display Range: limplausible/ocking/unlocking/not operated
003,4,Function LED,Lock,Display Range: implausible/locking/unlocking/not operated
;
004,0,Rear Lid
004,1,Rear Key Switch,,Display Range: open/closed/not operated
004,2,Rear Lid,Outside Button,Display Range: operated/not operated
004,3,Rear Lid,Main Latch,Display Range: open/closed
004,4,Rear Lid,Pre-Latch,Display Range: open/closed
;
005,0,Power Supply
005,1,Power Supply,(Terminal 30),Specification: 9...14 V
005,2,Voltage Supply
005,3,Terminal 15,,Display Range: Terminal 15 on/Terminal 15 off
005,4,S-Contact,,Display Range: operated/not operated
;
006,1,Driving Speed,,Specification: 0 km/h
006,2,Crash Signal,,Display Range: Yes/No
006,3,Request,Tank Lid Open,Display Range: Yes/No
006,4,Databus,Condition,Display Range: Single wire/Dual wire
;
007,1,Enabling SAD,,Display Range: Yes/No
007,2,Sunroof Control,,Display Range: open/closed/not operated
007,3,Comfort Function,Request,Display Range: not installed
;
008,1,Request,Terminal 58d,Display Range: 0...100 %
008,2,Signal,Terminal 58s,Display Range: 0...100 %
008,3,TIG,Illumination Request,Display Range: 0...100 %
008,4,TIG,Illumination Signal,Display Range: 0...100 %
;
009,0,Central Locking
009,1,Thermal,Protection,Display Range: Yes/No
009,2,Signal Doors,not closed,Display Range: open/closed
009,3,Request Left,Rear Exit Light,Display Range: off/on/not installed
009,4,Request Right,Rear Exit Light,Display Range: off/on/not installed
;
010,0,Remote Control
010,1,Remote Control,Key Number,Display Range: 0...4 (0 = no key recognized)
010,2,Remote Control,Buttons
010,3,Remote Buttons,encoded,Display Range: yes/no/not installed
;
011,0,Remote Control
011,1,Fixed Code,,Display Range: OK/not OK/no measuring value
011,2,Code in,Catch Area,Display Range: OK/not OK/no measuring value
011,3,Algorithm,,Display Range: OK/not OK/no measuring value
;
012,1,Immobilizer,Key Recognition,Display Range: Yes/No
012,2,Interior Button,Rear Lid Remote,Display Range: operated/not operated
012,3,Enabling Rear,Outside Button,Display Range: Yes/No
012,4,Hood Contact,,Display Range: open/closed
;
013,1,Telematics,,Display Range: open/closed/not operated/not installed
;
014,0,Interior monitoring
014,1,Sensor Status,,Display Range: activated/inactive/not installed
014,2,Alarm recognized,,Display Range: yes/no/not installed
014,3,Button,,Display Range: operated/not operated/not installed
014,4,Interior monitoring,LED,Display Range: off/on/not installed
;
015,0,Tilt Sensor
015,1,Sensor Status,,Display Range: activated/inactive/not installed
015,2,Alarm recognized,,Display Range: yes/no/not installed
015,3,Sensor Button,,Display Range: operated/not operated/not installed
015,4,Interior monitoring,LED,Display Range: off/on/not installed
;
016,0,Sounder
016,1,Sounder,Status,Display Range: activated/inactive/not installed
016,2,Sounder,Alarm recognized,Display Range: yes/no/not installed
016,3,Sounder,Output active,Display Range: operated/not operated/not installed
;
017,0,Tilt Sensor
017,1,X-Reference,Angle,Specification: -25.2...+25.4 ° | Display Range: no measuring value/not installed
017,2,Current,X-Delta Angle,Specification: -12.6...+12.7 ° | Display Range: no measuring value/not installed
017,3,Y-Reference,Angle,Specification: -25.2...+25.4 ° | Display Range: no measuring value/not installed
017,4,Current,Y-Delta Angle,Specification: -12.6...+12.7 ° | Display Range: no measuring value/not installed
;
018,0,Sounder (Alarm Trigger)
; 0 - no alarm trigger
; 1 - alarm trigger via comfort control module
; 2 - Communication open circuit, Ground (GND) open circuit
; 3 - Open circuit of supply voltage
018,1,1st Alarm Trigger
018,2,2nd Alarm Trigger
018,3,3rd Alarm Trigger
018,4,Alarm Trigger,Counter
;
019,0,Interior Monitoring (Alarm Trigger)
019,1,1st Alarm Trigger
019,2,2nd Alarm Trigger
019,3,3rd Alarm Trigger
019,4,4th Alarm Trigger
;
020,0,Alarm Sources
020,1,1st Alarm Source
020,2,2nd Alarm Source
020,3,3rd Alarm Source
020,4,4th Alarm Source
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A000,0,Remote Control - Erasing
A000,5,Remote Control - Erasing
A000,6,0 - Erase all Keys
;
A001,0,Remote Control - Key Matching
A001,5,Remote Control - Key Matching
A01,6,Enter the number of keys that should be adapted. Save.
A01,7, 
A01,8,Now press button 1 or 2 on every remote that
A01,9,should be adapted for at least 1 second.
A01,10, 
A01,11,Note #1: All keys must be adapted in one procedure.
A01,12,Note #2: Adaptation of all keys must not exceed 15 seconds.
;
A03,0,Door Locking
A03,5,Door Locking
A03,6,0 - locking of all doors
A03,7,1 - selective door locking
;
A04,0,Auto-Lock
A04,5,Auto-Lock
A04,6,The doors will lock automatically when the vehicle
A04,7,reaches a speed of 15 km/h or 10 mph.
A04,8, 
A04,9,Display Range; 0 = off / 1 = on
A04,10, 
A04,11,Note: This option has to be used in combination
A04,12,with "Auto-Unlock" (Channel 003).
;
A05,0,Auto-Unlock
A05,5,Auto-Unlock
A05,6,The doors will unlock automatically when the key
A05,7,is removed from the ignition switch.
A05,8, 
A05,9,Display Range: 0 = off / 1 = on
A05,10, 
A05,11,Note: This option has to be used in combination
A05,12,with "Auto-Lock" (Channel 002).
;
A007,0,Unlock Message - Remote
A007,5,Unlock Message - Remote
A007,6,Return message when unlocking via remote control.
A007,7, 
A007,8,0 - No Return Message
A007,9,1 - Beep
A007,10,2 - Blink
A007,11,3 - Beep & Blink
;
A008,0,Unlock Message - Key
A008,5,Unlock Message - Key
A008,6,Return message when unlocking via key switch.
A008,7, 
A008,8,0 - No Return Message
A008,9,1 - Beep
A008,10,2 - Blink
A008,11,3 - Beep & Blink
;
A010,0,Lock Message - Remote
A010,5,Lock Message - Remote
A010,6,Return message when locking via remote control.
A010,7, 
A010,8,0 - No Return Message
A010,9,1 - Beep
A010,10,2 - Blink
A010,11,3 - Beep & Blink
;
A011,0,Lock Message - Key
A011,5,Lock Message - Key
A011,6,Return message when locking via key switch.
A011,7, 
A011,8,0 - No Return Message
A011,9,1 - Beep
A011,10,2 - Blink
A011,11,3 - Beep & Blink
;
A012,0,Activation Message - Anti-Theft
A012,5,Activation Message - Anti-Theft
A012,6,Return message when anti theft warning system is active.
A012,7, 
A012,8,0 - No Return Message
A012,9,1 - Beep
A012,10,2 - Blink
A012,11,3 - Beep & Blink
;
A13,0,Alarm Horn Adjustment
A13,5,Alarm Horn Adjustment
A13,6,Country setting for alarm horn. This changes length
A13,7,and volume of the alarm horn sounding.
A13,8, 
A13,9,0 - Great Britain (Frequency Modulated - 10 Tamper Alarms)
A13,10,1 - Great Britain (Frequency Modulated - 1 Tamper Alarm)
A13,11,2 - Rest of World (Discontinuous - 10 Tamper Alarms)
A13,12,3 - Rest of World (Discontinuous - 1 Tamper Alarm)
;
A14,0,Tilt Sensor Sensitivity
A14,5,Tilt Sensor Sensitivity
A14,6,Display Range: 100 = 50 % / 200 = 100 %
;
A15,0,Interior Monitoring Sensitivity
A15,5,Interior Monitoring Sensitivity
;
A16,0,Battery Monitoring - Sounder
A16,5,Battery Monitoring - Sounder
A16,6,Display Range: 0 = off / 5 = on
;
A17,0,Comfort Function
A17,5,Comfort Function
A17,6,Display Range: 0 = off / 1 = on
A17,7, 
A17,8,NOTE: See long coding for more details/options.
;
A18,0,Anti-Theft Delay
A18,5,Anti-Theft Delay
A18,6,Deactivation of the anti theft warning delay
A18,7,when opening drivers door before the anti theft
A18,8,warning system is beeing activated.
A18,9, 
A18,10,Display Range: 0 = off / 1 = on
;
