;
; VAG-COM label file 3D0-909-135
;
; Bentley Continental GT (3W) / VW Phaeton (3D) / VW Touareg (7L)
;
; Access and Start Control Module (Kessy) -J518-  (address #05)
;
;      p/n: 3D0 909 135 M - Component: Kessy 6400  Coding: 0133356 
;                           (2004 Phaeton  W12 Canada)
;      p/n  3D0 909 135 K - Component: Kessy 6400  Coding: 0000232, or 0131304, or others 
;                           (Touareg - coding will vary with engine/transmission combination)
;      p/n  3D0 909 135 L - Component: Kessy 6400  Coding: 147693 
;                           (Bentley Continental GT - Europe)
;      p/n  3D0 909 135 R - Component: 0R Kessy 6610  Coding: 0139501 
;                           (Bentley Continental GT - Canada)
;      p/n  3D0 909 135 R - Component: Kessy 6610  Coding: 0137452 
;                           (2005 Phaeton V8 - Canada)
;
; by Michael Moore (Moore@ross-tech.com), 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; last modified: 27/March/2005 (Michael)
; last modified: 25/September/2005 (Michael) - Bentley information added above.
; last modified: 11/October/2005 (Michael) -checked against CSV and PLB, all blocks documented.
; last modified: 16/October/2005 (Michael) MVB text enhanced and simplified, additional hover balloons added to MVBs.
;
; includes measured value blocks and coding for Phaeton and Bentley.
;
; ready for VAG-COM 500.9 and above (500.9 supports block labels beginning with asterisks)
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
001,0,General Vehicle Electrical Status Information
001,1,Term 15 (Ignition),status,Possible Display: - Terminal 15 ON - Terminal 15 OFF
001,2,Terminal 15SV,status,Possible display: On or Off
001,3,Terminal 75X,status,Possible display: On or Off
001,4,Term 50 (Starter),status,Possible display: On or Off
;
002,0,Engine Start-Stop Button Status
002,1,Start 1,switch status,Possible display: On or Off
002,2,Start 2,switch status,Possible display: On or Off
002,3,Stop 1,switch status,Possible display: On or Off
002,4,Stop 2,switch status,Possible display: On or Off
;
003,0,NOTE: Parking Lock (block 2) is not used on the Phaeton.
003,1,El Ign Lock Supply,Diagnosis,Possible display: On or Off
003,2,Parking Lock,status,,Possible display: On or Off
003,3,Emergency,start mode,Possible display: On or Off
;
004,0,Door Handle Touch Sensor Recognition (for Phaetons with keyless access)
004,1,G415,Driver Door,Possible display: Operated or Not Operated
004,2,G416,Passenger Door,Possible display: Operated or Not Operated
004,3,G417,Left Rear Door,Possible display: Operated or Not Operated
004,4,G418,Right Rear Door,Possible display: Operated or Not Operated
;
005,0,Elapsed Time Counter
;
006,0,Vehicle Key Status -  Click on all 4 block of the values to read decoding information.
006,1,Key 1,bit display,Bit 7 = Battery strength. Bit 6 = Key adapted. Bit 5 = Key blocked. 
006,2,Key 2,bit display,Bit 4 = not synchronized. Bit 3 = Trunk button pressed. Bit 2 = Panic button pressed. 
006,3,Key 3,bit display,Bit 1 = Unlock Button pressed. Bit 0 = Lock button pressed.
006,4,Key 4,bit display,Bits read like this - 76543210.
;
007,0,Radio Frequency Information
007,1,Radio amp, phantom powering,Possible display: On or Off
007,2,Radio range,reduction,Possible display: On or Off
;
008,0,Play protection counter capacitive sensor for Door Handle Touch Sensors (G415 = Driver, G416 = Front Passenger)
008,1,G415 rest period,for shut-off,
008,2,G416 rest period,for shut-off,
008,3,Cycle counter,driver door,
008,4,Cycle counter,both pax side doors
;
009,0,Play protection counter capacitive sensor for Door Handle Touch Sensors (see block 004 for locations)
009,1,G415 cycle,protection status,Possible display: On or Off
009,2,G416 cycle,protection status,Possible display: On or Off
009,3,G417 cycle,protection status,Possible display: On or Off
009,4,G418 cycle,protection status,Possible display: On or Off
;
010,0,Unknown value
;Could this report on keys in range? See blocks below from file 1J0-959-799-aj (credit to Mike Sauve) for possible ideas.
;13,0,remotes
;13,1,Permanent code
;13,2,Code in range
;13,3,Algorithm
10,4,Key number,(press remote),This may identify the key
;
011,0,*Next documented blocks are group 22
;
022,0,Security Status
022,1,Start procedure,permitted,Yes = car can be driven  No = key is not or matched or incorrectly matched or the Engine Control Module is incorrectly adapted or malfunctioning
022,2,ECM,responding,,Yes = ECU communications OK (whether ECU is matched or not) No = not possible to match the Immo to the ECU at this time.
022,3,Key,condition OK,,Yes = a legitimate transponder code could be read (authorized or not) No = it will not be possible to match this particular key
022,4,Number of,adapted keys,A maximum of 8 adapted keys is permitted.
;
023,0,See Label File text for Block 23-4 decoding
; 0 - End of production original condition 1 - End of production new 20 - End of production programmed 21 - End of production 1.ECM adapted 22 - End of production 2.ECM adapted 23 - End of production 3.ECM adapted 24 - End of production 4.ECM adapted 30 - End of production ESCL adapted 3x - End of production x-th key adapated 4 - Service new 5 - Service programmed 6 - Immobilizer adapted 7 - ID sensor learning active 8 - ESCL adaptation 
023,1,Authentication,OK,Possible display: Yes or No
023,2,Lockbits,set,Possible display: Yes or No
023,3,Key ID,authorized,Possible display: Yes or No
023,4,Immobilizer,status,Please see the label file for decoding information.
;
024,0,Login Lockout times (all are displayed in minutes)
024,1,Immobilizer,minutes,
024,2,A-CAN,minutes
024,3,Scan protection,minutes (key)
024,4,After adaptation,minutes
;
025,0,ESCL Status
025,1,ESCL,authentication,Possible display: Valid or Not Valid
025,2,ESCL,access,Specified value:possible/not possible
;
026,0,Login Lock Status
026,1,ESL login lock,minutes,
026,2,Security access,lock (minutes)
026,3,Unknown
026,4,Unknown
;
027,0,ESCL Additional information (access to this depends on value of block 25-2 above)
027,1,ESCL mode,,Possible display:0 - end of line mode/1 - normal mode/2 - adaptation mode/3 - analyze mode
027,2,ESCL unlocking bit,status,Possible display: On or Off
027,3,ESCL locking bit,status,Possible display: On or Off
027,4,ESCL error,status,Possible display:0 - no error/1 - system info/ 2 - internal error/3 - fatal error
;
028,0,*Next documented blocks are group 50
;
50,0,Anti theft system status, rear lid status
050,1,Anti theft,alarm status,Possible display: On or Off
050,3,Rear lid,lock status,Possible display: On or Off
050,4,Unknown,(Valet Button?)
;
;Remark: This file supports Phaetons, Bentleys, and Touaregs.  'Rear Lid' can thus mean either 
;trunk lid or rear door, as is appropriate to the type of vehicle.
;
051,0,Driver Door Status
051,1,Opened,,Possible display: On or Off
051,2,Locked,,Possible display: On or Off
051,3,Safed,,Possible display: On or Off
051,4,Window,regulator,Possible display: - 0 to 100%
;
052,0,Front Passenger Door Status
052,1,Opened,,Possible display: On or Off
052,2,Locked,,Possible display: On or Off
052,3,Safed,,Possible display: On or Off
052,4,Window,regulator,Possible display: - 0 to 100%
;
053,0,Left Rear Passenger Door Status
053,1,Opened,,Possible display: On or Off
053,2,Locked,,Possible display: On or Off
053,3,Safed,,Possible display: On or Off
053,4,Window,regulator,Possible display: - 0 to 100%
;
054,0,Right Rear Passenger Door Status
054,1,Opened,,Possible display: On or Off
054,2,Locked,,Possible display: On or Off
054,3,Safed,,Possible display: On or Off
054,4,Window,regulator,Possible display: - 0 to 100%
;
056,0,Time of Day (from vehicle clock)
056,1,Unknown,,
056,2,Hour,,
056,3,Minute,,
056,4,Second,,
;
057,0,General Vehicle Information
057,1,click block,for more info,The value here relates to whether the ignition circuit is on or off - might be if car is listening for key.
057,2,Unknown,,
057,3,Vehicle,speed,Possible display:0 to 250 kilometers per hour
057,4,Gear lever,position,
;
058,0,Module Coding Status
058,1,Country,version
058,2,Engine,type
;
059,0,Solar Powered Ventilation (Parking Ventilation) status
059,1,Ventilation,status,Possible display: On or Off
;
060,0,Presumed to refer to Park Heating (stand-heating)
060,1,Park-heating,status
;
061,0,Sunroof Status
061,1,Sliding opening,range,Possible display: 0 = closed 1 - 2 - 3 - 4 - 5 = opened
061,2,Tilting opening,range,Possible display: 0 = closed 1 or 2 = opened
061,3,Function,slider open,Possible display: On or Off
061,4,Function,slider close,Possible display: On or Off
;
062,0,Status of Switches in Seat Belts
062,2,Driver Belt,switch status,Possible display: On or Off
062,3,Front Pax Belt,switch status,Possible display: On or Off
;
063,0,Diagnostic Bus Status
063,1,Unknown
063,2,Diagnostic bus,Powertrain,Possible display: On or Off
063,3,Diagnostic bus,Comfort,Possible display: On or Off
;
064,0,Unknown
;
065,0,Unknown
;
066,0,Unknown
;
067,0,*Next documented blocks - group 80
;
080,0,Manufacturer work number and identification
;
081,0,VIN number of vehicle and engine number of vehicle
;
082,0,Unknown
;
083,0,Unknown
;
084,0,*Next documented blocks are group 90
;
090,1,Clutch switch,,Possible display:on (activated)/off (not activated)
090,2,Brake light,switch,Possible display:on (activated)/off (not activated)
090,4,Starter,enabling,Possible display: On or Off
;
091,1,Engine speed,RPM,Possible display:Between 0 and 7000 RPM
091,2,Gearlever,position
;
092,0,*Next blocks are group 128
;
128,0,Unknown
;
129,0,Unknown
;
130,0,Unknown
;
131,0,Unknown
;
;
138,0,*Next blocks are group 153
;
154,0,*Next blocks are group 177
;
185,0,*Next blocks are group 188
;
189,0,*Next blocks are group 191
;
192,0,*Next blocks are group 207
;
211,0,*Next blocks are group 217
;
218,0,*End of Measured Value Blocks used by this controller.
;
;
;---------------------------------------------------
;
; Coding information
;
;---------------------------------------------------
;
;
C00,Phaeton Access and Start Control (Kessy 6400 unit - J518) Coding
C01,
C02,0133356 = USA + Keyless access + 5 speed transmission, W12 engine
C03,0137452 = USA + Keyless access + 6 speed transmission, V8 engine
C04,0002280 = USA + Central locking and remote control but no keyless + 5 speed transmission
C05,0006376 = USA + Central locking and remote control but no keyless + 6 speed transmission
C06,  
C07,0213228 = Rest of World + Keyless access + 5 speed transmission + left hand drive vehicle
C08,0218348 = Rest of World + Keyless access + 6 speed transmission + left hand drive vehicle
C09,0004328 = Rest of World + Central locking and remote control but no keyless + 6 speed transmission + left hand drive vehicle
C10,0000232 = Rest of World + Central locking and remote control but no keyless + 5 speed transmission + left hand drive vehicle
C11,  
C12,Other coding is possible for right hand drive vehicles or for Japan or for Taiwan. Contact Ross-Tech if you require it.
C13,Touareg coding will follow a similar pattern, but with different numbers.
C14,  
C15,WARNING - Only the 'whole number' combinations shown above are possible. Do NOT attempt to increment or
C16,decrement individual digits within the number. Make note of the pre-existing coding before you change anything.
;
