;
; VAG-COM label file
;
; Audi A3 (8PA)
;
; component: J234 - Airbag 9.41 (#15)
;
; p/n: 8P0-959-655-???
;
; includes measuring blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8P-15.LBL
; 8P0-959-655-8P1.LBL (8P1: 2 door)
; 8P0-959-655-8PA.LBL (8PA: 4 door)
;
; created on 01/Aug/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 22/Aug/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Igniter Status (Airbag && Tensioner)
001,1,Driver Airbag,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Passenger Airbag,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Driver Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Passenger Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
002,0,Igniter Status (Tensioner && Battery Disconnect)
002,1,Rear Left Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Rear Right Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,3,Rear Center Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,4,Battery Disconnect,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,1,Voltage supply,,Display Range: Correct/Signal too Low/Signal too High
003,2,Seat Occupation,Detection Passenger,Display Range: Child Seat/Light Adult/Medium Adult/Heavy Adult/Not Occup./Short to Ground/Short to Plus/Not Installed
003,3,Belt Inquiry,Driver,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Passenger,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry (Rear)
004,1,Belt Inquiry,Rear Left,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Right,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,3,Belt Inquiry,Rear Center,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
005,0,Igniter Status (Side Airbag)
005,1,Front Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,2,Front Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,3,Rear Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,4,Rear Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
007,0,Igniter Status (Head Airbag)
007,1,Driver Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
007,2,Passenger Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
010,0,Key Switch Status
010,1,Key Switch,Passenger Airbag,Display Range: ON/OFF
010,2,Key Switch,(HW Path),Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
010,3,Key Switch,(SW Path),Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
011,0,Igniter Status (Airbag Stage 2 && Knee Airbag)
011,1,Driver Airbag,Igniter (Stage 2),Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,2,Passenger Airbag,Igniter (Stage 2),Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,3,Driver Knee,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,4,Passenger Knee,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
016,0,Seat Occupation Recognition (J706)
016,1,Control Module,Serial: 1st/2nd digit
016,2,Control Module,Serial: 3rd/4th digit
016,3,Control Module,Serial: 5th digit
016,4,Control Module,Calibration
;
018,0,Seat Occupation Detection
018,1,Pressure Sensor
018,2,Belt Force Sensor
018,3,Acceleration Sensor
;
019,0,Workshop Codes
019,1,Workshop Code,(Last Coding),of seat occupation detection
019,2,Workshop Code,(Last 0 Calibration),of seat occupation detection
;
021,0,Igniter Resistance (Airbag && Tensioner)
021,1,Driver Airbag,Igniter,Specification: 2.1...5.6 Ohm
021,2,Passenger Airbag,Igniter,Specification: 1.6...5.6 Ohm
021,3,Driver Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
021,4,Passenger Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
;
022,0,Igniter Resistance (Tensioner && Battery)
022,1,Rear Left Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,2,Rear Right Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,3,Rear Center Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,4,Battery Disconnect,Igniter,Specification: 1.6...5.6 Ohm
;
025,0,Igniter Resistance (Side Airbag)
025,1,Front Left Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,2,Front Right Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,3,Rear Left Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,4,Rear Right Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
027,0,Igniter Resistance (Head Airbag)
027,1,Driver Head,Airbag Igniter,Specification: 1.6...5.6 Ohm
027,2,Passenger Head,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
031,0,Igniter Resistance (Airbag Stage 2 && Knee Airbag)
031,1,Driver Airbag,Igniter (Stage 2),Specification: 2.1...5.6 Ohm
031,2,Passenger Airbag,Igniter (Stage 2),Specification: 1.6...5.6 Ohm
031,3,Driver Knee,Airbag Igniter,Specification: 1.6...5.6 Ohm
031,4,Passenger Knee,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
080,0,Advanced Control Module Identification I
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Instrument Cluster,,Specification: Instruments 1
125,2,Brake Electronics,,Specification: ABS 1
;
225,0,CAN-Databus Time-Out (Powertrain)
225,1,Instrument Cluster
225,2,Brake Electronics
;
