;
; VAG-COM label file
;
; Audi A4 (8E2/8E5)
;
; component: J519 - Central electric (#09)
;
; p/n: 8E0 907 279  /A/B/C/D/E/F
;
; includes measuring blocks, adaptation and coding
;
; created by Eric Maurier (eric@ross-tech.com // www.vag.com.fr)
; adaptation/coding added by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 09/27/2004
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
1,0,Output signals,
1,1,Supply voltage,
1,2,Horn,
1,3,Terminal 75,
1,4,Headlight,washer

2,0,Output signals: Turn signals,
2,1,Turn signal FL,
2,2,Turn signal RL,
2,3,Turn signal FR,
2,4,Turn signal RR,

3,0,Output signals: Park, lights,
3,1,Park. light FL,
3,2,Park. light RL,
3,3,Park. light FR,
3,4,Park. light RR,

4,0,Output signals,
4,1,High beam G,
4,2,High beam D,
4,3,License plate,light
4,4,Warning button,illumination,

5,0,Output signals: wipers,
5,1,Front wiper,
5,2,Front washer,
5,3,Rear wiper,
5,4,Rear washer,

6,0,Input signals,
6,1,Rotary,light switch
6,2,Warning button,activation, 
6,3,Terminal 75,
6,4,Wiper speed


7,0,Input signals on comfort bus,
7,1,High beams,
7,2,Flashing,
7,3,Turn signal L,
7,4,Turn signal R,


8,0,Input signals on comfort bus: wipers,
8,1,Front wiper,
8,2,Front washer,
8,3,Rear wiper,
8,4,Rear washer,

9,0,Input signals on comfort bus,
9,1,Terminal 15,
9,2,S Contact,
9,3,Speed interval,
9,4,Vacant,

10,0,Output signals (highline only),
10,1,Low beam left,
10,2,Low beam right,
10,3,Backup light,left
10,4,Backup light,right

11,0,Output signals (highline only),
11,1,Fog light FL,
11,2,Fog light FR,
11,3,Fog light rear,
11,4,Vacant,

12,0,Output signals (highline only),
12,1,Brake light,left
12,2,Brake light,right
12,3,Brake light,center
12,4,Vacant

13,0,Input signals (highline only),
13,1,Brake switch
13,2,Brake switch,(test)
13,3,Light sensor
13,4,Vacant

14,0,Input signals bus confort(highline only),
14,1,Driver`s door,open
14,2,Speed,
14,3,Outside temp,
14,4,Vacant,

80,0,Controller advanced ID,
80,1,Manufacturer,
80,2,Completion date,
80,3,Version and,test stand
80,4,Man. number,

81,0,Controller advanced ID,
81,1,VIN,
81,2,Serial number,
81,3,Vacant,
81,4,Vacant,

125,0,Communications on comfort bus,
125,1,Instruments,
125,2,Steering wheel,
125,3,Comfort module,
125,4,Trailer controller,

126,0,Communications on comfort bus,
126,1,Driver`s door,controller
126,2,Vacant,
126,3,Vacant,
126,4,Vacant,
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,J519 - Central electric (Coding)
C1,0?xxx - Light sensor
C2,0 - without light sensor
C3,1 - with light sensor
C4, 
C5,0x?xx - trailer hitch
C6,0 - without trailer hitch
C7,1 - with trailer hitch
C8, 
C9,0xx?x - Headlights
C10,0 - Halogen headlights
C11,1 - Xenon headlights
C12, 
C13,0xxx? - Country variation
C14,1 - Rest of World
C15,2 - Rest of World North countries (Finland, Sweden, Norway, Denmark)
C16,3 - USA
C17,4 - Canada
;
;
;---------------------------------------------------
;
; Adaptation informations
;
;---------------------------------------------------
;
;
A1,0,Coming Home
A1,5,Coming Home
A2,6,Note: Only 8E0 907 279 E/F
A2,7, 
A1,8,If the system is activated and it's dark
A1,9,fog lights/parking lights/taillights/lisence plate lights
A1,10,are switched on as soon as the drivers door is opened.
A1,11, 
A1,12,Factory setting: 30 seconds
A1,13,Range: 30...60 seconds (increments 1 s)
;
A2,0,Brake light dimming
A2,5,Brake light dimming
A2,6,Note: Only 8E0 907 279 E/F
A2,7, 
A2,8,Sedan: 24%
A2,9,Avant: 0%
;
A81,0,Learned Values (Vehicle Data)
A81,5,Learned Values (Vehicle Data)
A81,6,To start the process for vehicle data (VIN)
A81,7,learning enter/save 46992 as new value.
;
