;
; VAG-COM label file
;
; VW New Beetle (1C) / New Beetle Cabriolet (1Y)
;
; component: Engine (#01) - BKF
;
; p/n: 06A-906-032-???
;
; includes measuring blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 06-01.LBL
; 06A-906-032-BKF.LBL  (1.8l T   @ 150 HP - BKF)
;
; created on 24/Aug/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 24/Aug/2005
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,Engine Speed,,Specification (idle): 780 RPM
001,2,Coolant,Temperature,Specification: 80.0...110.0 °C
001,3,Lambda,Controller,Specification: -10.0...+10.0
001,4,Basic Setting,Requirements
; 1xxxxxxx - Coolant Temperature below 80 °C
; x1xxxxxx - Engine Speed below 2000 RPM
; xx1xxxxx - Throttle Valve closed
; xxx1xxxx - Lambda Regulation correct
; xxxx1xxx - Idle Condition
; xxxxx1xx - A/C System Compressor deactivated
; xxxxxx1x - Catalyst Temperature correct
; xxxxxxx1 - No Malfunctions detected
;
002,0,Basic Functions (Mass Air Flow)
002,1,Engine Speed,,Specification (idle): 780 RPM
002,2,Engine Load,,Specification: 16.0...35.0 %
002,3,Injection,Timing
002,4,Intake Air Mass,,Specification: 2.0...4.5 g/s
;
003,0,Basic Functions (Mass Air Flow)
003,1,Engine Speed,,Specification (idle): 780 RPM
003,2,Intake Air Mass,,Specification: 2.0...4.5 g/s
003,3,Throttle Drive,Angle Sensor 1,for EPC (G187)
003,4,Ignition,Timing Angle
;
004,0,Basic Functions
004,1,Engine Speed,,Specification (idle): 780 RPM
004,2,Voltage Supply,,Specification: 11.0...15.0 V
004,3,Coolant,Temperature,Specification: 80...110 °C
004,4,Intake Air,Temperature
;
005,0,Basic Functions
005,1,Engine Speed,,Specification (idle): 780 RPM
005,2,Engine Load,,Specification: 16.0...35.0 %
005,3,Vehicle Speed,,Specification: 0 km/h
005,4,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
;
006,0,Basic Functions
006,1,Engine Speed,,Specification (idle): 780 RPM
006,2,Engine Load,,Specification: 16.0...35.0 %
006,3,Intake Air,Temperature
006,4,Altitude,Correction Factor
;
008,0,Basic Functions
008,1,Brake Condition,,Display Range: Operated/Not Oper.
008,2,Voltage Supply,,Specification: 11.0...15.0 V
008,3,Brake Vacuum,Pump Condition,Display Range: Pump ON/OFF
008,4,Brake Booster,Pressure
;
010,0,Ignition
010,1,Engine Speed,,Specification (idle): 780 RPM
010,2,Engine Load,,Specification: 16.0...35.0 %
010,3,Throttle Drive,Angle Sensor 1,for EPC (G187)
010,4,Ignition,Timing Angle
;
011,0,Ignition
011,1,Engine Speed,,Specification (idle): 780 RPM
011,2,Coolant,Temperature,Specification: 80...110 °C
011,3,Intake Air,Temperature
011,4,Ignition,Timing Angle
;
014,0,Ignition (Misfire Recognition)
014,1,Engine Speed,,Specification (idle): 780 RPM
014,2,Engine Load,,Specification: 16.0...35.0 %
014,3,Misfire,(total),Specification: 0
014,4,Misfire,recognition,Specification: active | Display Range: active/inactive
;
015,0,Misfire Recognition
015,1,Cylinder 1
015,2,Cylinder 2
015,3,Cylinder 3
015,4,Malfunction,Recognition,Display Range: activated/blocked
;
016,0,Misfire Recognition
016,1,Cylinder 4
016,4,Malfunction,Recognition,Display Range: activated/blocked
;
018,1,Lower,RPM Barrier
018,2,Upper,RPM Barrier
018,3,Lower,Load Barrier
018,4,Upper,Load Barrier
;
020,0,Ignition (Knock Control)
020,1,Cylinder 1 Ignition,Angle Delay
020,2,Cylinder 2 Ignition,Angle Delay
020,3,Cylinder 3 Ignition,Angle Delay
020,4,Cylinder 4 Ignition,Angle Delay
;
023,0,Ignition (Knock Control - Cyl 1 && 2)
023,1,Engine Speed
023,2,Engine Load,,Specification: 16.0...35.0 %
023,3,Cylinder 1 Ignition,Angle Delay
023,4,Cylinder 2 Ignition,Angle Delay
;
023,0,Ignition (Knock Control - Cyl 3 && 4)
023,1,Engine Speed
023,2,Engine Load,,Specification: 16.0...35.0 %
023,3,Cylinder 3 Ignition,Angle Delay
023,4,Cylinder 4 Ignition,Angle Delay
;
026,0,Ignition (Knock Control)
026,1,Voltage,Cylinder 1,Specification: max. 5 V
026,2,Voltage,Cylinder 2,Specification: max. 5 V
026,3,Voltage,Cylinder 3,Specification: max. 5 V
026,4,Voltage,Cylinder 3,Specification: max. 5 V
;
028,0,Knock Sensor Test (Short Trip)
028,1,Engine Speed
028,2,Engine Load
028,3,Engine Coolant,Temperature
028,4,Result,,Specification: Test ON/Test OFF/Sys. OK/Sys. not OK
;
030,0,Oxygen Sensor Status
030,1,Bank 1,Sensor 1
; 1xxxx - Lambda Sensor Control Cyl. 1 active
; x1xxx - Catalytic Converter Venting active
; xx1xx - Lambda Sensor Heating on
; xxx1x - Lambda Sensor ready
; xxxx1 - Lambda Regulation active
030,2,Bank 1,Sensor 2
; 1xxx - Enabling P Factor
; x1xx - Lambda Sensor Heating on
; xx1x - Lambda Sensor ready
; xxx1 - Lambda Regulation active
030,3,Bank 1,Sensor 3
; 1xxx - Enabling P Factor
; x1xx - Lambda Sensor Heating on
; xx1x - Lambda Sensor ready
; xxx1 - Lambda Regulation active
;
031,0,Lambda Regulation
031,1,Lambda Sensor,(actual)
031,2,Lambda Sensor,(specified)
;
032,0,Lambda Regulation
032,1,Lambda (Idle),Self-Adaptation,Specification: -5...+5 %
032,2,Lambda (Partial),Self-Adaptation,Specification: -10...+10 %
;
034,0,Lambda Regulation (befor Catalyst - Basic Setting: Aging Check)
034,1,Engine Speed
034,3,Period,Duration Sensor
034,4,Result,Lambda Aging,Display Range: Test ON/Test OFF/B1-S1 not OK/B1-S1 OK
;
037,0,Lambda Regulation (after Catalyst - Basic Setting)
037,1,Engine Load,,Specification: 16...35.0 %
037,2,Bank 1 Sensor 1,Voltage
037,3,Lambda Regulator,Dwell Period
037,4,Result,,Specification: Test ON/Test OFF/Sys. OK/Sys. not OK
;
039,0,Lambda Regulation (Sensor Exchange)
039,1,Intake Air Mass,,Specification: 2.0...4.5 g/s
039,2,Bank 1 Sensor 2,Voltage
039,3,Bank 1 Sensor 3,Voltage
039,4,Lambda Sensor,Exchange Result,Specification: Test ON/Test OFF/Sys. OK/Sys. not OK
;
041,0,Lambda Regulation (Lambda Probe Heating)
041,1,Resistance,Bank 1 Sensor 1
041,2,Heater Condition
041,3,Resistance,Bank 1 Sensor 2
041,4,Heater Condition
;
042,0,Lambda Regulation (Lambda Probe Heating)
042,1,Resistance,Bank 1 Sensor 3
042,2,Heater Condition
;
043,0,Oxygen Sensor Control (Bank 1 Sensor 2)
043,1,Engine Speed
043,2,Catalyst,Temperature
043,3,Lambda Sensor,Voltage (B1-S2)
043,4,Result,Aging Check,Specification: B1-S2 OK | Display Range: Test OFF/Test ON/B1-S2 OK/B1-S2 nOK
;
044,0,Oxygen Sensor Control (Bank 1 Sensor 3)
044,1,Engine Speed
044,2,Catalyst,Temperature
044,3,Lambda Sensor,Voltage (B1-S3)
044,4,Result,Aging Check,Specification: B1-S3 OK | Display Range: Test OFF/Test ON/B1-S3 OK/B1-S3 nOK
;
046,0,Oxygen Sensor Control (Pre-Catalytic Converter)
046,1,Engine Speed
046,2,Catalyst,Temperature
046,3,Amplitude Ratio
046,4,Result,Catalyst Test,Specification: Cat B1 OK | Display Range: Test OFF/Test ON/Cat B1 OK/Cat B1 nOK
;
047,0,Oxygen Sensor Control (Main-Catalytic Converter)
047,1,Engine Speed
047,2,Catalyst,Temperature
047,3,Amplitude Ratio
047,4,Result,Catalyst Test,Specification: Cat B1 OK | Display Range: Test OFF/Test ON/Cat B1 OK/Cat B1 nOK
;
050,0,Speed Regulation
050,1,Engine Speed,(actual),Specification (idle): 780 RPM
050,2,Engine Speed,(specified)
050,3,Condition,of A/C system,Display Range: A/C-High / A/C-Low
050,4,Operating condition,of A/C Compressor,Display Range: Compr.ON/Compr.OFF
;
051,0,Speed Regulation
051,1,Engine Speed,(actual),Specification (idle): 780 RPM
051,2,Engine Speed,(specified)
051,3,Selected Gear,,0 = P/N\n1...6 = Gear 1...6\n7 = R
051,4,Voltage Supply,,Specification: 11.0...15.0 V
;
052,0,Speed Regulation
052,1,Engine Speed,(actual),Specification (idle): 780 RPM
052,2,Engine Speed,(specified)
052,3,Condition,of A/C system,Display Range: A/C-High / A/C-Low
;
053,0,Speed Regulation
053,1,Engine Speed,(actual),Specification (idle): 780 RPM
053,2,Engine Speed,(specified)
053,3,Voltage Supply,,Specification: 11.0...15.0 V
;
054,0,Speed Regulation
054,1,Engine Speed,,Specification (idle): 780 RPM
054,2,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
054,3,Sender 2 for,Acc. Pedal Pos.,G79 (Specification: 0...100 %)
054,4,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0...100 %
;
055,0,Speed Regulation
055,1,Engine Speed,,Specification (idle): 780 RPM
055,2,Idle Regulator
055,3,Idle Stabilization,Self-Adaptation
055,4,Load Status,,see labelfile
; 1xxxx - Power assisted steering pressure switch on
; x1xxx - Rear window defroster
; xx1xx - Air conditioning system switched on
; xxx1x - Gear engaged
; xxxx1 - Air conditioner compressor switched on
;
056,0,Speed Regulation
056,1,Engine Speed,(actuial)
056,2,Engine Speed,(specified)
056,3,Idle Regulator
056,4,Load Status
; 1xxxx - Power assisted steering pressure switch on
; x1xxx - Rear window defroster
; xx1xx - Air conditioning system switched on
; xxx1x - Gear engaged
; xxxx1 - Air conditioner compressor switched on
;
057,0,Idle Air Control (A/C Compressor)
057,1,Engine Speed,(actuial)
057,2,Engine Speed,(specified)
057,3,A/C Compressor,Status
;
058,1,Engine Speed,,Specification (idle): 780 RPM
058,2,Engine Load,,Specification: 12...175 %
;
060,0,Speed Regulation (Basic Setting: Throttle Body Adaptation)
060,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0...100 %
060,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 100...0 %
060,3,Learn Step,Counter,Specification: 0...8
060,4,Result,Throttle Valve Adp.,Display Range: ADP runs/ADP OK/ADP ERROR
;
061,0,Speed Regulation (EPC)
061,1,Engine Speed,,Specification (idle): 780 RPM
061,2,Voltage Supply,,Specification: 11.0...15.0 V
061,3,Activation Throttle,Position Actuator,G186 (Specification: 0...100 %)
061,4,Operating,Condition
; 1xxxx - Power assisted steering pressure switch on
; x1xxx - Rear window defroster
; xx1xx - Air conditioning system switched on
; xxx1x - Gear engaged
; xxxx1 - Air conditioner compressor switched on

;
062,0,Speed Regulation (Basic Setting: EPC Adaptation)
062,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0...100 %
062,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 100...0 %
062,3,Throttle Position,Sensor (G79),Specification: 0...100 %
062,4,Accelerator Pedal,Position Sensor 2,G185 (Specification: 0...100 %)
;
063,0,Speed Regulation (Basic Setting: Kick-Down Adaptation)
063,1,Throttle Position,Sensor (G79),Display Range: 0...100 %
063,2,Accelerator Pedal,Position Sensor 2,G185
063,3,Kick-Down,Switch,Display Range: Kick Down
063,4,Kick-Down,Adaptation,Display Range: ADP runs/ADP OK/ADP ERROR
;
064,0,Throttle Valve Potentiometer Adaption Values
064,1,Potentiometer 1,Lower Adaptation
064,2,Potentiometer 2,Lower Adaptation
064,3,Emergency Air Gap,Potentiometer 1
064,4,Emergency Air Gap,Potentiometer 2
;
066,0,Cruise Cntrol System
066,1,Current,Vehicle Speed
066,2,Brake switch,clutch and CCS,Specification: ----1000
; ----1xxx - Cruise control system active
; ----x1xx - Clutch depressed (always 1 in automatic transmission)
; ----xx1x - Brake depressed (brake pedal switch)
; ----xxx1 - Brake depressed (brake light switch)
066,3,Specified,Vehicle Speed
066,4,CCS Control,Positions,Specification: ----0011
; ----1xxx - CCS slide handle on RES or RES button on multi-function steering wheel pressed
; ----x1xx - SET button pressed
; ----xx1x - CCS slide handle on OFF (not engaged or engaged)/OFF button on multi-function steering wheel pressed
; ----xxx1 - CCS slide handle on OFF
;
070,0,Emission Reduction (TEV - Basic Setting)
070,1,Evap. Emissions,Sol. Valve (Open),Specification: 0...100 %
070,2,Lambda Regulator,Deviation
070,3,Evap. Emissions,Sol. Valve (Flow)
070,4,Result,Evap. Emissions,Display Range: Test ON/Test OFF/TEV OK/TEV not OK
;
071,0,Exhaust Reduction (Basic Setting: Leak Diagnostic System)
071,1,Reed Contact,Condition,Display Range: Reed closed/Reed open
071,2,Malfunction Display,,Display Range: minor leak/significant leak/Open circuit
071,3,Diagnostic Status,,Display Range: System test/Measurement end
071,4,Result,Leak Test,Display Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
077,0,Emission Reduction (Basic Setting: Secondary Air System Diagnostic)
077,1,Engine Speed,,Specification (idle): 780 RPM
077,2,Intake Air Mass,,Specification: 2.0...4.5 g/s
077,3,Secondary Air,System Air Mass,Specification: -100...+100 %
077,4,Diagnostic,Result,Specification: Sys. OK\nDisplay Range: Test ON/Test OFF/Syst. OK/Syst. nOK
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,VIN & IMMO-ID
;
082,0,Advanced Control Module Identification III
;
089,0,Trip Odometer (MIL On)
089,1,Trip Distance,with MIL on
089,2,Tank empty,,Display Range: OK/too small
;
090,0,Camshaft Adjustment
090,1,Engine Speed,,Specification (idle): 780 RPM
090,2,Camshaft,Adjustment,Display Range: ON/OFF
090,3,Active Camshaft,Adjustment Angle
;
091,0,Camshaft Adjustment
091,1,Engine Speed,,Specification (idle): 780 RPM
091,2,Engine Load,,Specification: 12...175 %
091,3,Camshaft,Adjustment,Display Range: ON/OFF
091,4,Active Camshaft,Adjustment Angle
;
093,0,Camshaft Adaption Values (Intake)
093,1,Engine Speed,,Specification (idle): 780 RPM
093,2,Angle Deviation,(current vs. Spec.)
093,3,Phase Position,Bank 1
;
094,0,Camshaft Adjustment (Basic Setting)
094,1,Engine Speed,,Specification (idle): 780 RPM
094,2,Camshaft,Adjustment,Specification: Cam Ctrl. ON\nDisplay Range: Cam Ctrl. ON/OFF
094,3,Diagnostic,Result,Specification: Syst. OK\nDisplay Range: Test OFF/Test ON/Syst.OK/Syst. nOK
;
099,0,Oxygen Sensor Control (Basic Setting: Oxygen Sensor Operating Condition)
099,1,Engine Speed,,Specification (idle): 780 RPM
099,2,Coolant,Temperature,Specification: 80.0...110.0 °C
099,3,Lambda Sensor,Control
099,4,Lambda Sensor,Condition,Specification: O2-Reg ON/OFF
;
100,0,Readiness
100,1,Readiness Bits,,see labelfile
; 1xxxxxxx - Exhaust Gas Recirculation (EGR)
; x1xxxxxx - Sensor heater
; xx1xxxxx - Oxygen sensors
; xxx1xxxx - A/C system
; xxxx1xxx - Secondary Air Injection (AIR) system
; xxxxx1xx - Activated charcoal system
; xxxxxx1x - Catalytic converter heater
; xxxxxxx1 - Catalytic converter
100,2,Coolant,Temperature,Specification: 80.0...110.0 °C
100,3,Time since,Engine Start
100,4,OBD-Status,,see labelfile
; 1-xx--xx - MIL warning lamp on
; x-1x--xx - Complete distance
; x-x1--xx - At least one malfunction detected
; x-xx--1x - Heating cycle ended
; x-xx--x1 - Heating cycle not possible
;
101,0,Fuel Injection
101,1,Engine Speed,,Specification (idle): 780 RPM
101,2,Engine Load,,Specification: 12...175 %
101,3,Mean Injection,Timing
101,4,Intake Air Mass,,Specification: 2.0...4.5 g/s
;
102,0,Fuel Injection
102,1,Engine Speed,,Specification (idle): 780 RPM
102,2,Coolant,Temperature,Specification: 80.0...110.0 °C
102,3,Intake Air,Temperature
102,4,Mean Injection,Timing
;
104,1,Start Engine,Temperature
104,2,Temperature,Adaptation Factor 1
104,3,Temperature,Adaptation Factor 2
104,4,Temperature,Adaptation Factor 3
;
105,0,Cylinder Deactivation
105,1,Engine Speed,,Specification (idle): 780 RPM
105,2,Engine Load,,Specification: 12...175 %
105,3,Coolant,Temperature,Specification: 80.0...110.0 °C
105,4,Shut-Off Status,,Display Range: ON/OFF
;
107,0,Oxygen Sensor Control (Basic Setting: Diagnostic of Fuel System)
107,1,Engine Speed,,Specification (idle): 780 RPM
107,2,Oxygen Sensor,Control Bank 1
107,4,Result,Lambda Control,Display Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
110,0,Load/Full Load Enrichment
110,1,Engine Speed,,Specification (idle): 780 RPM
110,2,Coolant,Temperature,Specification: 80.0...110.0 °C
110,3,Average,Injection Time
110,4,Throttle Drive,Angle Sensor 1,for EPC (G187)\nDisplay Range: 0...100 %
;
111,0,Charge Pressure Control
111,1,RPM Range 1,,Specification: -33.0...+33.0 %
111,2,RPM Range 2,,Specification: -33.0...+33.0 %
111,3,RPM Range 3,,Specification: -33.0...+33.0 %
111,4,RPM Range 4,,Specification: -33.0...+33.0 %
;
113,0,Charge Pressure Control
113,1,Engine Speed,,Specification (idle): 780 RPM
113,2,Engine Load,,Specification: 12...175 %
113,3,Throttle Drive,Angle Sensor 1,for EPC (G187)\nDisplay Range: 0...100 %
113,4,Athmospheric,Pressure
;
114,0,Charge Pressure Control
114,1,Engine Load,(specified),Specification: max. 175.0 %
114,2,Engine Load,(spec. corrected),Specification: max. 175.0 %
114,3,Engine Load,(actual Value),Specification: 12.0...175.0 %
114,4,Wastegate (N75),Duty Cycle,Specification: 0...100 %
;
115,0,Charge Pressure Control
115,1,Engine Speed,,Specification (idle): 780 RPM
115,2,Engine Load,,Specification: 12...175 %
115,3,Boost Pressure,(specified),Specification: max. 2000 mbar
115,4,Boost Pressure,(actual),Specification: max. 2000 mbar
;
116,0,Charge Pressure Control
116,1,Engine Speed,,Specification (idle): 780 RPM
116,2,Fuel Temp.,Correction Factor
116,3,Coolant Temp.,Correction Factor
116,4,Intake Air Temp.,Correction Factor
;
117,0,Charge Pressure Control
117,1,Engine Speed,,Specification (idle): 780 RPM
117,2,Throttle Position,Sensor (G79),Display Range: 0...100 %
117,3,Throttle Drive,Angle Sensor 1,for EPC (G187)\nDisplay Range: 0...100 %
117,4,Boost Pressure,(specified),Specification : max. 2000 mbar
;
118,0,Charge Pressure Control
118,1,Engine Speed,,Specification (idle): 780 RPM
118,2,Intake Air,Temperature
118,3,Wastegate (N75),Duty Cycle,Specification: 0...100 %
118,4,Boost Pressure,(actual),Specification: max. 2000 mbar
;
119,0,Charge Pressure Control
119,1,Engine Speed,,Specification (idle): 780 RPM
119,2,Charge Limit
119,3,Wastegate (N75),Duty Cycle,Specification: 0...100 %
119,4,Boost Pressure,(actual),Specification: max. 2000 mbar
;
120,0,Traction Control (ASR)
120,1,Engine Speed,,Specification (idle): 780 RPM
120,2,Engine Load,(specified)
120,3,Engine Load,(actual)
120,4,Status,,Specification: active/not active
;
122,0,Transmission (automatic only)
122,1,Engine Speed,,Specification (ilde): 780 RPM
122,2,Engine Load,(specified
122,3,Engine Load,(actual)
122,4,Status,,Display Range: Engine interv./No engine interv.
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Transmission
125,2,Brake Electronics
125,3,Instrument Cluster
;
126,0,CAN-Databus Communication (Powertrain)
126,3,Airbag
;
