;
; VAG-COM label file
;
; Audi A4 (8E2/8E5)
;
; Component: J285 - Instrument cluster (#17)
;
; P/N: 
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8E-17.LBL
; 8E0-920-9xx-8E2.LBL
; 8E0-920-9xx-8ED.LBL
;
; created on 02/oct/2004 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 14/Sep/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,1,Speed,[km/h]
001,2,RPM,[1000/min]
001,3,Oil pressure,switch 2,Display range: Oilp.2<min/Oilp.2 OK
001,4,Time,[hh:mm]
;
002,1,Odometer,[km]
002,2,Status remote,clock receiver,Display range: OK/not OK
002,3,Comfort-CAN,Information,see Label-File
; xx1 - Right-Hand-Drive (RHD)/Left-Hand-Drive (LHD) (1=RHD/0=LHD)
; x1x - Install four-door (1=four-door/0=two-door)
; 1xx - °C/°F (1=°F/0=°C)
002,4,External,temperature,[°C]
;
003,1,Coolant,temperature
003,2,Standing,time [min]
003,3,Dimming signal,terminal 58d [%]
003,4,Dimming signal,terminal 58s [%]
;
004,1,Tank display,[liters]
004,2,Tank sensor,[Ohm]
004,3,Tank display,2nd sensor [l],All wheel drive only
004,4,Tank sensor,2nd sensor [Ohm],All wheel drive only
;
005,0,Service interval
005,1,Kilometers,before/after
005,2,Days,before/after
005,3,engine hood,contact,Display range: open/closed
005,4,Calculated,service interval
;
006,0,Oil level
006,1,Oil level,MIN value [mm]
006,2,Oil level,MAX value [mm]
006,3,Oil level 100 km,intermediate value
006,4,[N/A]
;
007,0,Oil level (resolution 0.01 mm)
007,1,Oil level,current value
007,2,Oil level,shaft,current value from engine control module
007,3,[N/A]
007,4,[N/A]
;
010,0,Adaptation channels
010,1,Channel 30
010,2,Adaptation of,tank sensor
010,3,Channel 9
010,4,Kilometer,,Resolution: 0.1
;
011,0,Adaptation channels
011,1,Channel 4
011,2,Language,variations,see adaptation channels
011,3,Channel 3
011,4,Consumption,correction
;
012,0,Adaptation channels
012,1,Channel 40
012,2,Distance traveled,as of insp.,Resolution: 0.01
012,3,Channel 41
012,4,Time as of,inspection
;
013,0,Adaptation channels
013,1,Channel 42
013,2,Min. value km
013,3,Channel 43
013,4,Max. value km
;
014,0,Adaptation channels
014,1,Channel 44
014,2,Max. time,interval
014,3,Channel 49
014,4,[N/A]
;
015,0,Adaptation channels
015,1,Channel 45
015,2,Oil quality
015,3,Channel 46
015,4,Consumption,quantity
;
016,0,Adaptation channels
016,1,Channel 47
016,2,Soot index
016,3,Channel 48
016,4,Thermal load
;
017,0,Adaptation channels
017,1,Channel 60
017,2,Powertrain,CAN-Databus
017,3,Channel 61
017,4,Comfort,CAN-Databus
;
018,0,Adaptation channels
018,1,Channel 62
018,2,Information,CAN-Databus
018,3,[N/A]
018,4,[N/A]
;
019,0,Adaptation channels
019,1,Channel 18
019,2,Auxiliary,heater
019,3,Channel 19
019,4,Remote clock,configuration
;
022,0,Immobilizer
022,1,Starting,permitted
022,2,Engine (ECM),responds
022,3,Key condition,OK
022,4,Number of,keys coded
;
023,0,Immobilizer
023,1,Variable code,authorized
023,2,Key status,(transponder)
023,3,Fixed code,authorized
023,4,Immobilizer,status,see labelfile
; 4 - new customer service - delivery condition (replacement part instrument cluster)
; 5 - customer service locked - adaptation data programmed in customer service
; 6 - immobilizer adapted - normal function condition
; 7 - key adaptation active - key adaptation via tester
;
024,0,Immobilizer - locking periods
024,1,Instrument,cluster
024,2,Engine control, module (ECM)
024,3,Emergency,release
024,4,Transponder,recognition
;
025,0,CAN-Communication
025,1,CAN-communication,to ECM
025,2,[N/A]
025,3,[N/A]
025,4,[N/A]
;
050,1,Odometer,[km]
050,2,RPM,[1/min]
050,3,Oil temperature,[°C]
050,4,Coolant,temperature,[°C]
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test number
;
082,0,Flash-Tool-Code (FTC)
; Flash-Date (in dd.mm.yy)
;
125,0,CAN-Databus communication (Powertrain)
125,1,Engine
125,2,Transmission
125,3,ABS
125,4,ADR
;
126,0,CAN-Databus communication (Powertrain)
126,1,[N/A]
126,2,4C air spring
126,3,[N/A]
126,4,[N/A]
;
130,0,CAN-Databus communication (Comfort)
130,1,Tire pressure
130,2,Auxiliary heater
130,3,Control module,comfort system
130,4,Trailer
;
131,0,CAN-Databus communication (Comfort)
131,1,Control module,electrical system
131,2,Steering column,module
131,3,Climate control
131,4,Operating,K-CAN,Display range: one wire/tow wire
;
132,0,CAN-Databus communication (Comfort)
132,1,Convertible top
132,2,[N/A]
132,3,[N/A]
132,4,[N/A]
;
140,0,CAN-Databus communication (Infotainment)
140,1,Radio
140,2,Telephone
140,3,Navigation
140,4,Telematics
;
141,0,CAN-Databus communication (Infotainment)
141,1,Speech input
141,2,[N/A]
141,3,[N/A]
141,4,Operating type,D-CAN
;
200,0,Tank display - consumption correction (per EEPROM-Bit switch off ability)
200,1,Uncorrected,display value,VAOK
200,2,Corrected,display value,VAK
200,3,Damped corrected,value,VA
200,4,[N/A]
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,J285 - Instrument cluster
C1,??x01 - Equipment variations
C2,+00 - 1. K-Number (Europe, USA, Rest of World)
C3,+01 - Smaller fuel tank volume (All wheel drive)
C4,+02 - Seatbelt warning (NAR old - NOT USA from 45/2004)
C5,+04 - 3. K-Number (rental cars)
C6,+08 - 2. K-Number (Australia)
C7, 
C8,xx?01 - Country variations
C9,0 - Germany (D) / 1 - Rest of World (RoW)
C10,2 - USA (US) / 3 - Canada (CDN)
C11,4 - Great Britain (GB) / 5 - Japan (JP)
C12,6 - Arabic states / 7 - Australia (AUS)
C13, 
C14,xxx?1: Seatbelt warning (USA only | 45/2004 >)
C15,3 - Seatbelt warning (NAR new)
C16,
C17,Note: The speedometer lead or distance driven lead is set with the K-number. 
C18,PR-9P1 - Seatbelt warning (E-contact in belt lock)
C19,PR-9P5 - Seatbelt warning (optical and acoustic / E-contact in belt lock)
C20,PR-F4F - Rental car equipment
;
;
;---------------------------------------------------
;
; Adaptation informations
;
;---------------------------------------------------
;
;
A3,0,Consumption correction
A3,5,Consumption correction
A3,6,85...115 % (in 5% increments)
;
A4,0,Language variants
A4,5,Language variants
A4,6,1 - German
A4,7,2 - English
A4,8,3 - French
A4,9,4 - Italian
A4,10,5 - Spanish
A4,11,6 - Portuguese
A4,12,8 - Chinese
;
A9,0,Mileage
A9,5,Mileage
A9,6,km/miles reading
A9,7,Resolution: 0.01
;
A18,0,Auxiliary heating
A18,5,Auxiliary heating
A18,6,0 - no auxiliary heating installed
A18,7,1 - Auxiliary heating installed
A18,8,2 - Auxiliary heating installed and goes out when turning engine off
A18,9,3 - only auxiliary ventilation
A18,10,4 - only auxiliary ventilation and goes out when turning engine off
;
A19,0,Additional features
A19,5,Additional features
A19,6,?xxxx - Illumination option
A19,7,0 - Needle and scala only active at 'Light on"
A19,8,1 - Needle already active at 'Ignition on'
A19,9,2 - Scale already active at 'Ignition on'
A19,10,3 - Scala (2. map) and needle at "ignition on" active
A19,11, 
A19,12,x?xxx - Board computer
A19,13,0 - only level 2 (long time memory)
A19,14,1 - level 1 and 2
A19,15, 
A19,16,xx?xx - Driver Information System (DIS)
A19,17,0 - DIS 1 / 1 - Highline without DIS / 2 - DIS 2
A19,18, 
A19,19,xxx?x - Outside temperature
A19,20,0 - no display, illumination goes out
A19,21,1 - Display and illumination active
A19,22, 
A19,23,xxxx? - Remote clock
A19,24,0 - Remote clock not active / 1 - Remote clock active
;
A29,0,Tank characteristic (fuel level sensor 2)
A29,5,Tank characteristic (fuel level sensor 2)
A29,6,Parallel shift of tank characteristic by +/- 32 Ohm
A29,7,Value range: 96...160
;
A30,0,Tank characteristic
A30,5,Tank characteristic
A30,6,Parallel shift of tank characteristic by +/- 32 Ohm
A30,7,Value range: 96...160
;
A34,0,Fuel gauge display - additional functions
A34,5,Fuel gauge display - additional functions
A34,6,?xx - Full correction sensor 1
A34,7,1 - active / 0 - not active
A34,8, 
A34,9,x?x - Empty correction sensor
A34,10,1 - active / 0 - not active
A34,11, 
A34,12,xx? - Monitoring sensor
A34,13,1 - active / 0 - not active
;
A35,0,Speed threshold
A35,5,Speed threshold
A35,6,Value for speed threshold of dynamic oil pressure system
A35,7,from 0 to 1000 RPM in increments from 250 RPM.
;
A40,0,Distance from inspection
A40,5,Distance from inspection
A40,6,Resolution: 1 = 100 km
A40,7, 
A40,8,NOTE: Adaptation channels 40-48 must be
A40,9,entered and stored in the following order:
A40,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A41,0,Time from inspection
A41,5,Time from inspection
A41,6, 
A41,7,NOTE: Adaptation channels 40-48 must be
A41,8,entered and stored in the following order:
A41,9,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A42,0,Minimum value mileage
A42,5,Minimum value mileage
A42,6,Resolution: 1 = 1000 km
A42,7, 
A42,8,NOTE: Adaptation channels 40-48 must be
A42,9,entered and stored in the following order:
A42,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A43,0,Maximum value mileage
A43,5,Maximum value mileage
A43,6,Resolution: 1 = 1000 km
A43,7, 
A43,8,NOTE: Adaptation channels 40-48 must be
A43,9,entered and stored in the following order:
A43,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A44,0,Maximum time interval
A44,5,Maximum time interval
A44,6, 
A44,7,NOTE: Adaptation channels 40-48 must be
A44,8,entered and stored in the following order:
A44,9,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A45,0,Oil quality
A45,5,Oil quality
A45,6,Value range: 0.5 - 2.0
A45,7, 
A45,8,NOTE: Adaptation channels 40-48 must be
A45,9,entered and stored in the following order:
A45,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A46,0,Total consumption amount (Gas only)
A46,0,Total consumption amount (Gas only)
A46,6, 
A46,7,NOTE: Adaptation channels 40-48 must be
A46,8,entered and stored in the following order:
A46,9,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A47,0,Soot entry (Diesel only)
A47,5,Soot entry (Diesel only)
A47,6,Resolution: 1 = 100 km
A47,7, 
A47,8,NOTE: Adaptation channels 40-48 must be
A47,9,entered and stored in the following order:
A47,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A48,0,Thermal load (Diesel only)
A48,5,Thermal load (Diesel only)
A48,6,Resolution: 1 = 100 km
A48,7, 
A48,8,NOTE: Adaptation channels 40-48 must be
A48,9,entered and stored in the following order:
A48,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A60,0,Powertrain CAN-Databus
A60,5,Powertrain CAN-Databus
A60,6,+0001 - Engine
A60,7,+0002 - Automatic transmission
A60,8,+0004 - Brake
A60,9,+1024 - Instrument cluster
;
A61,0,Comfort CAN-Databus
A61,5,Comfort CAN-Databus
A61,6,+00001 - Vehicle electrical system control module (ILM)
A61,7,+00002 - CCE (central comfort electric)
A61,8,+00064 - Trailer
A61,9,+00128 - Convertible top
A61,10,+00256 - Instrument cluster
A61,11,+00512 - Tire pressure control
A61,12,+01024 - Steering column module
A61,13,+02048 - Climate control
A61,14,+32768 - Auxiliary heating
;
A62,0,Infotainment CAN-Databus
A62,5,Infotainment CAN-Databus
A62,6,+01 - Radio
A62,7,+02 - Telephone
A62,8,+04 - Navigation
A62,9,+08 - Telematic
A62,10,+16 - Intrument cluster (only if 2. unit is installed)
;
