;
; VAG-COM Labelfile
;
; Audi A3 (8P) / Audi A4 (8E) / Audi A6 (4F) / VW Golf/Jetta (1K)
;
; Component: Engine (#01) - AXX/BGB/BPJ/BPY/BWA
;
; P/N: ???-9??-115-???
;
; includes measuring blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-01.LBL
; 4F-01.LBL
; 8E-01.LBL
; 8P-01.LBL
; xxx-907-115-AXX.LBL (2.0l TE  @ 200 HP - AXX/BGB/BPJ/BPY/BWA)
;
; created on 17/Apr/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 31/Jul/2005
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,1,Basic Functions
001,1,Engine Speed
001,2,Coolant,Temperature,Specification: 80...115 °C
001,3,Lambda,Regulator
001,4,Basic Setting,Requirements,see labelfile
; 1xxxxx-x - Coolant temperature below 80 °C
; x1xxxx-x - Engine speed below 2000 RPM
; xx1xxx-x - Throttle valve closed
; xxx1xx-x - Lambda regulation correct
; xxxx1x-x - State of idle
; xxxxx1-x - A/C system compressor deactivated
; xxxxxx-1 - No malfunction detected by Self-Diagnosis
;
002,0,Basic Functions
002,1,Engine Speed
002,2,Engine Load
002,3,Injection,Timing
002,4,Intake Air Mass
;
003,0,Basic Functions
003,1,Engine Speed
003,2,Intake Air Mass
003,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
003,4,Ignition,Timing Angle
;
004,1,Engine Speed
004,2,Voltage Supply,,Specification: 12.0...15.0 V
004,3,Coolant,Temperature,Specification: 80...115 °C
004,4,Intake Air,Temperature,Specification: -40.0...+140.0 °C
;
005,0,Basic Functions
005,1,Engine Speed
005,2,Engine Load
005,3,Vehicle Speed,,Specification: 0 km/h
005,4,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
;
006,0,Basic Functions
006,1,Engine Speed
006,2,Engine Load
006,3,Intake Air,Temperature,Specification: -40.0...+140.0 °C
006,4,Heights Correction,Factor
;
007,1,Engine Speed
007,2,Engine Load
007,3,Engine Coolant,Temperature,Specification: -40...+140 °C
007,4,Operating Mode
;
009,1,Engine Oil,Level
009,2,Engine Oil,Warning Barrier
009,3,Fuel Consumption,Signal
009,4,Consumption,Equivalent
;
010,0,Ignition
010,1,Engine Speed
010,2,Engine Load
010,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
010,4,Ignition,Timing Angle
;
011,1,Engine Speed
011,2,Engine Coolant,Temperature
011,3,Intake Air,Temperature,Specification: -40...+140 °C
011,4,Timing Angle,(current Value)
;
014,1,Engine Speed
014,2,Engine Load
014,3,Misfire,Sum Counter
014,4,Misfire,Recognition
;
015,0,Misfire Recognition
015,1,Cylinder 1
015,2,Cylinder 2
015,3,Cylinder 3
015,4,Malfunction,Recognition,Display Range: activated/blocked
;
016,0,Misfire Recognition
016,1,Cylinder 4
016,4,Malfunction,Recognition,Display Range: activated/blocked
;
018,1,Lower,RPM Barrier
018,2,Upper,RPM Barrier
018,3,Lower,Load Barrier
018,4,Upper,Load Barrier
;
020,0,Ignition (Knock Control - Cyl 1 - 4)
020,1,Cylinder 1 Ignition,Angle Delay
020,2,Cylinder 2 Ignition,Angle Delay
020,3,Cylinder 3 Ignition,Angle Delay
020,4,Cylinder 4 Ignition,Angle Delay
;
022,0,Ignition (Knock Control - Cyl 1 && 2)
022,1,Engine Speed
022,2,Engine Load
022,3,Cylinder 1 Ignition,Angle Delay
022,4,Cylinder 2 Ignition,Angle Delay
;
023,0,Ignition (Knock Control - Cyl 3 && 4)
023,1,Engine Speed
023,2,Engine Load
023,3,Cylinder 3 Ignition,Angle Delay
023,4,Cylinder 4 Ignition,Angle Delay
;
028,0,Knock Sensor Test (Short Trip)
028,1,Engine Speed
028,2,Engine Load
028,3,Engine Coolant,Temperature
028,4,Result,,Specification: Test ON/Test OFF/Sys. OK/Sys. not OK
;
030,0,Oxygen Sensor Status
030,1,Bank 1,Sensor 1,Specification: 111
; 1xx - Lambda sensor heating on
; x1x - Lambda sensor ready
; xx1 - Lambda regulation active
030,2,Bank 1,Sensor 2,Specification: 110
; 1xx - Lambda sensor heating on
; x1x - Lambda sensor ready
; xx1 - Lambda regulation active
;
031,0,Lambda Regulation (Contant Operation of Lambda Probes)
031,1,Lambda Sensor,Current Value
031,2,Lambda Sensor,Specified Value
;
032,0,Lambda Regulation
032,1,Lambda (Idle),Self-Adaptation
032,2,Lambda (Partial),Self-Adaptation
;
033,0,Lambda Regulation
033,1,Bank 1,Lambda Control
033,2,Bank 1 Voltage,of Oxygen Sensors
;
034,0,Lambda Regulation (befor Catalyst - Basic Setting: Aging Check)
034,1,Engine Speed
034,2,Catalytic Converter,Temperature
034,3,Period,Duration Sensor
034,4,Result,Lambda Aging,Display Range: Test ON/Test OFF/B1-S1 not OK/B1-S1 OK
;
036,1,Bank 1 Sensor 2,Sensor Voltage
036,2,Bank 1 Sensor 2,Result,Specification: Test ON/Test OFF/B1-S2 OK/B1-S2 not OK
;
037,1,Engine Load
037,2,Bank 1 Sensor 2,Voltage
037,3,Bank 1 Oxygen,Sensor Value
037,4,Result,,Specification: Test ON/Test OFF/Sys. OK/Sys. not OK
;
041,0,Lambda Regulation (Lambda Probe Heating)
041,1,Resistance,Bank 1 Sensor 1
041,2,Heater Condition,,Specification: Htg.bC.ON
041,3,Resistance,Bank 1 Sensor 2
041,4,Heater Condition,,Specification: Htg.aC.ON
;
043,0,Lambda Regulation (befor Catalyst - Basic Setting)
043,1,Engine Speed
043,2,Catalytic Converter,Temperature
043,3,Bank 1 Sensor 2,Voltage
043,4,Result,Lambda Aging,Display Range: Test ON/Test OFF/B1-S2 not OK/B1-S2 OK
;
046,0,Lambda Regulation (Basic Setting: Conversion Test)
046,1,Engine Speed
046,2,Catalytic Converter,Temperature
046,3,Amplitude,Behavior
046,4,Result Catalytic,Conversion,Pre-Catalytic Converter (Display Range: Test ON/Test OFF/CatConvB1 not OK/CatConvB1 OK)
;
050,1,Engine Speed
050,2,Engine Speed,(specified)
050,3,Condition,of A/C system,Display Range: A/C-High / A/C-Low
050,4,Operating condition,of A/C Compressor,Display Range: Compr.ON/Compr.OFF
;
051,1,Engine Speed
051,2,Specified,Engine Speed
051,3,Driving mode,,Gear 1...6 (only for automatic)
051,4,Voltage Supply,,Specification: 12.0...15.0 V
;
052,1,Engine Speed
052,2,Engine Speed,(Specified)
052,3,Condition,of A/C system,Display Range: A/C-High / A/C-Low
052,4,Window Heaters
;
053,0,Speed Regulation
053,1,Engine Speed,,Specification: 640...900 RPM
053,2,Engine Speed,(specified),Specification (manual): 670...760 RPM | Specification (automatic): 800...860 RPM
053,3,Voltage Supply,,Specification: 12.0...15.0 V
053,4,Generator Load
;
054,0,Speed Regulation
054,1,Engine Speed
054,2,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
054,3,Sender 2 for,Acc. Pedal Pos.,G79 (Display Range 0...100 %)
054,4,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
;
055,0,Speed Regulation
055,1,Engine Speed
055,2,Idle Regulator
055,3,Idle Stabilization,Self-Adaptation
055,4,Load Status,,see labelfile
; 1-xxx - Power assisted steering pressure switch on
; x-1xx - Air conditioning system switched on
; x-x1x - Heating switched on
; x-xx1 - Air conditioner compressor switched on
;
056,0,Speed Regulation
056,1,Engine Speed
056,2,Engine Speed,(specified)
056,3,Idle Regulator
056,4,Load Status,,see labelfile
; 1-xxx - Power assisted steering pressure switch on
; x-1xx - Air conditioning system switched on
; x-x1x - Heating switched on
; x-xx1 - Air conditioner compressor switched on
;
057,1,Engine Speed
057,2,Engine Speed,Specified Value
057,3,A/C Compressor
057,4,Duty Cycle,Pressure Sensor,Torque A/C Compressor
;
060,0,Speed Regulation (Basic Setting: Throttle Body Adaptation)
060,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0...100 %
060,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 100...0 %
060,3,Self-Adaptation,Steps Counter
060,4,Result,Throttle Valve Adp.,Display Range: ADP runs/ADP OK/ADP ERROR
;
061,1,Engine Speed
061,2,Voltage Supply,,Specification: 12.0...15.0 V
061,3,Activation Throttle,Position Actuator
061,4,Operating,Condition
;
062,1,Throttle Drive,Angle Sensor 1,for EPC (G187)
062,2,Throttle Drive,Angle Sensor 2,for EPC (G188)
062,3,Throttle Position,Sensor (G79)
062,4,Accelerator Pedal,Position Sensor 2,G185
;
063,0,Speed Regulation (Basic Setting: Kick-Down Adaptation)
063,1,Throttle Position,Sensor (G79),Display Range: 0...100 %
063,2,Accelerator Pedal,Position Sensor 2,G185
063,3,Kick-Down,Switch,Display Range: Kick Down
063,4,Kick-Down,Adaptation,Display Range: ADP runs/ADP OK/ADP ERROR
;
064,1,Potentiometer 1,Lower Adaptation
064,2,Potentiometer 2,Lower Adaptation
064,3,Emergency Air Gap,Potentiometer 1
064,4,Emergency Air Gap,Potentiometer 2
;
066,1,Actual,Driving Speed
066,2,Switch Positions
066,3,Specified,Driving Speed,by Cruise Control System (CCS)
066,4,Switch Positions
;
067,2,CCS Switch,Positions
;
068,1,Engine Speed
068,2,Engine Load
068,3,Driving Mode,,only for automatic transmission
068,4,Converter,Clutch Status
;
070,0,Emission Reduction (TEV - Basic Setting)
070,1,Evap. Emissions,Sol. Valve (Open),Specification: 0...100 %
070,2,Oxygen Sensor,Control Deviation
070,3,Evap. Emissions,Sol. Valve (Flow)
070,4,Result,Evap. Emissions,Display Range: Test ON/Test OFF/TEV OK/TEV not OK
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test number
;
082,0,Flash-Tool-Code (FTC)
; Flash-Date (in dd.mm.yy)
; Hardware subassembly
; Software subassambly
;
083,0,Primary Vehicle Identification Number (VIN) of first install
;
086,1,Readiness Bits
086,2,Cycle-Flags
086,3,Cycle-Flags
086,4,Cycle-Flags
;
087,1,Readiness Bits
087,2,System,Malfunction
087,3,System,Malfunction
087,4,System,Malfunction
;
088,1,System Condition
088,2,System Condition
088,3,System Condition
;
089,0,Trip Recorder
089,1,Distance travelled,with MIL active
089,2,Condition,"Tank Empty",Display Range: OK/too low
;
091,1,Engine Speed
091,2,Intake Camshaft,Duty Cycle
091,3,Camshaft,Adjustment (spec.)
091,4,Camshaft,Adjustment (act.)
;
093,1,Engine Speed
093,2,Intake Camshaft,Duty Cycle
093,3,Phase Position,Bank 1
;
094,0,Camshaft Adjustment (Basic Setting)
094,1,Bank 1 Camshaft,Adjustment,Specification: CAM-ADJ.ON | Display Range: CAM-ADJ.ON/CAM-ADJ.OFF
094,2,Bank 2 Camshaft,Adjustment,Specification: CAM-ADJ.ON | Display Range: CAM-ADJ.ON/CAM-ADJ.OFF
094,3,Diagnostic,Result,Specification: Syst. OK  | Display Range: Test OFF/Test ON/Syst.OK/Syst. nOK
;
099,0,Lambda Control Shut-Off (Basic Setting)
099,1,Engine Speed
099,2,Coolant,Temperature,Specification: 80...115 °C
099,3,Lambda Regulator,(before catalyst)
099,4,Status Lambda,Regulation,Display Range: ON/OFF
;
100,1,Readiness Bits,,see labelfile
; 1xxxxxxx - Exhaust Gas Recirculation (EGR)
; x1xxxxxx - Sensor heater
; xx1xxxxx - Oxygen sensors
; xxx1xxxx - A/C system
; xxxx1xxx - Secondary Air Injection (AIR) system
; xxxxx1xx - Activated charcoal system
; xxxxxx1x - Catalytic converter heater
; xxxxxxx1 - Catalytic converter
100,2,Coolant,Temperature
100,3,Time since,Engine Start
100,4,OBD-Status,,see labelfile
; 1-xxxxxx - MIL warning lamp on
; x-1xxxxx - Complete distance
; x-x1xxxx - At least one malfunction detected
; x-xx--1x - Heating cycle ended
; x-xx--x1 - Heating cycle not possible
;
101,1,Engine Speed
101,2,Engine Load
101,3,Median,injection timing
101,4,Intake Air Mass
;
102,1,Engine Speed
102,2,Coolant,Temperature,Specification: -40...+140 °C
102,3,Intake air,temperature
102,4,Median,injection timing
;
103,1,Current,Fuel Pressure
103,2,Fuel Pressure,Regulator
103,3,Adaptation Value,elect. Fuel Pump
103,4,Demand controlled,Fuel Pump Adapt.
;
104,1,Start Engine,Temperature
104,2,Temperature,Adaptation Factor 1
104,3,Temperature,Adaptation Factor 2
104,4,Temperature,Adaptation Factor 3
;
106,1,Fuel Rail,Pressure
106,2,Electrical,Fuel Pump 1
106,3,Electrical,Fuel Pump 2
;
107,1,Engine Speed
107,2,Lambda Controller,Bank 1 Med. Value
107,4,Result Short Trip
;
110,1,Engine Speed
110,2,Coolant,Temperature,Specification: -40...+140 °C
110,3,Median Injection,Timing
110,4,Throttle Valve Angle,(Potentiometer)
;
111,0,Charge Pressure Control
111,1,RPM Range 1
111,2,RPM Range 2
111,3,RPM Range 3
111,4,RPM Range 4
;
112,1,Exhaust Temp.,Bank 1
112,2,Enrichment Factor,Sensor Bank 1
112,3,Exhaust Temp.,Projection
112,4,Median,Exhaust Temp.
;
113,1,Engine Speed
113,2,Engine Load
113,3,Throttle Valve Angle,(Potentiometer)
113,4,Air Pressure,(Atmosphere)
;
114,0,Charge Pressure Control
114,1,Engine Load,(specified)
114,2,Engine Load,(spec. corrected)
114,3,Engine Load,(actual Value)
114,4,Wastegate (N75),Duty Cycle
;
115,0,Charge Pressure Control
115,1,Engine Speed
115,2,Engine Load
115,3,Boost Pressure,(specified)
115,4,Boost Pressure,(actual)
;
116,1,Engine Speed
116,2,Correction Factor,Fuel
116,3,Correction Factor,Coolant Temp.
116,4,Intake Air Temp.,Correction Factor
;
117,0,Charge Pressure Control
117,1,Engine Speed
117,2,Throttle Position,Sensor (G79),Display Range: 0...100 %
117,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
117,4,Boost Pressure,(specified)
;
118,0,Charge Pressure Control
118,1,Engine Speed
118,2,Intake Air,Temperature
118,3,Wastegate (N75),Duty Cycle
118,4,Boost Pressure,(actual)
;
119,0,Charge Pressure Control
119,1,Engine Speed
119,2,Charge Limit
119,3,Wastegate (N75),Duty Cycle
119,4,Boost Pressure,(actual)
;
120,0,Traction Control (TC/ASR)
120,1,Engine Speed
120,2,Engine Load,(specified)
120,3,Engine Load,(actual)
120,4,Status,,Display Range: TC active/TC n.active
;
122,0,Transmission
122,1,Engine Speed
122,2,Engine Load,(specified)
122,3,Engine Load,(actual)
122,4,Status,,Display Range: Torque red./No tor.red.
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Transmission
125,2,Brake Electronics
125,3,Instrument Cluster
125,4,A/C System
;
126,0,CAN-Databus Communication (Powertrain)
126,2,Steering Angle,Sensor (G85)
126,3,Airbag
126,4,Central,Electronics
;
127,0,CAN-Databus Communication (Powertrain)
127,1,All-Wheel-Drive
127,3,Steering Wheel,Electronics
127,4,Brake Booster
;
128,0,CAN-Databus Communication (Powertrain)
128,1,Electrical,Ignition Key
128,2,NOX-Sensor 1
128,3,NOX-Sensor 2
;
129,0,CAN-Databus Communication (Powertrain)
129,2,Oil Temperature,Sensor
129,3,CAN-Gateway
;
130,0,Mapped Cooling
130,1,Coolant temp.,engine outlet,Specification: 80...115 °C
130,2,Cooland temp.,radiator outlet,Specification: 0...100 °C
130,3,Thermostat,duty cycle,Specification: 0...100 %
130,4,Result,,Display Range: Test ON/Test OFF/Syst. OK/Syst. n.OK
;
131,0,Mapped Cooling
131,1,Coolant temp.,engine outlet,(actual) Specification: 80...115 °C
131,2,Coolant temp.,engine outlet,(specified) Specification: 0...115 °C
131,3,Cooland temp.,radiator outlet,Specification: 0...100 °C
131,4,Thermostat,duty cycle,Specification: 0...100 %
;
132,0,Mapped Cooling
132,1,Coolant,temperature,radiotor outlet
132,2,Temperature,difference,between engine and radiator outlet
132,3,Heater supply,potentiometer,Specification (w/o Climatronic): 0.2...4.8 V | Specification (with Climatronic): 0.2...5.1 V
132,4,Cooling,Status
;
134,1,Oil temperature
134,2,Ambient,temperature
134,3,Intake air,temperature
134,4,Engine output,temperature
;
135,1,Radiator output,temperature
135,2,Duty cycle cooling,fan activation 1
;
136,0,Relay for coolant actuation
136,1,Relay 1,,Specification: ON/OFF
136,2,Relay 2,,Specification: ON/OFF
136,3,Auxiliary water,pump condition
136,4,Fan after-run
;
137,0,A/C Requirements
137,1,AC-Input,,Specification: ON/OFF
137,2,Compressor,Condition,Specification: ON/OFF
137,3,High-Pressure Sw.,or A/C-Pressure
137,4,Fan desire,from A/C-System
;
138,1,Engine Start,Temperature
138,2,Mean Engine,Air Mass
138,3,Median,Vehicle Speed
138,4,Result
;
139,1,Engine Coolant,Temperature Diag.
139,2,Actual Integral,Mass Air Flow
139,3,Specified Integral,Mass Air Flow
139,4,Result
;
140,1,Quantity Valve,closing Angle
140,2,Quantity Valve,opening Angle
140,3,Rail Pressure,(actual)
140,4,Quantity Control,Valve Status
;
141,1,High pressure,system adaptation
141,2,Controller Portion
141,3,Total Compression,Volume
141,4,Rail Pressure,(actual)
;
142,1,Voltage,Upper Stop
142,2,Voltage,Lower Stop
142,3,Adaptation,Status
142,4,Adaptation,Condition
;
143,1,Engine Speed
143,2,Engine Load
143,3,Load shift flap,opening angle
143,4,Operating mode,(GDI)
;
166,1,Lambda
166,2,Sensor Voltage,behind cat. conv.
166,3,Integrated Air Mass
166,4,Result
;
167,1,Oxygen Portion
167,2,Diagnostic,Decelerator Count.
167,3,Const. Oxygen,Sens. Correction,value oxygen sensor
167,4,Result
;
