;
; VAG-COM Labelfile
;
; Audi A4 (8D) / Audi A6 (4A)
;
; Component: J234 - Airbags (#15) - AIRBAG V
;
; P/N: 8A0-959-655-???
;
; includes measuring blocks and coding
;
; created on 10/Dec/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 10/Dec/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Ignitiers I (Front Airbags && Front Belt Tensioners)
001,1,Airbag,Driver Side,1111 = Correct\n1011 = Signal too Low\n0111 = Signal too High\n1101 = Short to Ground\n1110 = Short to Plus
001,2,Airbag,Passenger Side,1111 = Correct\n1011 = Signal too Low\n0111 = Signal too High\n1101 = Short to Ground\n1110 = Short to Plus
001,3,Belt Tensioner,Front Driver Side,1111 = Correct\n1011 = Signal too Low\n0111 = Signal too High\n1101 = Short to Ground\n1110 = Short to Plus
001,4,Belt Tensioner,Front Pass. Side,1111 = Correct\n1011 = Signal too Low\n0111 = Signal too High\n1101 = Short to Ground\n1110 = Short to Plus
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Airbags (J234) Coding
C01,00766 = Driver Airbag & Belt Tensioners
C02,01022 = Driver/Passenger Airbag & Belt Tensioners
;
