;
; VAG-COM label file
;
; VW Touareg (7L)
;
; component: instrument cluster (#17)
;
; tested with p/n: 7L6 920 980 D
;
; includes coding, adaptation & measuring blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 7L-17.LBL
; 7L6-920-xxx-17.LBL
;
; by Sebastian Stange
; sebastian@ross-tech.com
;
; last modification: 12/13/2004
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; measuaring block informations
;
;---------------------------------------------------
;
;
001,0,Common Informations
001,1,Vehicle Speed,,via CAN from brake control module
001,2,Engine Speed,,via CAN from transmission control module
001,3,Oil Pressure,,Specified Value: Oilpr.2 i.O.
001,4,Clock
;
002,0,Common Informations
002,1,Mileage
002,2,Fuel Tank Content
002,3,[N/A]
002,4,Ambient,Temperature,Display Range: -45...+65 °C | +70 °C = short circuit | -50 °C = open circuit
;
003,0,Coolant && Oil Temperature
003,1,Coolant,Temperature,via CAN from engine control module
003,2,Oil Level
003,3,Oil Temperature
;
004,1,Battery Voltage
;
005,1,Fuel Gauge
005,2,Fuel Supply,Sensor 3
;
006,1,Tank Content,(Main Chamber)
006,2,Tank Content,(Side Chamber)
;
050,0,Common Informations
050,1,Mileage
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
060,0,Installation Information (Senders && Sensors)
;
061,0,Checking Installation Information
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
082,0,Flash-Tool-Code (FTC)
; Flash-Date (in dd.mm.yy)
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine
125,2,Transmission
125,3,ABS
;
126,0,CAN-Databus Communication (Powertrain)
126,2,Airbag
;
127,0,CAN-Databus Communication (Powertrain)
127,2,All wheel,drive (AWD)
;
128,0,CAN-Databus Communication (Powertrain)
128,2,Electrical Ignition
128,3,Level Control
;
130,0,CAN-Databus Communication (Comfort)
130,1,Comfort-CAN,Condition
130,2,Comfortsystem
130,3,Driver Door
130,4,Passenger Door
;
131,0,CAN-Databus Communication (Comfort)
131,1,Rear/Left Door
131,2,Rear/Right Door
131,3,Driver,Memory Seat
131,4,Electrical System
;
132,0,CAN-Databus Communication (Comfort)
132,2,Steering Wheel
132,3,Climate
132,4,Tire Pressure
;
133,0,CAN-Databus Communication (Comfort)
133,2,Passenger,Memory Seat
133,4,Parking Aid
;
134,0,CAN-Databus Communication (Comfort)
134,2,Electrical Ignition
;
140,0,CAN-Databus Communication (Infotainment)
140,1,Infotainment-CAN,Condition
140,3,Radio/Navigation
140,4,Telephone
;
141,0,CAN-Databus Communication (Infotainment)
141,3,TV-Tuner
;
143,0,CAN-Databus Communication (Infotainment)
143,1,Digital,Sound Package
143,3,Parking Heater
143,4,Roof Electronics
;
201,1,K-Value
201,2,Wheel,Circumference
201,3,Starting impulse,recognized
;
202,1,Engine Hood,Switch
;
;
;---------------------------------------------------
;
; coding informations
;
;---------------------------------------------------
;
;
C00,Touareg (7L) - Instrument Cluster Coding
C01, ??xxx - additional equipment
C02,+01 - break pad wear indicator
C03,+02 - seat belt warning
C04,+04 - windshield washer fluid warning
C05,Coding of this options is the sum of the individual options
C06,xx?xx - Country version
C07,1 - Europe (EU)
C08,2 - USA (US)
C09,3 - Canada (CDN)
C10,4 - Great Britain (GB)
C11,5 - Japan (JP)
C12,6 - Saudi Arabia (SA)
C13,7 - Australia (AUS)
C14,xxx?x: Service interval extension
C15,1 - SIE with flexible intervals (QG1)
C16,2 - SIE with fixed intervals (QG2)
C17,3 - no service intervals (USA/Canada)
C18,xxxx? - Engine/Transmission
C19,1 - Standard
;
;
;---------------------------------------------------
;
; adaptation informations
;
;---------------------------------------------------
;
;
A04,0,Language selection
A04,5,Possible selections:
A04,6,1 - German
A04,7,2 - English
A04,8,3 - French
A04,9,4 - Italian
A04,10,5 - Spanish
A04,11,6 - Portuguese
A04,12,7 - without text (symbols)
A04,13,8 - Czech
A04,14, 
A04,15,NOTE: not all values might be possible.
;
A09,0,Mileage
A09,5,Mileage shown in instrument cluster
A09,6,Mileage can only be changed once until it
A09,7,is not over 100 km/mi. On some instrument
A09,8,clusters you do not need any login/security
A09,9,code to change the value.
;
A30,0,Tank sensor
A30,5,Tank sensor
A30,6,Tank sensor can be adjusted by
A30,7,steps of 1 from 108 to 148.
;
A35,0,Undocumented
;
A60,0,Undocumented (DATA-BUS Engine)
;35951
;
A61,0,Undocumented (DATA-BUS Comfort)
;447
;
A62,0,Undocumented (DATA-BUS Infotainment)
;28752 = 111000001010000
;
