;
; VAG-COM label file
;
; Audi A4 (8E/8H) / Audi A6 (4B) / Audi A8 (4D)
; Skoda Superb (3U / VW Passat (3B)
;
; component: J431 - Headlight Aim Control (#55)
;
; p/n: 4B0 907 357 A/B/C
;      4Z7 907 357
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4B-55.LBL
; 4Z-55.LBL
; 4B0-907-357-AUT.LBL
; 4B0-907-357-DYN.LBL
;
; created on 27/Sep/2004 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 02/Jun/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,0,Basic Setting: Adjustment Position
001,1,Voltage Supply,(Terminal 15),Specifcation: 0.0...15.0 V
001,2,Light Switch,,Specification:\n0 = Light OFF\n1 = Light ON
001,3,Vehicle Speed,,Specification: 0...300 km/h
001,4,Acceleration,,Specification: 0.00...7.00 m/sē
;
002,0,Basic Setting: Adjustment Position learning
002,1,Voltage front,level sensor (G78),Specification: 1.56...3.45 V\n0.00 V = level sensor faulty\n5.00 V = wiring faulty
002,2,Voltage rear,level sensor G76),Specification: 0.50...4.50 V\n0.00 V = level sensor faulty\n5.00 V = wiring faulty
002,3,Specification,actuator motors,Specification: 0...100 %
002,4,Time constant,,Specification: 0...2 s
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,Head Light Aim Control (J431) Coding
C1,00001 - Audi A8 (4D)
C2,00005 - Skoda Superb (3U) FWD
C3,00006 - Skoda Superb (3U) AWD
C4,00007 - VW Passat (3B) FWD
C5,00008 - VW Passat (3B) AWD
C6,00020 - Audi A6/S6 (4B) (through MY 2000)
C7,00030 - Audi Allroad (4H)
C8,00040 - Audi A6 (4B) FWD (from MY 2001)
C9,00050 - Audi A6 (4B) AWD (from MY 2001)
C10,00060 - Audi A4 (8E)
C11,00070 - Audi Cabrio/Coupe (8E/8H)
;
