;
; VAG-COM Labelfile
;
; Audi A4 (8EC/8ED)
;
; Component: J104 - Brake Electronics (#03) - Bosch 8.0
;
; P/N: 8E0-910-517-???
;
; includes measuring blocks and coding
;
; created on 05/Sep/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 26/Oct/2005
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left,Display Range: 0.0...255.0 km/h
001,2,Wheel Speed,Front Right,Display Range: 0.0...255.0 km/h
001,3,Wheel Speed,Rear Left,Display Range: 0.0...255.0 km/h
001,4,Wheel Speed,Rear Right,Display Range: 0.0...255.0 km/h
;
002,1,Brake Test Switch,,0 = not operated\n1= operated
002,2,Brake Light Switch,,0 = not operated\n1= operated
002,3,Parking Brake,,0 = not operated\n1= operated
002,4,ESP-Button,,0 = not operated\n1= operated
;
003,0,Engine Data
003,1,Engine Speed
003,2,Engine Torque
003,3,Engine Torque,(loss)
003,4,Throttle Valve Angle
;
004,1,Standing Time
004,2,EDL-T Flag,,Display Range: ON/OFF\nSpecification: OFF
;
005,1,Steering Angle,,Display Range: -720.0...+720.0 °\nTolerance (when straight): ±5.0 °
005,2,Rotation Rate,,Display Range: -69.0...+69.0 °/s
005,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n40.0 bar = Short to Ground\n290.0 bar = Short to Plus
005,4,Transverse,Acceleration,Display Range: -25.0...+25.0 m/s²
;
006,1,Supply Voltage,(Terminal 30),Specification: 9.8...17.4 V
006,2,Valve Relay,,Display Range: ON = OK / OFF = not OK
006,3,Return Flow Pump,,Display Range: ON/OFF
006,4,Work Shop Code
;
009,1,Brake Test Switch,,0 = not operated\n1= operated
009,2,Brake Light Switch,,0 = not operated\n1= operated
009,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n40.0 bar = Short to Ground\n290.0 bar = Short to Plus
;
021,0,ESP Sensor Unit (G419) Data
021,4,HW/SW Number
;
022,0,Steering Angle Sensor Data
;
023,0,Data Variant Coding
023,1,Data Variant,Coding
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Steering Angle,Sensor,Specification: Steer. ang. 1
125,2,Engine,,Specification: Engine 1
125,3,Transmission,,Specification: Transm. 1
125,4,Instrument Cluster,,Specification: Instruments 1
;
126,0,CAN-Databus Communication (Powertrain)
126,4,ESP Sensors,,Specification: ESP Sens. 1
;
127,0,CAN-Databus Communication (Powertrain)
127,2,Airbag,,Specification: Airbag 1
;
225,0,CAN-Databus Time-Out (Powertrain)
225,1,Steering Angle,Sensor
225,2,Engine
225,3,Transmission
225,4,Instrument Cluster
;
226,0,CAN-Databus Time-Out (Powertrain)
226,4,ESP Sensors
;
227,0,CAN-Databus Time-Out (Powertrain)
227,2,Airbag
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Brake Electronics - Bosch 8.0 (J104) Coding
C01,If necessary request a specific coding directly from us:
C02,http://www.ross-tech.com/contact.html
;
