;
; VAG-COM Labelfile
;
; VW Passat (3C)
;
; Component: J527 - Steering Wheel Electronics (#16)
;
; P/N: 3C0-953-549-???
;
; includes measuring blocks and coding
;
; created on 29/Oct/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 17/Dec/2005
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,1,Blinker,,Display Range: Not Oper./Left/Right
001,2,Headlamp Flasher,,Display Range: Not Oper./Operated
001,3,High Beam,,Display Range: Not Oper./Operated
001,4,Front Wiper,,Display Range: Not Oper./Level/Stage Int./Stage 1/Stage 2
;
002,0,Wiper && Washer
002,1,Interval Stages,,Display Range: Stage 1/Stage 2/Stage 3/Stage 4
002,2,Wash Front,,Display Range: Not Oper./Operated
002,3,Wiping Rear,,Display Range: Not Oper./Operated/Not Installed
002,4,Washing Rear,,Display Range: Not Oper./Operated/Not Installed
;
003,1,Terminal Status
; ?xxxx = P-Contact
; x?xxx = S-Contact
; xx?xx = Terminal 75
; xxx?x = Terminal 15
; xxxx? = Terminal 50
003,2,Horn,,Display Range: Not Oper./Operated
003,3,Board Computer,,Display Range: Not Installed/Not Oper./Operated/Switch Reset/Switch UP/Switch DN/Switch Off
;
004,0,Cruise Control System (CCS) / Adaptive Cruise Control (ACC)
004,1,Main Switch,,Display Range: ON/OFF
004,2,CCS/ACC-Set,,Display Range: Not Oper./Operated/Accel/Delay/Stored Off
004,3,CCS/ACC-Status,,Display Range: Not Oper./Operated/Accel/Delay/Stored Off
;
005,1,Selector Lever,P Lock Switch
005,2,Selector Lever,P Position (CAN)
005,3,CCS Soleniod,,Display Range: ON/OFF
005,4,Ignition Key,Removal Lock
;
006,0,Multifunction Steering Wheel I
006,1,Communication,,Display Range: Not Installed/OK/not OK
006,2,Software Version
006,3,Hardware Version
006,4,Malfunction,recognized,Display Range: Yes/No
;
007,0,Multifunction Steering Wheel II
007,1,Vehicle Type
007,2,Vehicle Version
;
008,0,Multifunction Steering Wheel III
008,1,Thumb Wheel,(Left),Display Range: Not Installed/Not Oper.
008,2,Thumb Wheel,(Right),Display Range: Not Installed/Not Oper.
008,3,Tiptronic,(Down),Display Range: Not Installed/Not Oper./Operated
008,4,Tiptronic,(Up),Display Range: Not Installed/Not Oper./Operated
;
009,0,Multifunction Steering Wheel IV
009,1,Steering Wheel,Buttons
;
010,0,Heated Steering Wheel && Heated Seats
010,1,Steering Wheel,Heater,Display Range: Not Installed/OFF/ON\nSignal Type: Output
010,2,Temperature,,Display Range: Not Installed/Temperature\nSignal Type: Input
010,3,Steering Wheel,Heater Output,Signal Type: Output
010,4,Heated Seats,,Display Range: OFF/Stage\nSignal Type: Input
;
011,0,Dimming
011,1,Dimming,,Display Range: 0.0...100.0 %\nSignal Type: Input
011,2,Dimming,(Discrete),Display Range: 0.0...100.0 %\nSignal Type: Input
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Steering Wheel Electronics (J527) Coding
C01,?xxxxxx: Voice Operation (Symbols)
C02,0 - No Voice Operation (Standard Symbols) / 1 - Voice Operation (Modified Symbols)
C03,x?xxxxx: Country (Parking Light) / 0 - Rest of World (with Parking Light)
C04,1 - North America (without Parking Light)
C05,xx?xxxx: Vehicle Type
C06,0 - Normal Vehicle / 1 - Special Purpose Vehicle (e.g. Taxi)
C07,xxx?xxx: Transmission
C08,0 - Manual Transmission / 1 - Automatic Transmission
C09,xxxx?xx: Steering Wheel/Tiptronic
C10,0 - without Multi-Function Steering Wheel
C11,1 - with Multi-Function Steering Wheel / without Tiptronic
C12,2 - with Multi-Function Steering Wheel / with Tiptronic
C13,xxxxx?x: Cruise Control
C14,0 - wiithout Cruise Control System / 1 - with 6 Position Cruise Control System
C15,2 - with 6 Position Cruise Control System and Distance Regulation
C16,xxxxxx?: Rear Wiper/Board Computer
C17,1 - without Rear Wiper (Sedan) / without Board Computer
C18,2 - with Rear Wiper (Wagon) / without Board Computer
C19,3 - without Rear Wiper (Sedan) / with Board Computer
C20,4 - with Rear Wiper (Wagon) / with Board Computer
;
