;
; VAG-COM label file
;
; Audi A4 (8EC/8ED)
;
; component: J234 - Airbag 9.41 (#15)
;
; p/n: 8E0-959-655-???
;
; includes measuring blocks and adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8E-15.LBL
; 8E0-959-655-8E2.LBL (8E2/8E5: pre-facelift)
; 8E0-959-655-8EC.LBL (8EC/8ED: facelift)
;
; created on 25/Aug/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 24/Oct/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Igniter Status (Airbag && Tensioner)
001,1,Driver Airbag,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Passenger Airbag,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Driver Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Passenger Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
002,0,Igniter Status (Tensioner && Battery Disconnect)
002,1,Rear Left Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Rear Right Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,3,Rear Center Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,4,Battery Disconnect,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,1,Voltage supply,,Display Range: Correct/Signal too Low/Signal too High
003,2,Seat Occupation,Detection Passenger,Display Range: Child Seat/Light Adult/Medium Adult/Heavy Adult/Not Occup./Short to Ground/Short to Plus/Not Installed
003,3,Belt Inquiry,Driver,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Passenger,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry (Rear)
004,1,Belt Inquiry,Rear Left,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Right,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,3,Belt Inquiry,Rear Center,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
005,0,Igniter Status (Side Airbag)
005,1,Front Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,2,Front Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,3,Rear Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,4,Rear Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
007,0,Igniter Status (Head Airbag)
007,1,Driver Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
007,2,Passenger Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
010,0,Key Switch Status
010,1,Key Switch,Passenger Airbag,Display Range: ON/OFF
010,2,Key Switch,(HW Path),Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
010,3,Key Switch,(SW Path),Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
011,0,Igniter Status (Airbag Stage 2 && Knee Airbag)
011,1,Driver Airbag,Igniter (Stage 2),Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,2,Passenger Airbag,Igniter (Stage 2),Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,3,Driver Knee,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,4,Passenger Knee,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
016,0,Seat Occupied Recognition Control Module (J706) I
016,1,Serial Number,(1/2)
016,2,Serial Number,(3/4)
016,3,Serial Number,(5)
016,4,Calibration Status
;
018,0,Seat Occupied Recognition Control Module (J706) II
018,1,Pressure Sensor
018,2,Belt Force Sensor
018,3,Acceleration,Sensor
;
019,0,Seat Occupied Recognition Control Module (J706) III
019,1,Workshop Code,(Last Coding)
019,2,Workshop Code,(Last 0-Balance)
;
020,0,Battery Separating Relay (J655)
;
021,0,Igniter Resistance (Airbag && Tensioner)
021,1,Driver Airbag,Igniter,Specification: 2.1...5.6 Ohm
021,2,Passenger Airbag,Igniter,Specification: 1.6...5.6 Ohm
021,3,Driver Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
021,4,Passenger Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
;
022,0,Igniter Resistance (Tensioner && Battery)
022,1,Rear Left Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,2,Rear Right Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,3,Rear Center Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,4,Battery Disconnect,Igniter,Specification: 1.6...5.6 Ohm
;
025,0,Igniter Resistance (Side Airbag)
025,1,Front Left Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,2,Front Right Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,3,Rear Left Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,4,Rear Right Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
027,0,Igniter Resistance (Head Airbag)
027,1,Driver Head,Airbag Igniter,Specification: 1.6...5.6 Ohm
027,2,Passenger Head,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
031,0,Igniter Resistance (Airbag Stage 2 && Knee Airbag)
031,1,Driver Airbag,Igniter (Stage 2),Specification: 2.1...5.6 Ohm
031,2,Passenger Airbag,Igniter (Stage 2),Specification: 1.6...5.6 Ohm
031,3,Driver Knee,Airbag Igniter,Specification: 1.6...5.6 Ohm
031,4,Passenger Knee,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Identification Number (VIN)
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Instrument Cluster,,Specification: Instruments 1
125,2,Brake Electronics,,Specification: ABS 1
125,3,Immobilizer,,Specification: Immobilizer 1
;
225,0,CAN-Databus Time-Out (Powertrain)
225,1,Instrument Cluster
225,2,Brake Electronics
225,3,Immobilizer
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Airbag 9.41 (J234) Coding
C01,0?3xxxx: Battery Seperating
C02,0 - without Battery Seperating / 4 - with Battery Seperating (4.2l V8 only / PR-TK7)
C03,0x3?xxx: Options
C04,0 - with/without Belt Warning (PR-4UE+9P0/9P1)
C05,1 - Passenger Airbag with Key Switch / Belt Warning (PR-4UE+9P0/9P1)
C06,2 - Passenger Airbag with Seat Occupation Detection / Belt Warning (PR-4UB+9P5)
C07,3 - with Belt Warning (PR-4UE+9P3) OR Passenger Airbag with Seat Occupation Detection / Belt Warning (PR-4UB+9P3)
C08,4 - Passenger Airbag with Key Switch / Belt Warning (PR-4UF+9P3)
C09,0x3x?xx: Side Airbags
C10,6 - Front Side Airbags with Head Airbags (PR-4X3)
C11,7 - Front & Rear Side Airbags with Head Airbags (PR-4X4)
C12,0x3xx?x: Belt Inquiry
C13,0 - North America (USA/Canada) OR Rest of World (RoW): without Belt Inquiry (PR-9P0)
C14,1 - Rest of World (RoW): Belt Inquiry Driver's Side (PR-9P1)
C15,2 - Rest of World (RoW): Belt Inquiry Driver's & Passenger Side (PR-9P3)
C16,0x3xxx?: Belt Tensioner
C17,2 - Rest of World (RoW): Front Belt Tensioner
C18,2 - Rest of World (RoW) & Belt Inquiry (PR-9P1): Front & Rear Belt Tensioner
C19,7 - Rest of World (RoW) & Belt Inquiry (PR-9P0/9P3): Front & Rear Belt Tensioner
C20,7 - North America (USA/Canada)
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A001,0,Front Passenger Airbag Deactivation
A001,1,Front Passenger,Airbag
A001,2,Current Status
A001,5,Front Passenger Airbag Deactivation
A001,6,0 - Airbag Enabled
A001,7,1 - Airbag Disabled
A001,8, 
A001,9,Note: Refer to Service Manual!
;
A002,0,Front Driver Airbag Deactivation
A002,1,Front Driver,Airbag
A002,2,Current Status
A002,5,Front Driver Airbag Deactivation
A002,6,0 - Airbag Enabled
A002,7,1 - Airbag Disabled
A002,8, 
A002,9,Note: Refer to Service Manual!
;
A003,0,Front Passenger Side Airbag Deactivation
A003,1,Front Passenger,Side Airbag
A003,2,Current Status
A003,5,Front Passenger Side Airbag Deactivation
A003,6,0 - Airbag Enabled
A003,7,1 - Airbag Disabled
A003,8, 
A003,9,Note: Refer to Service Manual!
;
A004,0,Front Driver Side Airbag Deactivation
A004,1,Front Driver,Side Airbag
A004,2,Current Status
A004,5,Front Driver Side Airbag Deactivation
A004,6,0 - Airbag Enabled
A004,7,1 - Airbag Disabled
A004,8, 
A004,9,Note: Refer to Service Manual!
;
A005,0,Front Passenger Belt Tensioner Deactivation
A005,1,Front Passenger,Belt Tensioner
A005,2,Current Status
A005,5,Front Passenger Belt Tensioner Deactivation
A005,6,0 - Belt Tensioner Enabled
A005,7,1 - Belt Tensioner Disabled
A005,8, 
A005,9,Note: Refer to Service Manual!
;
A006,0,Front Driver Belt Tensioner Deactivation
A006,1,Front Driver,Belt Tensioner
A006,2,Current Status
A006,5,Front Driver Belt Tensioner Deactivation
A006,6,0 - Belt Tensioner Enabled
A006,7,1 - Belt Tensioner Disabled
A006,8, 
A006,9,Note: Refer to Service Manual!
;
A007,0,Front Passenger Head Airbag Deactivation
A007,1,Front Passenger,Head Airbag
A007,2,Current Status
A007,5,Front Passenger Head Airbag Deactivation
A007,6,0 - Airbag Enabled
A007,7,1 - Airbag Disabled
A007,8, 
A007,9,Note: Refer to Service Manual!
;
A008,0,Front Driver Head Airbag Deactivation
A008,1,Front Driver,Head Airbag
A008,2,Current Status
A008,5,Front Driver Head Airbag Deactivation
A008,6,0 - Airbag Enabled
A008,7,1 - Airbag Disabled
A008,8, 
A008,9,Note: Refer to Service Manual!
;
A011,0,Rear Passenger Belt Tensioner Deactivation
A011,1,Rear Passenger,Belt Tensioner
A011,2,Current Status
A011,5,Rear Passenger Belt Tensioner Deactivation
A011,6,0 - Belt Tensioner Enabled
A011,7,1 - Belt Tensioner Disabled
A011,8, 
A011,9,Note: Refer to Service Manual!
;
A012,0,Rear Driver Belt Tensioner Deactivation
A012,1,Rear Driver,Belt Tensioner
A012,2,Current Status
A012,5,Rear Driver Belt Tensioner Deactivation
A012,6,0 - Belt Tensioner Enabled
A012,7,1 - Belt Tensioner Disabled
A012,8, 
A012,9,Note: Refer to Service Manual!
;
A050,0,ESP-Data (Powertrain)
A050,1,Powertrain
A050,5,ESP-Data (Powertrain)
A050,6,1 - Front-Wheel-Drive (FWD)
A050,7,2 - All--Wheel-Drive (AWD)
;
A051,0,ESP-Data (Brake)
A051,1,Brake
A051,5,ESP-Data (Brake)
A051,6,02 - Front: C54 / Rear: C38 (PR-1LZ+1KD)
A051,7,04 - Front: FN3 15" / Rear: C38 (PR-1LB/1LE+1KD)
A051,8,06 - Front: FN3 16" / Rear: C38 (PR-1LT/1LF+1KP)
A051,9,12 - Front: FNR G60 16" / Rear: CII 41 (PR-1LA/1LC/1LD-1KW)
A051,10,14 - Front: FNR G60 17" / Rear: CII 43 (PR-1LJ+1KE)
A051,11,20 - Front: Brembo M6 19" / Rear: CII 43 (PR-1LU+1KY)
A051,12,22 - Front: Brembo M8 18" / Rear: CII 43 (PR-1LP+1KY or PR-1LV+2EG)
;
A081,0,Learned Values (Vehicle Data)
A081,5,Learned Values (Vehicle Data)
A081,6,To start the process for vehicle data (VIN)
A081,7,learning enter/save 02905 as new value.
;
