;
; VAG-COM label file
;
; Audi A3 (8L) / Audi A4 (8D) / Audi A6 (4B)
;
; component: J347 - Interior Monitoring (#45)
;
; p/n: 4B0-951-173
;
; includes measuring blocks, adaptation and coding
;
; created on 07/Jun/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 07/Jun/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; Measuring block informations
;
;---------------------------------------------------
;
;
;
001,0,Basic Functions
001,1,Switch,Positions,?xxx - Switch for Int. Monitoring\nx?xx - Driver-side door contact switch\nxx?x - Anti-theft warning system\nxxx? - Glass breakage system (Avant only)
001,2,Sensor,Sensitivity,Specification: 50...100 % (see Adaptation Channel 001)
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,Interior Monitoring (J247) Coding
C1,00?xx - Type
C2,0 - Audi A3 (8L)
C3,1 - Audi A4 (8D) / Audi A6 (4B)
C4, 
C5,00x?x - Arming Mode
C6,0 - Static
C7, 
C8,00xx? - Chassis Type
C9,1 - Sedan
C10,2 - Avant
;
;
;---------------------------------------------------
;
; Adaptation informations
;
;---------------------------------------------------
;
;
A1,0,Sensitivity
A1,5,Sensitivity
A1,6,Sensitivity settings of the ultra-sound sensors can
A1,7,be set so that the sensors react with less sensitivity
A1,8, 
A1,9,Basic value: 100 (= 100 %)
A1,10,Specification: 50...100 %
;
