;
; VAG-COM Labelfile
;
; Audi A4 (8E)
;
; Component: J527 - Steering Wheel Electronics (#16)
;
; P/N: 8E0-953-549-???
;
; includes measuring blocks, coding and adaptation
;
; created on 26/Sep/2004 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 06/Oct/2005
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,1,Ignition,switch,Display range: 12345 (1=P-contact/2=S-contact/3=term. 75/4=term. 15/5=term. 50)
001,2,Signal light,,Display range: not activated/left/right
001,3,Light horn,,Display range: not activated/activated
001,4,High beam,,Display range: not activated/activated
;
002,1,Horn,,Display range: not activated/activated
002,2,Wiping front,,Display range: not activated/interval step 1/step 1/step 2
002,3,Interval,steps,Display range: step 1/step 2/step 3/step 4
002,4,Washing,front,Display range: not activated/activated
;
003,1,Wiping rear,,Display range: not installed/not activated/activated
003,2,Washing rear,,Display range: not installed/not activated/activated
003,3,Board computer,,Display range: not installed/button reset/button on/button down
003,4,[N/A]
;
004,0,Cruise control switch
004,1,Cruise control,,Display range: on/off
004,2,Cruise control,-SET-,Display range: not activated/activated
004,3,Cruise control,,Display range: not activated/accelerating/decelerating/stored Off/Resume
004,4,[N/A]
;
005,0,Steering wheel (M-equipment)
005,1,Tip down,,Display range: not installed/not activated/activated
005,2,Tip up,,Display range: not installed/not activated/activated
005,3,Steering wheel,heater,Display range: not installed/on/off
005,4,Sensor,[°C],127 = open circuit / 248 = not installed
;
006,0,Multi-function steering wheel
006,1,Communication,,Display range: OK/not OK
006,2,Electronic,version
006,3,Malfunction,recognized?,Display range: yes/no
006,4,[N/A]
;
007,0,Multi-function buttons
007,1,Button 1,,Display range: not activated/activated
007,2,Button 2,,Display range: not activated/activated
007,3,Button 3,,Display range: not activated/activated
007,4,Button 4,,Display range: not activated/activated
;
008,0,Multi-function buttons
008,1,Button 5,,Display range: not activated/activated
008,2,Button 6,,Display range: not activated/activated
008,3,[N/A]
008,4,[N/A]
;
009,0,Inputs via Comfort CAN-bus
009,1,Diming,,Display range: diming value
009,2,Right hand,steering,Display range: yes/no
009,3,Left,heated seat,Display range: off/step
009,4,Right,heated seat,Display range: off/step
;
010,0,Inputs via Comfort CAN-bus
010,1,M-path,Tiptronic,Display range: not activated/activated
010,2,[N/A]
010,3,[N/A]
010,4,[N/A]
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test number
;
125,0,CAN-Databus communication (Comfort)
125,1,Instrument,cluster
125,2,Central comfort,electric
125,3,Climate control
125,4,[N/A]
;
126,0,CAN-Databus communication (Comfort) - Door control modules
126,1,driver,side
126,2,passenger,side
126,3,rear,left,only with electrical power windows
126,4,rear,right,only with electrical power windows
;
127,0,CAN-Databus communication (Comfort)
127,1,Radio
127,2,Telephone
127,3,Voice activation,input
127,4,[N/A]
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Steering Wheel Electronics (J527) Coding
C1,0?xxx - Steering wheel type
C2,0 - Standard steering wheel (4-spoke without multi-function)
C3,1 - 3-spoke steering wheel (sport steering wheel)
C4,2 - Multi-function steering wheel with radio control
C5,3 - Multi-function steering wheel with radio/telephone control
C6,4 - Multi-function steering wheel with radio/telephone/speech operating system control
C7, 
C8,0x?xx - Additional equipment
C9,+1 - Tiptronic
C10,+2 - Steering wheel heating (not for 3-spoke steering wheel)
C11, 
C12,0xx?x - Board computer / Cruise control
C13,0 - No board computer / no cruise control
C14,1 - Board computer
C15,2 - Cruise control system
C16,4 - Board computer and cruise control system
C17, 
C18,0xxx? - Chassis type (rear wiper)
C19,1 - Sedan, Cabriolet
C20,2 - Avant, Coupe (rear wiper)
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A081,0,Learned Values (Vehicle Data)
A081,5,Learned Values (Vehicle Data)
A081,6,To start the process for vehicle data (VIN)
A081,7,learning enter/save 00111 as new value.
;
