;
; VAG-COM Labelfile
;
; Seat Ibiza (6K)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 6K0-920-???-???
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 6K-17.LBL
; 6K0-920-xxx.LBL
;
; created on 27/Nov/2005 by Jose Carlos Fernandez (josecarlosfernandez@terra.es)
; updated on 08/Dec/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2 (< min)
001,4,Time
;
002,0,General
002,1,Mileage
002,2,Fuel Level
002,3,Fuel Sender,Resistance
;
003,0,General
003,1,Coolant,Temperature
;
020,0,Immobilizer - ID Block 1
020,1,Digit 1 && 2
020,2,Digit 3 && 4
020,3,Digit 5 && 6
020,4,Digit 7 && 8
;
021,0,Immobilizer - ID Block 2
021,1,Digit 9 && 10
021,2,Digit 11 && 12
021,3,Digit 13 && 14
;
022,0,Immobilizer I
022,1,Engine Start,permitted,Specification: 1 = Yes\nDisplay Range: 0 = No / 1 = Yes
022,2,Engine (ECU),responds,Specification: 1 = Yes\nDisplay Range: 0 = No / 1 = Yes
022,3,Key Status,,Specification: 1 = Key OK\nDisplay Range: 0 = Key not OK / 1 = Key OK
022,4,Number of,adapted Keys,Specification: 1...4
;
023,0,Immobilizer II
023,1,Variable Code,authorized,Specification: 1 = Yes\nDisplay Range: 0 = No / 1 = Yes
023,2,Key Status,(Transponder),Display Range: 0 = not locked / 1 = locked
023,3,Fixed Code,authorized,Specification: 1 = Yes\nDisplay Range: 0 = No / 1 = Yes
023,4,Immobilizer,Status,See Labelfile
; 4 - New Customer Service / Delivery Condition (Replacement Instrument Cluster)
; 5 - Customer Service locked / Adaptation Data Programmed in Customer Service
; 6 - Immobilizer adapted / Normal Function Condition
; 7 - Key Adaptation active
;
050,0,General
050,1,Mileage
050,2,Engine Speed
050,4,Coolant,Temperature
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A003,0,Fuel Consumption
A003,5,Fuel Consumption
A003,6,Standard Value: 100
A003,7,Value Range: 85 - 115
A003,8,Increments: 1 % (percent)
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km/62 mi.
;
A016,0,Distance Impulse Number
;
A021,0,Immobilizer - Key Adaptation
A021,5,Immobilizer - Key Adaptation
;
A030,0,Tank Characteristic
A030,5,Tank Characteristic
A030,6,Parallel shift of tank characteristic by ± 6 °
A030,7,Standard Value: 128
A030,8,Value Range: 120...136
A030,9,Increments: 1 = 0.5 °
A030,8, 
A030,9,Adaptation should be performed after emptying the tank
A030,10,and filling it with 7 liters of fuel.
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Resolution: 1 = 100 km
A040,7, 
A040,8,NOTE: Adaptation channels 40-44 must be
A040,9,entered and stored in the following order:
A040,10,43 > 44 > 40 > 41
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Resolution: 1 = 1 day(s)
A041,7, 
A041,8,NOTE: Adaptation channels 40-44 must be
A041,9,entered and stored in the following order:
A041,10,43 > 44 > 40 > 41
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Resolution: 1 = 1000 km
A043,7, 
A043,8,NOTE: Adaptation channels 40-44 must be
A043,9,entered and stored in the following order:
A043,10,43 > 44 > 40 > 41
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Resolution: 1 = 1 day(s)
A044,7, 
A044,8,NOTE: Adaptation channels 40-44 must be
A044,9,entered and stored in the following order:
A044,10,43 > 44 > 40 > 41
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C00,Instruments Cluster (J285) Coding
C01,??xxx: Optional Equipment
C02,+00 - No optional equipment active
C03,+01 - Brake pad wear indicator, active
C04,+02 - Seat belt warning, active
C05,+04 - Washer water warning activated
C06, 
C07,??xxx: Code number for country variants
C08,0 - Germany (D)        \ 1 - Europe (EU)
C09,2 - USA (US)           \ 3 - Canada (CAN)
C10,4 - Great Britain (GB) \ 5 - Japan (JP)
C11,6 - Saudi Arabia (SA)  \ 7 - Australia (AUS)
C12, 
C13,xxx?x: Code number for number of cylinder
C14,4 - 4 cylinders / 5 - 5 cylinders / 6 - 6 cylinders
C15, 
C16,xxxx?: Code for distance progress (code K)
C17,1 - 3775 / 2 - 3833 / 3 - 3875 / 6 - 4492
C18,(See label file for more information)
;
;1 - 3775 (1.0l ALD/ANV/AFR/AST with transmission)
;1 - 3775 (1.4l AKK/ANW/AUD/APE/AUA/AQQ/AUB with transmission)
;1 - 3775 (1.6l ALM with transmission)
;2 - 3833 (1.6l AEH/AKL/APF/AUR with autom. Transmission)
;2 - 3833 (1.8l AQX with transmission)
;2 - 3833 (1.9l AGR/ALH with transmission and 1.9l ASV with transmission)
;3 - 3875 (1.9l AGP/AQM with transmission)
;6 - 4492 (1.6l AEH/AKL/APF/AUR with transmission)
;
