;
; VAG-COM label file 3D0-035-704.lbl
;
; VW Phaeton (3D) - up to and including model year 2005 
;
; component: Telephone  -J526-  (#77)
;
;
; p/n: 3D0 035 729  Component: Telefon 0118   Coding: 0000000 
;
;    The above controller is used in conjunction with NAR Telematics controller 3D0 035 617 A,
;    Component: Telematik NAR1 0106, coding 0061850 to support both OnStar and NAR GSM with
;    a removable handset (Nokia), no bluetooth.  Details taken from VW Villa 2005 Phaeton.
;
; p/n: 3W0 035 729 C  Component: Telefon 0241   Coding: 0000000 - from 2004 W12, DD AM 2662
; p/n: 3W0 035 729 C  Component: Telefon 0241   Coding: 0000000 - from 2005 V6 TDI, Germany, Kai
; p/n: 3W0 035 729 C  Component: Telefon 0241   Coding: 0000000 - from 2005 V6 TDI, Swiss, Alex
;
;    The three parts listed above - all with 3W0 prefixes - are all installed in European cars.
;
; p/n: 3W0 035 729 K  Component: Telefon 0252   Coding: 0000000 - from 2005 Bentley Continental GT, Canadian
;      3D0 035 729    Component: Telefon 0118 - from a 2005 Phaeton with single handset prep, Canada
;
; by Michael Moore (Moore@ross-tech.com)
;
; created: 16/October/2005 (Michael)
; modified 23/November 2005 (Michael) - various part numbers added above.
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
;
001,3,Term 30,voltage,Possible Display: Between 6 and 15 volts
;
002,1,Term 15,status,Possible Display: On or Off
;
003,1,Telematics,status,Possible Display: 0 or 1 (indicates received Telematic message or not.)
;
004,2,Microphone,status,Possible displays: Short circuit Ground (GND) - short circuit B+ - open circuit or OK
004,4,Front,speaker,Possible displays: Short circuit Ground (GND) - short circuit B+ or OK
;
005,3,Telephone,charge current,Possible Display: Between 6 and 15 volts
;
006,2,Private,handset,Possible displays: Short circuit Ground (GND) - short circuit B+ or OK
006,4,Telephone,charge condition,Possible displays: 0 to 10
;
007,2,Phone,cradle,Possible displays: OK or open circuit
007,4,cradle,recognition,Possible displays: Short circuit B+ or OK (refers to private handset)