; For VW Passat (3C), no guaranties
Byte 00 Bit 0 Fog light installed
Byte 00 Bit 1 Xenon headlights with shutter installed
Byte 00 Bit 2 Footwell light installed
Byte 00 Bit 3 Daytime driving lights (Scandinavia) active
Byte 00 Bit 4 Daytime driving lights (North America) active
Byte 00 Bit 5 Assistance drivinglight with Leaving Home
Byte 00 Bit 6 Rain-/Lightsensor installed
Byte 00 Bit 7 Coming-Home installed
Byte 01 Bit 0 Rear seat recognition installed
Byte 01 Bit 1 Front Headlight washer installed
Byte 01 Bit 2 Electronic fuelpump relay installed
Byte 01 Bit 3 Rear wiper installed
Byte 01 Bit 4 Heated side mirror installed
Byte 01 Bit 5 Rear hatch remote opening
Byte 01 Bit 6 Rear hatch remote opening allowed - active
Byte 01 Bit 7 Rear Wiper when active driving backwards with continuesly wiper in front
Byte 02 Bit 0 Rear Wiper when active driving backwards with intermit wiper in front
Byte 02 Bit 1 Automatic turn signal on Highway when changing lane (press turn signal arm light)
Byte 02 Bit 2 Cold lamp diagnostics (no light on) (mandatory)
Byte 02 Bit 3 Loadmanagement (mandatory)
Byte 02 Bit 4 Coming-Home Mode by (0 = Adaption / 1 = Potentiometer)
Byte 02 Bit 5 Rear lid remote openening (0 = impuls activated / 1 = contact activated)
Byte 02 Bit 6 Side turn signal lights installed
Byte 02 Bit 7 Seat heating installed
Byte 03 Bit 0 Relay pin 15 inside installed
Byte 03 Bit 1 Rear fog light active (0 = 2 rear fog lights / 1 = 1 rear fog lights)
Byte 03 Bit 2 Reverse driving light active (0 = 2 reverse driving lights / 1 = 1 reverse driving lights)
Byte 03 Bit 3 Reverse driving light switched of when rear lid is open
Byte 03 Bit 4 Xenon head lights without shutter installed
Byte 03 Bit 5 Rear Wiper on, one time after normal wiper cycle (drip function)
Byte 03 Bit 6 Second battery installed
Byte 03 Bit 7 Rear light activation (0 = rear light dimmed / 1= rear light/Brake light dimmed)
Byte 04 Bit 0 Cabinheater installed
Byte 04 Bit 1 Extra airheater installed
Byte 04 Bit 2 Trailer Connection Unit installed
Byte 04 Bit 3 Electrical seatadjustment with memory
Byte 04 Bit 4 Activation of both rear fog lights installed
Byte 04 Bit 5 0 = Right hand drive (PR-L0R) / 1 = Left hand drive (PR-L0L)
Byte 04 Bit 6 Rear fog light not active
Byte 04 Bit 7 Automatic airconditioning installed
Byte 05 Bit 0 Front light cleaning delay - Resolution 50ms
Byte 05 Bit 1 - Decimal value multiply resolution
Byte 05 Bit 2 - For example: Byte decimal value: 20 is 20 x 50 = 1000 ms
Byte 05 Bit 3 
Byte 05 Bit 4 
Byte 05 Bit 5 
Byte 05 Bit 6 
Byte 05 Bit 7 
Byte 06 Bit 0 Frontlight cleaning activation time - Resolution 50ms
Byte 06 Bit 1 - Decimal value multiply resolution
Byte 06 Bit 2 - For example: Byte decimalvalue: 16 is 16 x 50 = 800 ms
Byte 06 Bit 3 
Byte 06 Bit 4 
Byte 06 Bit 5 
Byte 06 Bit 6 
Byte 06 Bit 7 
Byte 07 Bit 0 Extra function turn signal front left/right as parkinglight front left/right (USA and Canada)
Byte 07 Bit 1 - Decimalvalue (Resolution 1%)
Byte 07 Bit 2 
Byte 07 Bit 3 
Byte 07 Bit 4 
Byte 07 Bit 5 
Byte 07 Bit 6 
Byte 07 Bit 7 
Byte 08 Bit 0 Daylight dimming
Byte 08 Bit 1 - Decimalvalue (Resolution 1%)
Byte 08 Bit 2 
Byte 08 Bit 3 
Byte 08 Bit 4 
Byte 08 Bit 5 
Byte 08 Bit 6 
Byte 08 Bit 7 
Byte 09 Bit 0 Extra function Brakelight left/right as rear parkinglight
Byte 09 Bit 1 - Decimalvalue (Resolution 1%)
Byte 09 Bit 2 
Byte 09 Bit 3 
Byte 09 Bit 4 
Byte 09 Bit 5 
Byte 09 Bit 6 
Byte 09 Bit 7 
Byte 10 Bit 0 Extra function rear foglight left/right as parkinglight
Byte 10 Bit 1 - Decimalvalue (Resolution 1%)
Byte 10 Bit 2 
Byte 10 Bit 3 
Byte 10 Bit 4 
Byte 10 Bit 5 
Byte 10 Bit 6 
Byte 10 Bit 7 
Byte 11 Bit 0 Extra function front parkinglight left/right
Byte 11 Bit 1 - Decimalvalue (Resolution 1%)
Byte 11 Bit 2 
Byte 11 Bit 3 
Byte 11 Bit 4 
Byte 11 Bit 5 
Byte 11 Bit 6 
Byte 11 Bit 7 
Byte 12 Bit 0 Parkinglight left/right dimming
Byte 12 Bit 1 - Decimalvalue (Resolution 1%)
Byte 12 Bit 2 
Byte 12 Bit 3 
Byte 12 Bit 4 
Byte 12 Bit 5 
Byte 12 Bit 6 
Byte 12 Bit 7 
Byte 13 Bit 0 Replacement function front Side turn signal left/right as front Parkinglight left/right
Byte 13 Bit 1 - Decimalvalue (Resolution 1%)
Byte 13 Bit 2 
Byte 13 Bit 3 
Byte 13 Bit 4 
Byte 13 Bit 5 
Byte 13 Bit 6 
Byte 13 Bit 7 
Byte 14 Bit 0 Replacement function front Parkinglight left/right as front Side turn signal left/right
Byte 14 Bit 1 - Decimalvalue (Resolution 1%)
Byte 14 Bit 2 
Byte 14 Bit 3 
Byte 14 Bit 4 
Byte 14 Bit 5 
Byte 14 Bit 6 
Byte 14 Bit 7 
Byte 15 Bit 0 Replacement function Backlight left/right as rear Side turn signal left/right
Byte 15 Bit 1 - Decimalvalue (Resolution 1%)
Byte 15 Bit 2 
Byte 15 Bit 3 
Byte 15 Bit 4 
Byte 15 Bit 5 
Byte 15 Bit 6 
Byte 15 Bit 7 
Byte 16 Bit 0 Replacement function front fog light left/right as headlight low beam left/right
Byte 16 Bit 1 - Decimalvalue (Resolution 1%)
Byte 16 Bit 2 
Byte 16 Bit 3 
Byte 16 Bit 4 
Byte 16 Bit 5 
Byte 16 Bit 6 
Byte 16 Bit 7 
Byte 17 Bit 0 Ermergency flash light installed
Byte 17 Bit 1 Deactivation of High beam light with Bi-Xenon
Byte 17 Bit 2 Heated frontwindow installed
Byte 17 Bit 3 Diagnostics pin 50 active
Byte 17 Bit 4 Fog light as driving Daylight active
Byte 17 Bit 5 Fog light deactivated when Headlight high beam
Byte 17 Bit 6 Park light function USA/Canada not active
Byte 17 Bit 7 Free
Byte 18 Bit 0 Cold lamp diagnostics License plate light active
Byte 18 Bit 1 Cold lamp diagnostics Brake light active
Byte 18 Bit 2 Cold lamp diagnostics Fog head light active
Byte 18 Bit 3 Cold lamp diagnostics Rear Fog light active
Byte 18 Bit 4 Cold lamp diagnostics Head light high beam active
Byte 18 Bit 5 Cold lamp diagnostics Turn signal active
Byte 18 Bit 6 Cold lamp diagnostics Back light active
Byte 18 Bit 7 Cold lamp diagnostics Side turn signal active
Byte 19 Bit 0 Cold lamp diagnostics Head light low beam active
Byte 19 Bit 1 Cold lamp diagnostics Front Parking light active
Byte 19 Bit 2 Cold lamp diagnostics Rear Parking light active
Byte 19 Bit 3 Diagnostic Rear Parking light active
Byte 19 Bit 4 Relay pin 75 mounted
Byte 19 Bit 5 Relay pin 15 engine room installed
Byte 19 Bit 6 Electrical Parkbrake installed
Byte 19 Bit 7 Free
Byte 20 Bit 0 Fog light dimming
Byte 20 Bit 1 - Decimalvalue (Resolution 1%)
Byte 20 Bit 2 
Byte 20 Bit 3 
Byte 20 Bit 4 
Byte 20 Bit 5 
Byte 20 Bit 6 
Byte 20 Bit 7 
