;
; VAG-COM label file 3D0-907-040.lbl
;
; VW Phaeton (3D) - up to and including model year 2005 
;
; component: Airbags  -J234-  (#15)
;
;
; p/n: 3D0 907 040 F     Component: 0C Airbag 8.4E+ H07 0935    Coding: 0000001 (2004 German spec W12 Phaeton)
; p/n: 3D0 909 601 D     Component: 0A Airbag 8.4E+ H07 0934    Coding: 0012353 (2004 Canadian spec W12 Phaeton)
; p/n: 3D0 909 601 E     Component: 0A Airbag 8.4E+ H10 0934    Coding: 0012353 (2004 USA spec W12 Phaeton)
; p/n: 3D0 909 601 E     Component: 0P Airbag 8.4E+ H10 0936    Coding: 0012368 (2004 Canadian spec Bentley Continental GT)
; p/n: 3D0 909 601 D     Component: 0P Airbag 8.4E+ H07         Coding: 0012360 (2004 Europe spec Bentley Continental GT)
; p/n: 3D0 909 601 E     Component: 0G Airbag 8.4E+ H10 0934    Coding: 0012359 (2005 Canadian spec V8 Phaeton)
; p/n: 3D0 909 601 H     Component: 04 Airbag 8.4E++H01 0554    Coding: 0012340 (2005 USA spec V8 Phaeton with pax airbag light)
;
; NOTE: 3D0 909 601 H includes slave controller 3D0 959 339, Component: BF-Gewichtsensor 006 0005 to run pax airbag light. This is cut in beginning late 2005 MY production. 
; 
;
; by Michael Moore (Moore@ross-tech.com)
;
; Created:       30/August/2005 (Michael)
; last modified: 23/November/2005 (Michael) - H version controller and slave info added.
; last modified: 29/November/2005 (Michael) - All MVB's and adaptation channels mapped.
;                                           - Tested on a 2004 NAR LWB Phaeton.
;
; This controller uses blocks 1 to 4, 6 to 9, 11, 80, 125, and 225 only.
;
; Ready for VAG-COM 500.9 and above (500.9 supports block labels beginning with asterisks)
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
001,0,Igniter Status for Front Seating Positions
001,1,Driver Igniter,Status,This is the steering wheel airbag.
001,2,Passenger Igniter,Status,This is the front dashboard airbag.
001,3,Driver Seat Belt,Tensioner Igniter,
001,4,Passenger Seat Belt,Tensioner Igniter,
;
002,0,Igniter Status for Rear Seating Positions and Starter Battery Explosive Disconnect
002,1,Rear Driver Side,Igniter Status
002,2,Rear Pax Side,Igniter Status
002,3,Rear Middle Seat,Igniter Status
002,4,Battery Isolation,Igniter Status,This is the explosive disconnect on the starter battery.
;
003,0,Front Seating Positions - Belt in Use Sensors and Passenger Seat Occupancy Sensor
003,1,Voltage Supply,to Controller
003,2,Front Pax Seat,Occupancy Sensor,Not installed in all cars. It is possible that 'Too High' actually means 'Not Installed'.
003,3,Belt Fastened,Sensor Driver,This is the microswitch in the seat belt buckle
003,4,Belt Fastened,Sensor Passenger,This is the microswitch in the seat belt buckle
;
004,0,Rear Seating Positions - Belt in Use Sensors
004,1,Rear Driver Side,Belt in Use Sensor
004,2,Rear Pax Side,Belt in Use Sensor
004,3,Rear Middle,Belt in Use Sensor,It is possible that 'Too High' means 'Not Installed'.
004,4,Not Used
;
005,0,*This Group returns an error message.
;
006,0,Igniter Status for Side Airbags
006,1,Front Side Airbag,Driver Side
006,2,Front Side Airbag,Passenger Side
006,3,Rear Side Airbag,Driver Side
006,4,Rear Side Airbag,Passenger Side
;
007,0,*This Group returns an error message.
;
008,0,Igniter Status for Additional Airbags
008,1,Front Airbag 2,Driver Side
008,2,Front Airbag 2,Passenger Side
008,3,Driver Side,Head Level Airbag
008,4,Passenger Side,Head Level Airbag
;
009,0,Status of Key Switch for Passenger Airbag Control (may not installed in North American cars)
009,1,Key Switch,Status,Can be On or Off.
009,2,Unknown,,It is possible that this component is not installed in all cars.
009,3,Unknown,,It is possible that this component is not installed in all cars.
009,4,Not Used
;
010,0,*This Group returns an error message.
;
011,0,Unknown - may refer to components that are not installed in all cars.
;
012,0,*Next MVB used is block 80.
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,*Next block used is 125
;
125,0,CAN Bus Communications Status
;
126,0,*Next block used is 225
;
225,0,Unknown
;
;
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
; All channels have been mapped, but there does not appear to be any channels used
; for adaptation of this controller.
;
;
;end of file
;