;
; VAG-COM Labelfile
;
; Audi A6 (4F)
;
; Component: J104 - Brake Electronics (#03)
;
; P/N: 4F0-910-517-???
;
; includes measuring blocks and coding
;
; created on 27/Jun/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 02/Dec/2005
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left,Display Range: 0...255 km/h
001,2,Wheel Speed,Front Right,Display Range: 0...255 km/h
001,3,Wheel Speed,Rear Left,Display Range: 0...255 km/h
001,4,Wheel Speed,Rear Right,Display Range: 0...255 km/h
;
002,0,Switches && Buttons
002,1,Brake Test Switch,,Display Range: 0/operated
002,2,Brake Light Switch,,Display Range: 0/operated
002,3,Parking Brake,Button,Display Range: 0/operated
002,4,ESP-Passive,Button,Display Range: 0/operated
;
003,0,Engine Data
003,1,Engine Speed
003,2,Engine Torque
003,3,Engine Torque,(loss)
003,4,Throttle Valve Angle
;
004,0,Standing Time && EDL-T Flag
004,1,Standing Time
004,2,EDL-T Flag,,Display Range: ON/OFF\nSpecification: OFF
;
005,1,Steering Angle,Sensor (G85),Display Range: -720.0...+720.0 °\nTolerance: +/- 5.0 °
005,2,Turn Rate,,Display Range: -69.0...+69.0 °/s
005,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n\n-41.0 bar = short to ground\n290 bar = short to plus
005,4,Lateral,Acceleration,Display Range: -25.0...+25.0 m/sē
;
006,1,Voltage Supply,(Terminal 30),Specification: 9.8...17.4 V
006,2,Valve Relay,,Display Range: ON/OFF\nSpecification: ON
006,3,Return Flow Pump,Status,Display Range: ON/OFF
006,4,Workshop Code
;
007,0,Installation Position
007,1,Install. Position,Front Left,Display Range: invalid/OK/not OK (invalid when standig still)
007,2,Install. Position,Front Right,Display Range: invalid/OK/not OK (invalid when standig still)
007,3,Install. Position,Rear Left,Display Range: invalid/OK/not OK (invalid when standig still)
007,4,Install. Position,Rear Right,Display Range: invalid/OK/not OK (invalid when standig still)
;
008,0,Direction of Rotation
008,1,Direction,Front Left,Display Range: invalid/forward/reverse (invalid when standig still)
008,2,Direction,Front Right,Display Range: invalid/forward/reverse (invalid when standig still)
008,3,Direction,Rear Left,Display Range: invalid/forward/reverse (invalid when standig still)
008,4,Direction,Rear Right,Display Range: invalid/forward/reverse (invalid when standig still)
;
009,1,Brake Test Switch,,Display Range: 0/operated
009,2,Brake Light Switch,,Display Range: 0/operated
009,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n\n-41.0 bar = short to ground\n290 bar = short to plus
;
011,0,Additional Brake Pressure Sensors (only with ACC)
011,1,Brake Pressure,Front Right,Display Range: -41.0...+292.0 bar\n\n-41.0 bar = short to ground\n290 bar = short to plus
011,2,Brake Pressure,Front Left,Display Range: -41.0...+292.0 bar\n\n-41.0 bar = short to ground\n290 bar = short to plus
;
014,0,Airbag Coding Info (not relevant)
;
015,0,Engine Coding Info (not relevant)
;
016,0,Signals of Electro-Mechanical Parking Brake (not relevant)
;
021,0,Data from ESP Sensor Unit -G419- (not relevant)
;
022,0,Steering Angle Sensor Data (not relevant)
;
023,0,Variant Coding Data (not relevant)
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Steering Angle,Sensor,Specification: Steer. ang. 1
125,2,Engine,,Specification: Engine 1
125,3,Automatic,Transmission,Specification: Transm. 1
125,4,Instrument Cluster,,Specification: Instruments 1
;
126,0,CAN-Databus Communication (Powertrain)
126,1,Distance,Regulation (ACC),Specification: Distance 1
126,2,CAN-Gateway,,Specification: Gateway 1
126,3,Electric Parking,Brake (EPB),Specification: Park Brake 1
126,4,ESP Sensor,Cluster,Specification: ESP Sens. 1
;
127,0,CAN-Databus Communication (Powertrain)
127,1,Level Control,,Specification: Level 1
127,2,Airbag,,Specification: Airbag 1
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104) Coding
C01,ESP-Variant:
C02,Available on request.
C03, 
C04,Options:
C05,Available on request.
C06, 
C07,Trailer Hitch (4F0-910-517-K and above):
C08,+0000000 = with Trailer Hitch with Towing Recognition Control Module (J345)
C09,+0016384 = with/without Trailer Hitch without Towing Recognition Control Module (J345)
C10, 
C11,Detailed coding instructions for this
C12,control module are available on request.
C13,Mail to: sebastian@ross-tech.com
;
