;
; VAG-COM Labelfile
;
; Skoda Superb (3U)
;
; Component: J255 - A/C Heating Electronics (#08)
;
; P/N: 3U0-907-044-???
;
; includes measuring blocks and coding
;
; created on 09/Dec/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 09/Dec/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,A/C Heating Electronics (J255) Coding
C01,?xxxx: Compressor Type
C02,0 = Internally regulated
C03,1 = Internally regulated with temp. sensor behind evaporator
C04, 
C05,x?xxx: Vehicle Type
C06,7 = Skoda Superb (3U)
C07, 
C08,xx?xx: Country
C09,0 = Rest of World
C10,1 = Japan
C11,2 = USA
C12, 
C13,xxx?x: Engine Cooling
C14,0 = w/o characteristic map cooling
C15,1 = with characteristic map cooling
C16, 
C17,xxxx?: Equipment
C18,0 = with outside temperature indication
C19,1 = w/o outside temperature indication
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
000,0,Basic Setting (Specified Value: 0)
000,1,Temperature Regulator Flap Motor (V68),Specified Value: 0
000,2,Central Air Flap Motor (V70),Specified Value: 0
000,3,Footwell/Defroster Flap Motor (V85),Specified Value: 0
000,4,Air Flow Flap Motor (V71),Specified Value: 0
;
001,0,General
001,1,Compressor,Shut-Off,
001,2,Engine Speed
001,3,Vehicle Speed,,Display Range: 0...255 km/h
001,4,Standing Time,,Specification: 0...240 Min\n\n250 = Battery disconnected\n255 = Transfer Malfunction
;
002,0,Temperature Regulator Flap Motor (V68)
002,1,Measured Value,,Display Range: 0...255
002,2,Specified Value,,Display Range: 0...255
002,3,Flap Position,(air supply cooled),Specification: 150...250
002,4,Flap Position,(air supply heated),Specification: 5...100
;
003,0,Central Air Flap Motor (V70)
003,1,Measured Value,,Display Range: 0...255
003,2,Specified Value,,Display Range: 0...255
003,3,Flap Position,(air flow to panel),Specification: 150...250
003,4,Flap Position,(air flow to footwell),Specification: 5...100
;
004,0,Footwell/Defroster Flap Motor (V85)
004,1,Measured Value,,Display Range: 0...255
004,2,Specified Value,,Display Range: 0...255
004,3,Flap Position,(air flow to footwell),Specification: 150...250
004,4,Flap Position,(air flow to defrost.),Specification: 5...100
;
005,0,Air Flow Flap Motor (V71)
005,1,Measured Value,,Display Range: 0...255
005,2,Specified Value,,Display Range: 0...255
005,3,Flap Position,(fresh air flow),Specification: 150...250
005,4,Flap Position,(recirculating),Specification: 5...100
;
006,0,Temperatures I && Photo Sensor
006,1,Calculated,Temperature
006,2,Fresh Air Duct,Temperature (G89)
006,3,Outside Air,Temperature (G17)
006,4,Sunlight Photo,Sensor (G107)
;
007,0,Temperatures II
007,1,Center Vent (G191),Temperature
007,2,Footwell (G192),Temperature
007,3,Dash Panel (G56),Temperature 
007,4,Evaporator (G263),Temperature
;
008,0,Voltages
008,1,Fresh Air Blower,(V2 - specified),Display Range: 0 V = Blower Off / 3.6 V = Blower Speed 1 / 12 V = Blower Speed 7
008,2,Fresh Air Blower,(V2 - actual),Specification: ± 0.8 V to Specification (in Field 1)
008,3,Voltage,(Terminal 15)
008,4,Fresh Air Blower,(V2) Load
;
009,0,Blower && Heating I
009,3,Fresh Air Blower,(V2) Stage
;
010,0,Blower && Heating II
010,1,External Heater
010,2,Heating
010,3,Front Wiper
010,4,Coolant,Temperature
;
011,1,Dimming,(Terminal 58d)
011,2,Engine Speed,Increase
;
013,0,CAN-Databus Communication (Comfort)
013,1,CAN-Comfort,Status,Specification: 2-Wire\nDisplay Range: 2-Wire/1-Wire
013,2,CAN-Gateway,(J533),Specification: Gateway 1\nDisplay Range: Gateway 0/Gateway 1
013,3,Instrument Cluster,(J285),Specification: Instruments 1\nDisplay Range: Instruments 0/Instruments 1
;
080,0,Advanced Control Module Identification I
;
