;
; VAG-COM Labelfile
;
; VW Passat (3C)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 3C0-920-???-???
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 3C-17.LBL
; 3C0-920-xxx-17.LBL
;
; created on 29/Oct/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 29/Oct/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Display range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Mileage
002,2,Fuel Level,(G)
002,3,Fuel Level,Sender (G)
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
;
004,0,General
004,1,Voltage,(Terminal 30)
;
005,0,Service Reminder
005,1,Service Exceeding,(Distance),in Kilometers (km)
005,2,Service Exceeding,(Time),in Days
005,3,Remaining to,Service (Distance),in Kilometers (km)
005,4,Remaining to,Service (Time),in Days
;
006,0,Service Reminder
006,1,Minimum Oil Level,in Service Interval
006,2,Maximum Oil Level,in Service Interval
006,3,Long Time Avarage,Oil Level Difference
;
007,0,Fuel Level Sender (G) Raw Data
;
012,0,Adaptation Channels 040 && 041
012,1,Adaptation,Channel
012,2,Mileage,since Service,See Adaptation Channel 040
012,3,Adaptation,Channel
012,4,Time,since Service,See Adaptation Channel 041
;
013,0,Adaptation Channels 042 && 043
013,1,Adaptation,Channel
013,2,Minimum Mileage,to Service,See Adaptation Channel 042
013,3,Adaptation,Channel
013,4,Maximum Mileage,to Service,See Adaptation Channel 043
;
014,0,Adaptation Channels 044 && 049
014,1,Adaptation,Channel
014,2,Maximum Time,to Service,See Adaptation Channel 044
014,3,Adaptation,Channel
014,4,Minimum Time,to Service,See Adaptation Channel 049
;
015,0,Adaptation Channel 045
015,1,Adaptation,Channel
015,2,Oil Quality,,See Adaptation Channel 045
;
016,0,Adaptation Channels 047 && 048
016,1,Adaptation,Channel
016,2,Soot Entry,,See Adaptation Channel 047
016,3,Adaptation,Channel
016,4,Thermal Load,,See Adaptation Channel 048
;
050,0,General
050,1,Mileage
050,2,Engine Speed
050,4,Coolant,Temperature
;
060,0,Installation Information I (Senders and Sensors)
;
061,0,Installation Information II (Board Computer Buttons)
;
062,0,Installation Information III (Shift Information)
;
065,0,Installation Information IV (Indicator Lamps)
;
066,0,Installation Information V (Indicator Lamps)
;
067,0,Installation Information VI (Indicator Lamps)
;
068,0,Installation Information VII (Indicator Lamps)
;
090,0,Dimming I
090,1,Dimming,(Terminal 58d)
090,2,Dimming,(Photo Transistor)
;
091,0,Dimming II
;
092,0,Dimming III
;
094,0,Dimming IV
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine,,Specification: Engine 1\nDisplay Range: Engine 1/Engine 0
125,2,Transmission,,Display Range: Transm. 1/Transm. 0
125,3,Brake Electronics,(J104),Specification: ABS 1\nDisplay Range: ABS 1/ABS 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,CAN-Gateway,,Specification: Gateway 1\nDisplay Range: Gateway 1/Gateway 0
126,1,Airbag,(J234),Specification: Airbag 1\nDisplay Range: Airbag 1/Airbag 0
126,3,Steering,,Specification: Steering 1\nDisplay Range: Steering 1/Steering 0
;
129,0,CAN-Databus Powertrain (Communication)
129,1,Parking Brake,,Specification: Parking 1\nDisplay Range: Parking 1/Parking 0
;
201,1,Distance Impulse,Number
201,2,Start Impulse,recognized,Display Range: Yes/No
;
202,2,Wheel,Circumference
;
203,1,Failed Logins
203,2,Lock-Time
;
225,0,CAN-Databus Powertrain (Time-Out)
225,1,Engine
225,2,Transmission
225,3,Brake Electronics
;
226,0,CAN-Databus Powertrain (Time-Out)
226,1,CAN-Gateway
226,2,Airbag
226,3,Steering
;
229,0,CAN-Databus Powertrain (Time-Out)
229,1,Parking Brake
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??x05: Options
C02,+01 - Brake Pad Warning active
C03,+02 - Seatbelt Warning active
C04,+04 - Low Washer Fluid Warning active
C05, 
C06,xx?05: Country
C07,1 - Europe
C08,2 - USA
C09,3 - Canada
C10,4 - Great Britain
C11,5 - Japan
C12,6 - Arabian States
C13,7 - Australia
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 - Service NOT Due
A002,7,1 - Service Due
A002,8, 
A002,9,To reset the service reminder save 00000 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
;
A004,0,Language
A004,5,Language
A004,6,1 - German
A004,7,2 - English
A004,8,3 - French
A004,9,4 - Italian
A004,10,5 - Spanish
A004,11,6 - Portuguese
A004,12,7 - Symbols
A004,13,8 - Czech
A004,14,9 - Chinese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km/62 mi.
;
A030,0,Tank Characteristic
A030,5,Tank Characteristic
A030,6,Parallel shift of tank characteristic by ± 6 °
A030,7,Standard Value: 128
A030,8,Value Range: 116...140
A030,9,Increments: 1 = 0.5 °
A030,8, 
A030,9,Adaptation should be performed after emptying the tank
A030,10,and filling it with 7 liters of fuel.
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A039,0,Oil Level Sensor Adaptation
A039,5,Oil Level Sensor Adaptation
A039,6,Determines if the TOG Sensor is installed or not.
A039,7,0 - TOG Evaluation from the Instrument Cluster not activated
A039,8,1 - TOG Evaluation from the Instrument Cluster activated
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km or 1 = 100 mi
A040,7, 
A040,8,NOTE: Adaptation channels 40-49 must be
A040,9,entered and stored in the following order:
A040,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
A041,7, 
A041,8,NOTE: Adaptation channels 40-49 must be
A041,9,entered and stored in the following order:
A041,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 100 km or 1 = 100 mi
A042,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A042,8,00150 - flexible Service Intervals (15.000 km - with Longlife)
A042,9,or (if coded to miles)
A042,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A042,11,00090 - flexible Service Intervals (9.000 mi - with Longlife)
A042,12, 
A042,13,NOTE: Adaptation channels 40-49 must be
A042,14,entered and stored in the following order:
A042,15,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 100 km or 1 = 100 mi
A043,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A043,8,00300 - flexible Service Intervals (30.000 km - with Longlife)
A043,9,or (if coded to miles)
A043,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A043,11,00190 - flexible Service Intervals (19.000 mi - with Longlife)
A043,12, 
A043,13,NOTE: Adaptation channels 40-49 must be
A043,14,entered and stored in the following order:
A043,15,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 - fixed Service Intervals (w/o Longlife)
A044,8,00730 - flexible Service Intervals (with Longlife)
A044,9, 
A044,10,NOTE: Adaptation channels 40-49 must be
A044,11,entered and stored in the following order:
A044,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 - fixed Service Intervals (w/o Longlife)
A045,7,2 - flexible Service Intervals (with Longlife)
A045,8, 
A045,9,NOTE: Adaptation channels 40-49 must be
A045,10,entered and stored in the following order:
A045,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display
A046,8, 
A046,9,NOTE: Adaptation channels 40-49 must be
A046,10,entered and stored in the following order:
A046,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
A047,9, 
A047,10,NOTE: Adaptation channels 40-49 must be
A047,11,entered and stored in the following order:
A047,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
A048,9, 
A048,10,NOTE: Adaptation channels 40-49 must be
A048,11,entered and stored in the following order:
A048,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A049,0,Minimum Time to Service
A049,5,Minimum Time to Service
A049,6,Increments: 1 = 1 day(s)
A049,7,00365 - fixed Service Intervals (w/o Longlife)
A049,8,00730 - flexible Service Intervals (with Longlife)
A049,9, 
A049,10,NOTE: Adaptation channels 40-49 must be
A049,11,entered and stored in the following order:
A049,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
