;
; VAG-COM label file
;
; VW Phaeton (3D)
;
; component: Control Module for Telematics - J526 - (#75) (analog OnStar three button system)
;
;    p/n: 3D0 035 617   Telematik NAR1 0101 Coding: 0061860 (2004 Phaeton NAR, no GSM phone)
;    p/n: 3D0 035 617 A Telematik NAR1 0106 Coding: 0061850 (2005 Phaeton NAR, with GSM phone, no Bluetooth)
;      refer to 3D0 035 729 for the phone controller (address 77) used for NAR GSM without Bluetooth.
;
; includes some measured value blocks and coding - data is incomplete.
;
; by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; Modification History
;
; 27/March/2005 - Created by Michael
; 24/November/2005 - p/n added for NAR Phaeton with GSM phone prep.
; 30/November/2005 - Additional MVB data added, all MVB and adaptation channels mapped.
;
; ready for VAG-COM 402.3 and above
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
C00,Phaeton (3D) - Telematics System (J526) Coding
C01,61850 - Phaeton with 8 Channel Soundsystem
C02,61860 - Phaeton with 12 Channel Soundsystem
C03,61851 - Phaeton with 8 Channel Soundsystem - Information sent to Indicator Unit in Instrument Panel Insert
C04,61861 - Phaeton with 12 Channel Soundsystem - Information sent to Indicator Unit in Instrument Panel Insert
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
001,0,Telephone Signal Strength Available
001,2,Communication,with cell station,Possible Value: Acquired
001,4,Signal Strength,Percentage
;
002,0,GPS Satellite Status for OnStar System (NOT Phaeton Navigation GPS System)
002,3,GPS System,Status,Possible Value: Acquiring Satellites (looking)
002,4,Satellites,in view,Vehicle must be outside in order to see satellites!
;
003,0,Status of Automatically Generated Breakdown Signal (e.g. airbag deployment)
003,4,OnStar Button,Status,Refers to large blue button
;
004,0,Status of Red and White OnStar Buttons
004,2,Emergency Button,Status,Refers to red button
004,4,Hang-up Button,Status,Refers to white button
;
005,0,Vehicle Electrical System Status
005,1,Terminal 15,Status
;
006,0,*Next measured value block is 20.
;
020,0,Longitude (Only valid when GPS constellation has been acquired)
020,2,Degrees
020,3,Minutes
020,4,Seconds
;
021,0,Latitude (Only valid when GPS constellation has been acquired)
021,2,Degrees
021,3,Minutes
021,4,Seconds
;
022,0,Altitude (Only valid when GPS constellation has been acquired)
022,2,Height
;
023,0,Longitude (Only valid when GPS constellation has been acquired) 
023,2,Degrees
023,3,Minutes
023,4,Seconds
;
024,0,Latitude (Only valid when GPS constellation has been acquired)
024,2,Degrees
024,3,Minutes
024,4,Seconds
;
025,0,Altitude above sea level (Only valid when GPS constellation has been acquired)
025,2,Height
;
026,0,Date (Only valid when GPS constellation has been acquired)
026,2,Day
026,3,Month
026,4,Year
;
027,0,Time (Only valid when GPS constellation has been acquired)
027,2,Hour
027,3,Minute
027,4,Second
;
028,0,Heading, DP (Only valid when GPS constellation has been acquired)
028,2,Heading
028,4,DP
;
029,0,Vehicle Speed and Antenna Status
029,2,Vehicle Speed
029,4,Antenna Status
;
030,0,Voltage Supplied to Controller
030,2,Voltage
;
031,0,*Next MVB is 076.
;
076,0,Vehicle 10 digit Phone Number - xxx ??????????x (disregard the x numbers)
;
077,0,Expanded Control Module Identification
;
078,0,Electronic Serial Number (ESN) of Analog Phone Module - xxx ??????????? (disregard the x numbers)
;
079,0,Control Module Identification Code (STID) - xxx ??????????? (disregard the x numbers)
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,*Next MVB is 125.
;
125,0,Presumed to be CAN bus status - but not sure.
;
126,0,Data Bus Status
;
127,0,*Next MVB is 203
;
203,0,Unknown
;
204,0,Unknown
;
205,0,Unknown
;
206,0,Unknown
;
207,0,Unknown
;
208,0,*End of MVB for this controller.
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
A03,0,Enabling Service or Transport Mode
A03,2,Service Mode,Status
A03,5,Instructions
A03,6,To disable transport mode (in other words to enable
A03,7,normal OnStar operation) enter a value of 0 in channel
A03,8,three and save this value.
;
A07,0,Test Call Status
A07,2,Test Call Status
;
A99,0,Test Mode
A99,1,Test Mode,Status
;
;
; end of file