;
; VAG-COM Labelfile
;
; Seat Altea/Toledo (5P) / Skoda Octavia II (1Z)
; VW Caddy (2K) / VW Golf/Jetta (1K) / VW Touran (1T)
;
; Component: J255 - A/C Heating Electronics (#08) - Climatronic
;
; P/N: 1K0-907-044-???
;
; includes measuring blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1T-08.LBL
; 1K0-907-044.LBL
;
; created on 23/Mar/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 17/Dec/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,General
001,1,Compressor,Shut-Off Code
001,2,Engine Speed
001,3,Vehicle Speed
001,4,Standing Time
;
002,0,Compressor
002,1,Compressor,Current (actual)
002,2,Compressor,Current (specified)
002,3,Compressor,Rotations
002,4,Compressor Load
;
003,1,Coolant,Pressure
003,2,Radiator Fan,Activation (actual)
003,3,Radiator Fan,Activation (spec.)
003,4,Engine Speed,(increase)
;
004,0,Temperatures
004,1,Outside Temp.,Unfiltered,Display Range: -50...+63 °C
004,2,Outside Temp.,Regulation,Display Range: -50...+77 °C
004,3,Fresh Air Intake,Temperature,Display Range: -40...+60 °C
004,4,Coolant,Temperature,Display Range: -48...+126 °C
;
005,0,Outlet/Footwell Blower Temperature
005,1,Left Outlet Blower,Temperature,Display Range: 0...84 °C
005,2,Right Outlet Blower,Temperature,Display Range: 0...84 °C
005,3,Left Footwell,Blower Temp.,Display Range: 0...84 °C
005,4,Right Footwell,Blower Temp.,Display Range: 0...84 °C
;
006,1,Evaporator,Temperature
006,2,Interior,Temperature
006,3,Left Sunlight,Intensity (G107),W/m²
006,4,Right Sunlight,Intensity (G134),W/m²
;
007,1,Turbine Voltage,(actual),Display Range: 0.0...13.0 V
007,2,Turbine Voltage,(specified),Display Range: 0.0...13.0 V
007,3,Turbine Load,,Display Range: 0.0...100.0 %
007,4,Voltage,(Terminal 30)
;
008,1,Voltage,(Terminal 15)
008,3,Dimming,(Terminal 58d),Display Range: 0.0...100.0 %
008,4,Country,,1 = Rest of World (RoW)\n2 = North America (NAR)
;
009,0,Rear Window Heater (Z2) && Aux. Heater
009,1,Rear Window,Heater (Z2 / Actual)
009,2,Rear Window,Heater (Z2 / Spec.)
009,3,Aux. Heater,Status,Display Range: ON/OFF
009,4,Aux. Heater,Current
;
010,1,Aux. Heater,Request,Display Range: ON/OFF
010,2,Heater OFF,,Display Range: ON/OFF
010,3,Back-Up Lights,,Display Range: ON/OFF
010,4,Front Wiper,,Display Range: ON/OFF
;
011,0,Air Recirculation Flap Control Motor (V113) / Potentiometer (G143)
011,1,Current Value
011,2,Specified Value
011,3,Minimum Position,(Lower Stop/Close)
011,4,Maximum Position,(Upper Stop/Open)
;
012,0,Left Temperature Flap Control Motor (V158) / Potentiometer (G220)
012,1,Current Value
012,2,Specified Value
012,3,Minimum Position,(Lower Stop/Close)
012,4,Maximum Position,(Upper Stop/Open)
;
013,0,Right Temperature Flap Control Motor (V159) / Potentiometer (G221)
013,1,Current Value
013,2,Specified Value
013,3,Minimum Position,(Lower Stop/Close)
013,4,Maximum Position,(Upper Stop/Open)
;
014,0,Center Flap Control Motor (V70) / Potentiometer (G112)
014,1,Current Value
014,2,Specified Value
014,3,Minimum Position,(Lower Stop/Close)
014,4,Maximum Position,(Upper Stop/Open)
;
015,0,Defroster Flap Control Motor (V107) / Potentiometer (G135)
015,1,Current Value
015,2,Specified Value
015,3,Minimum Position,(Lower Stop/Close)
015,4,Maximum Position,(Upper Stop/Open)
;
016,0,Air Flow Flap Control Motor (V71) / Potentiometer (G113)
016,1,Current Value
016,2,Specified Value
016,3,Minimum Position,(Lower Stop/Close)
016,4,Maximum Position,(Upper Stop/Open)
;
080,0,Advanced Control Module Identification I
;
