;
; VAG-COM Labelfile
;
; Aud A3 (8P) / Audi A4 (8E) / Audi TT (8N)
; VW Golf/Jetta (1K) / VW New Beetle (1C) / VW Passat (3C)
;
; Component: R146 - Digital Radio (#0F) - XM
;
; P/N: 8E0-035-593-???
;
; includes measuring blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8E-0F.LBL
; 8E0-035-593-SIR.LBL
; 8E0-035-593-XM.LBL
;
; created on 03/Aug/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 29/Aug/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,General
001,1,Supply Voltage,(Terminal 30),Specification: 8.5...15.5 V
;
004,0,Electronic Serial Number (ESN)
004,1,Enabling Code
;
005,0,Signal
005,1,Signal Quality,,1 = No Signal\n2 = Too weak\n3 = OK\n4 = Optimum
005,2,Audi Signal,Status (present),Display Range: Yes/No
;
007,0,Status
007,1,Status,(bounded),Display Range: Yes/No
007,2,Status,(subscribed),Display Range: Yes/No
;
008,0,Service Information
008,1,Provider,Information
; 0 = Normal Operation
; 1 = Antenna not connected
; 2 = Update enabling code
; 3 = No Signal
; 4 = Channel Change
; 5 = Channel not offered
; 6 = Channel no longer available
; 7 = Additional channel info not available
008,2,Satellite,Antenna Status,0 = OK\n1 = Short to Ground\n2 = Short to Plus
008,3,Terrestrial,Antenna Status,0 = OK\n1 = Short to Ground\n2 = Short to Plus
;
