;
; VAG-COM label file
;
; Audi A3 (8L) / Skoda Octavia (1U) / VW Golf/Jetta (1J)
;
; component: Engine (#01) - AVU
;
; p/n: 06A 906 033 ?
;
; includes measuring blocks, coding and adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 03-01.LBL
; 06-01.LBL
; 06A-906-033-AVU.LBL (1.6l E   @ 102 HP - AVU)
;
; created on 10/Apr/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,Engine Control Module Coding
C1,00?xx: Additional Functions
C2,0 - No additional functions
C3,2 - Climatronic
C4, 
C5,00x?x: CAN-Databus
C6,+1 - Anti-Blocking-System (ABS)
C7,+2 - Airbag
C8, 
C9,00xx?: Transmission
C10,1 - 5-Speed Manual Transmission
C11,3 - Automatic Transmission
;
;
;---------------------------------------------------
;
; Anpassungs Informationen
;
;---------------------------------------------------
;
;
A01,0,Idle Speed Adapatation
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,1,Basic Functions
001,1,Engine Speed,,Specification: 640...900 RPM
001,2,Coolant,Temperature,Specification: 80...115 °C
001,3,Lambda,Regulator,Specification: -10.0...+10.0 %
001,4,Basic Setting,Requirements,see labelfile
; 1xxxxx-x - Coolant temperature below 80 °C
; x1xxxx-x - Engine speed below 2000 RPM
; xx1xxx-x - Throttle valve closed
; xxx1xx-x - Lambda regulation correct
; xxxx1x-x - State of idle
; xxxxx1-x - A/C system compressor deactivated
; xxxxxx-1 - No malfunction detected by Self-Diagnosis
;
002,0,Basic Functions
002,1,Engine Speed,,Specification: 640...900 RPM
002,2,Engine Load,,Specification: 24.0...35.0 %
002,3,Injection,Timing,Specification: 2.0...4.0 ms
002,4,Intake Air Mass,,Specification: 2.0...4.5 g/s
;
003,0,Basic Functions
003,1,Engine Speed,,Specification: 640...900 RPM
003,2,Intake Air Mass,,Specification: 2.0...4.5 g/s
003,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 % | Specification: 1.9...4.0 %
003,4,Ignition,Timing Angle,Specification: 0...15 °BTDC
;
004,0,Basic Functions
004,1,Engine Speed,,Specification: 640...900 RPM
004,2,Voltage Supply,,Specification: 11.5...15.0 V
004,3,Coolant,Temperature,Specification: 80...115 °C
004,4,Intake Air,Temperature,Specification: -38.0...+80.0 °C
;
005,0,Basic Functions
005,1,Engine Speed,,Specification: 640...900 RPM
005,2,Engine Load,,Specification: 24.0...35.0 %
005,3,Vehicle Speed,,Specification: 0 km/h
005,4,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
;
006,0,Basic Functions
006,1,Engine Speed,,Specification: 640...900 RPM
006,2,Engine Load,,Specification: 24.0...35.0 %
006,3,Intake Air,Temperature,Specification: -38.0...+80.0 °C
006,4,Heights Correction,Factor,Display Range: -50.0...+10.0 %
;
010,0,Ignition
010,1,Engine Speed,,Specification: 640...900 RPM
010,2,Engine Load,,Specification: 24.0...35.0 %
010,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 % | Specification: 1.9...4.0 %
010,4,Ignition,Timing Angle,Specification: 0..15 °BTDC
;
012,0,Ignition (Position of Camshaft vs. Crankshaft)
012,1,Engine Speed,,Specification: 640...900 RPM
012,2,Engine Load,,Specification: 24.0...35.0 %
012,3,Crankshaft Tooth,(low > high),No. of crankshaft tooth at camshaft flank (Specification: 26...30)
012,4,Crankshaft Tooth,(high > low),No. of crankshaft tooth at camshaft flank (Specification: 86...90)
;
015,0,Misfire Recognition
015,1,Cylinder 1
015,2,Cylinder 2
015,3,Cylinder 3
015,4,Malfunction,Recognition,Display Range: activated/blocked
;
016,0,Misfire Recognition
016,1,Cylinder 4
016,4,Malfunction,Recognition,Display Range: activated/blocked
;
020,0,Ignition (Knock Control - Cyl 1 - 4)
020,1,Cylinder 1 Ignition,Angle Delay,Specification: 0...12 °CA
020,2,Cylinder 2 Ignition,Angle Delay,Specification: 0...12 °CA
020,3,Cylinder 3 Ignition,Angle Delay,Specification: 0...12 °CA
020,4,Cylinder 4 Ignition,Angle Delay,Specification: 0...12 °CA
;
022,0,Ignition (Knock Control - Cyl 1 && 2)
022,1,Engine Speed,,Specification: 640...6500 RPM
022,2,Engine Load,,Specification: 40.0...100.0 %
022,3,Cylinder 1 Ignition,Angle Delay,Specification: 0...12 °CA
022,4,Cylinder 2 Ignition,Angle Delay,Specification: 0...12 °CA
;
023,0,Ignition (Knock Control - Cyl 3 && 4)
023,1,Engine Speed,,Specification: 640...6500 RPM
023,2,Engine Load,,Specification: 40.0...100.0 %
023,3,Cylinder 3 Ignition,Angle Delay,Specification: 0...12 °CA
023,4,Cylinder 4 Ignition,Angle Delay,Specification: 0...12 °CA
;
028,0,Ignition (Knock Sensor Test)
028,1,Engine Speed,,Specification: 640...6500 RPM
028,2,Engine Load,,Specification: 40.0...100.0 %
028,3,Coolant,Temperature,Specification: 80...115 °C
028,4,Result,Knock Sensor Test,Display Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
030,0,Oxygen Sensor Status
030,1,Bank 1,Sensor 1,Specification: 111
; 1xx - Lambda sensor heating on
; x1x - Lambda sensor ready
; xx1 - Lambda regulation active
030,2,Bank 1,Sensor 2,Specification: 110
; 1xx - Lambda sensor heating on
; x1x - Lambda sensor ready
; xx1 - Lambda regulation active
;
031,0,Lambda Regulation (Contant Operation of Lambda Probes)
031,1,Lambda Sensor,Current Value,Specification: 0.99...1.01
031,2,Lambda Sensor,Specified Value,Specification: 0.99...1.01
;
032,0,Lambda Regulation
032,1,Lambda (Idle),Self-Adaptation,Specification: -14...+14
032,2,Lambda (Partial),Self-Adaptation,Specification: -10...+10
;
033,0,Lambda Regulation
033,1,Bank 1,Lambda Control,Specification: 1.4...1.6 V
033,2,Bank 1 Voltage,of Oxygen Sensors,Specification: -10.0...+10.0 %
;
034,0,Lambda Regulation (befor Catalyst - Basic Setting: Aging Check)
034,1,Engine Speed,,Specification: 2500...4000 RPM
034,2,Catalytic Converter,Temperature,Specification: min. 400 °C
034,3,Period,Duration Sensor,Specification: > 0.21
034,4,Result,Lambda Aging,Display Range: Test ON/Test OFF/B1-S1 not OK/B1-S1 OK
;
041,0,Lambda Regulation (Lambda Probe Heating)
041,1,Resistance,Bank 1 Sensor 1
041,2,Heater Condition,,Specification: Htg.bC.ON
041,3,Resistance,Bank 1 Sensor 2,Specification: 96...608
041,4,Heater Condition,,Specification: Htg.aC.ON
;
043,0,Lambda Regulation (befor Catalyst - Basic Setting)
043,1,Engine Speed,,Specification: ~1400 RPM
043,2,Catalytic Converter,Temperature,Specification: min. 200 °C
043,3,Bank 1 Sensor 2,Voltage,Specification: 0.0...1.0 V
043,4,Result,Lambda Aging,Display Range: Test ON/Test OFF/B1-S2 not OK/B1-S2 OK
;
046,0,Lambda Regulation (Basic Setting: Conversion Test)
046,1,Engine Speed,,Specification: 2500...4500 RPM
046,2,Catalytic Converter,Temperature,Specification: min. 400 °C
046,3,Amplitude,Behavior
046,4,Result Catalytic,Conversion,Pre-Catalytic Converter (Display Range: Test ON/Test OFF/CatConvB1 not OK/CatConvB1 OK)
;
050,1,Engine Speed,,Specification: 640...900 RPM
050,2,Engine Speed,(specified),Specification (manual): 670...760 RPM | Specification (automatic): 800...860 RPM
050,3,Condition,of A/C system,Display Range: A/C-High / A/C-Low
050,4,Operating condition,of A/C Compressor,Display Range: Compr.ON/Compr.OFF
;
053,0,Speed Regulation
053,1,Engine Speed,,Specification: 640...900 RPM
053,2,Engine Speed,(specified),Specification (manual): 670...760 RPM | Specification (automatic): 800...860 RPM
053,3,Voltage Supply,,Specification: 11.5...15.0 V
053,4,Current,Consumption,Display Range: 0...100 %
;
054,0,Speed Regulation
054,1,Engine Speed,,Specification: 640...6500 RPM
054,2,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
054,3,Sender 2 for,Acc. Pedal Pos.,G79 (Display Range 0...100 %)
054,4,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
;
055,0,Speed Regulation
055,1,Engine Speed,,Specification: 640...900 RPM
055,2,Idle Regulator,,Specification: -10.0...+10.0 %
055,3,Idle Stabilization,Self-Adaptation,Specification: -10.0...+10.0 %
055,4,Load Status,,see labelfile
; 1-xxx - Power assisted steering pressure switch on
; x-1xx - Air conditioning system switched on
; x-x1x - Heating switched on
; x-xx1 - Air conditioner compressor switched on
;
056,0,Speed Regulation
056,1,Engine Speed,,Specification: 640...900 RPM
056,2,Engine Speed,(specified),Specification (manual): 670...760 RPM | Specification (automatic): 800...860 RPM
056,3,Idle Regulator,,Specification: -10.0...+20.0 %
056,4,Load Status,,see labelfile
; 1-xxx - Power assisted steering pressure switch on
; x-1xx - Air conditioning system switched on
; x-x1x - Heating switched on
; x-xx1 - Air conditioner compressor switched on
;
060,0,Speed Regulation (Basic Setting: Throttle Body Adaptation)
060,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0...100 %
060,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 100...0 %
060,3,Self-Adaptation,Steps Counter,Specification: 0...9
060,4,Result,Throttle Valve Adp.,Display Range: ADP runs/ADP OK/ADP ERROR
;
062,1,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 3...97 %
062,2,Throttle Drive,Angle Sensor 2,for EPC (G188) | Specification: 97...3 %
062,3,Throttle Position,Sensor (G79),Specification: 6...96 %
062,4,Accelerator Pedal,Position Sensor 2,G185 (Specification: 3...48 %)
;
063,0,Speed Regulation (Basic Setting: Kick-Down Adaptation)
063,1,Throttle Position,Sensor (G79),Display Range: 0...100 %
063,2,Accelerator Pedal,Position Sensor 2,G185
063,3,Kick-Down,Switch,Display Range: Kick Down
063,4,Kick-Down,Adaptation,Display Range: ADP runs/ADP OK/ADP ERROR
;
066,0,Cruise Control System (CCS/GRA)
066,1,Actual,Vehicle Speed
066,2,Brake switch,clutch and CCS,see labelfile
; ----1xxx - Cruise control system active
; ----x1xx - Clutch depressed (always 1 in automatic transmission)
; ----xx1x - Brake depressed (brake pedal switch)
; ----xxx1 - Brake depressed (brake light switch)
066,3,Specified,Vehicle Speed
066,4,CCS Control,Positions,see labelfile
; ----1xxx - CCS slide handle on RES or RES button on multi-function steering wheel pressed
; ----x1xx - SET button pressed
; ----xx1x - CCS slide handle on OFF (not engaged or engaged)/OFF button on multi-function steering wheel pressed
; ----xxx1 - CCS slide handle on OFF
;
070,0,Emission Reduction (TEV - Basic Setting)
070,1,Evap. Emissions,Sol. Valve (Open),Specification: 0...100 %
070,2,Oxygen Sensor,Control Deviation
070,3,Evap. Emissions,Sol. Valve (Flow)
070,4,Result,Evap. Emissions,Display Range: Test ON/Test OFF/TEV OK/TEV not OK
;
074,0,Emission Reduction (Basic Setting)
074,1,Min.-Position,,Specification: 0.3...1.5 V
074,2,Max.-Position,,Specification: 3.0...4.8 V
074,3,Potentiometer,(actual),Specification: 0...100 %
074,4,Adaptation,Status,Display Range: ADP run/ADP OK/ADP ERROR
;
075,0,Exhaus Gas Recirculation (Basic Setting)
075,1,Engine Speed,,Specification: 640...900 RPM
075,2,Potentiometer,Value,Specification: 0...100 %
075,3,Valve Stroke,Difference,Specification: -10...+25 %
075,4,Display Range: Test ON/Test OFF/Syst. OK/Syst. n.OK
;
077,0,Emission Reduction (Basic Setting)
077,1,Engine Speed,,Specification: ~1400 RPM
077,4,Result,,Display Range: Test ON/Test OFF/Syst. OK/Syst. n.OK
;
089,0,Trip Recorder
089,1,Distance travelled,with MIL active
089,2,Condition,"Tank Empty",Display Range: OK/too low
;
095,0,Variable Intake Manifold (Single Stage Changeover)
095,1,Engine Speed,,Specification: 640...900 RPM
095,2,Engine Load
095,3,Coolant,Temperature,Specification: 80...115 °C
095,4,Variable Intake,Manifold Status,Display Range: ON/OFF
;
099,0,Lambda Regulation (Basic Setting)
099,1,Engine Speed,,Specification: 640...900 RPM
099,2,Coolant,Temperature,Specification: 80...115 °C
099,3,Lambda Regulator,(before catalyst),Specification: -10.0...+10.0 %
099,4,Status Lambda,Regulation,Display Range: ON/OFF
;
100,1,Readiness Bits,,see labelfile
; 1xxxxxxx - Exhaust Gas Recirculation (EGR)
; x1xxxxxx - Sensor heater
; xx1xxxxx - Oxygen sensors
; xxx1xxxx - A/C system
; xxxx1xxx - Secondary Air Injection (AIR) system
; xxxxx1xx - Activated charcoal system
; xxxxxx1x - Catalytic converter heater
; xxxxxxx1 - Catalytic converter
100,2,Coolant,Temperature
100,3,Time since,Engine Start
100,4,OBD-Status,,see labelfile
; 1-xxxxxx - MIL warning lamp on
; x-1xxxxx - Complete distance
; x-x1xxxx - At least one malfunction detected
; x-xx--1x - Heating cycle ended
; x-xx--x1 - Heating cycle not possible
;
120,0,Traction Control (TC/ASR)
120,1,Engine Speed,,Specification: 640...6500 RPM
120,2,Engine Load,(specified),Specification: 0...399 Nm
120,3,Engine Load,(actual),Specification: 0...260 Nm
120,4,Status,,Display Range: TC active/TC n.active
;
122,0,Transmission
122,1,Engine Speed,,Specification: 640...6500 RPM
122,2,Engine Load,(specified),Specification: 0...399 Nm
122,3,Engine Load,(actual),Specification: 0...260 Nm
122,4,Status,,Display Range: Torque red./No tor.red.
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Transmission
125,2,Brake Electronics
125,3,Instrument Cluster
;
126,0,CAN-Databus Communication (Powertrain)
126,3,Airbag
;
130,0,Mapped Cooling
130,1,Coolant temp.,engine outlet,Specification: 80...115 °C
130,2,Cooland temp.,radiator outlet,Specification: 0...100 °C
130,3,Thermostat,duty cycle,Specification: 0...100 %
130,4,Result,,Display Range: Test ON/Test OFF/Syst. OK/Syst. n.OK
;
131,0,Mapped Cooling
131,1,Coolant temp.,engine outlet,(actual) Specification: 80...115 °C
131,2,Coolant temp.,engine outlet,(specified) Specification: 0...115 °C
131,3,Cooland temp.,radiator outlet,Specification: 0...100 °C
131,4,Thermostat,duty cycle,Specification: 0...100 %
;
132,0,Mapped Cooling
132,1,Coolant,temperature,radiotor outlet
132,2,Temperature,difference,between engine and radiator outlet
132,3,Heater supply,potentiometer,Specification (w/o Climatronic): 0.2...4.8 V | Specification (with Climatronic): 0.2...5.1 V
132,4,Cooling,Status
; 1xxxxx - Fan stage 1 active
; x1xxxx - Fan stage 2 active
; xx1xxx - Control deviation below spec.
; xxx1xx - Fan activation
; xxxx1x - Thermostat activation
; xxxxx1 - Malfunction
;
