; VAG-COM  Measuring Block Label for Golf 98+
; Code: AHW,AKQ ,ecu :036 906 041M
; MARELLI 4AV
; Jozsef Molnar < romcej.molnar@xnet.ro>
;
; // File appears not to have been tested.
; // replaced some commas with decimal points
; // -- Uwe


;
;0,0,Measuring block
;0,1,IAT,156...44 =15..70 C
;0,2,Batt Voltage,120...160 =12..14.5V
;0,3,Engine Temp,37..18 =85...120 C
;0;4,Manifold Abs Press,32...71 =240...420mbar
;0,5,Oxygen Sensor,0...184 =0.00...090V
;0;6,Oxygen Regl.Not for Customer
;0;7,Not Use
;0,8,Throttle Potm Voltage,200240 =4.0...4.5V
;0,9,Injection Time,5...14 =3.00...7.00ms
;0,10,Engine Speed,21...25 =700...800/min
;
1,0,General Engine Data
1,1,Engine Speed,700...800/min
1,2,Coolant Temp,85...110C
1,3,Oxygen Sensor Volt,0.000...0.900V
1,4,BIN,00000000
;            1             -DTC in memory,0- No DTC recogn
;              1           -Gear boxon,0-Gear box free
;                1         -Aircond on,0-Aircond off
;                  1       -F60 Open,0-Close
;                    1     -Oxygen regl Not OK,0-Oxyben regl OK
;                      1   -Throttle sw Open,.0-Throttle sw Close
;                        1 -Engine speed>1800.Engine speed<1800
;                          1-Coolant temp<80C,0-Coolant temp>80C
;
2,0,General Engine Data
2;1,Engine Speed,700...800/min
2,2,Injection Time,2.56...5.12ms
2,3,ECU Voltage,11.5...14.5V
2,4,IAT,15...70C
;
3,0,General Engine Data
3,1,Engine Speed,700...800/min
3,2,Engine Load,12...40%
3,3,Throttle Angle,1...7
3,4,Thottle Regl,.........%
;
4,0,General Engine Data
4,1,Engine Speed,700...800/min
4,2,Engine Load,12..40%
4,3,Vehicle Speed,0km/h
4,4,BIN,00000000
;           1              -Deceleration
;            1             -Idle
;             1            -Partially Open Throttle
;              1           -Wide Open Thottle
;               1          -Not In Use
;                1         -Not In Use
;                 1        -Not In Use
;                  1       -Not In Use
;
5,0,Throttle Controll
5,1,Engine Speed,700...800/min
5,2,Valve Duty,6.0...19.0%
5,3,Fuel Consumption,0.50...1.10l/h
5,4,Throttle Calibration Status,00000000
;                                            
;                                             
;                                             1 -Not In Use
;                                              1-Not In Use
;                                               1-Batt-Voltage too low,0-Battery-OK
;                                                1-Idle sin OK,0-Idle sign not OK
;                                                 1-F60 Open,0-Close
;                                                  1-Signal Between G88&G69 not OK,0-OK
;                                                   1 -Voltage Between G88&G69 not OK,0-OK
;                                                     1-F60 In Basic Setting Open,0-Close
;
6,0,General Engine Data
6,1,Not for Customer
6,2,Not In Use
6,3,Not In Use
6,4,Not for Customer
;
98,0,Throttle Control Basic Setting
98,1,Throttle Pot G69 Voltage,0.500...5.00V
98,2,Throttle Pot G88 Voltage,0.500...5.00V
98,3,Operating Mode
98,4,Adaptation Status,Idle/OK/ERROR
;