;
; VAG-COM label file
;
; Audi A3 (8P)
;
; component: J285 - Instrument Cluster (#17)
;
; p/n: 8P0-920-???-???
;
; includes measuring blocks, adaptation, coding and security access
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8P-17.LBL
; 8P-25.LBL
; 8P0-920-xxx-17.LBL
; 8P0-920-xxx-25.LBL
;
; created on 14/Jul/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 17/Aug/2005
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure
001,4,Time
;
002,1,Mileage
002,2,Remote Clock,(Test Mode)
002,3,Tank Content
002,4,Ambient,Temperature
;
003,1,Coolant,Temperature
003,2,Standing Time
003,3,Dimming Signal,(Terminal 58d)
003,4,Dimming Signal,(Terminal 58s)
;
004,0,Supply Voltage && Outside Temperature
004,1,Supply Voltage,(Terminal 30)
004,2,Outside Temp.,(Climate Control)
004,3,Outside Temp.,(Display)
004,4,Phototransistor
;
005,0,Service Reminder
005,1,Distance since,Service exceeded,Unit: 100 km
005,2,Time since,Service exceeded,Unit: 1 day(s)
005,3,Remaining Dist.,until Service,Unit: 100 km
005,4,Remaining Time,until Service,Unit: 1 day(s)
;
006,1,Min. (M2) Oil Level,in Service Interval
006,2,Max. (M2) Oil Level,in Service Interval
006,3,Long Time Average,Oil Level Dif.,
006,4,Engine Hood,Contact,Display Range: open/closed
;
008,1,Short Time Mean,Oil Level Dif.,
008,2,Current (M2) Value
;
010,0,Adaptation Channels 003 && 004
010,1,Adaptation,Channel
010,2,Consumption,Correction,See Adaptation Channel 003
010,3,Adaptation,Channel
010,4,Language,,See Adaptation Channel 004
;
011,0,Adaptation Channels 009 && 019
011,1,Adaptation,Channel
011,2,Mileage,,See Adaptation Channel 009
011,3,Adaptation,Channel
011,4,Remote Control,Clock Synchron.,See Adaptation Channel 019
;
012,0,Adaptation Channels 040 && 041
012,1,Adaptation,Channel
012,2,Mileage,since Service,See Adaptation Channel 040
012,3,Adaptation,Channel
012,4,Time,since Service,See Adaptation Channel 041
;
013,0,Adaptation Channels 042 && 043
013,1,Adaptation,Channel
013,2,Minimum Mileage,to Service,See Adaptation Channel 042
013,3,Adaptation,Channel
013,4,Maximum Mileage,to Service,See Adaptation Channel 043
;
014,0,Adaptation Channels 044 && 049
014,1,Adaptation,Channel
014,2,Maximum Time,to Service,See Adaptation Channel 044
014,3,Adaptation,Channel
014,4,Minimum Time to Service,See Adaptation Channel 049
;
015,0,Adaptation Channel 045
015,1,Adaptation,Channel
015,2,Oil Quality,,See Adaptation Channel 045
;
016,0,Adaptation Channels 047 && 048
016,1,Adaptation,Channel
016,2,Soot Entry,,See Adaptation Channel 047
016,3,Adaptation,Channel
016,4,Thermal Load,,See Adaptation Channel 048
;
019,0,Adaptation Channel 030
019,3,Adaptation,Channel
019,4,Fuel Gauge,Sender 1,See Adaptation Channel 030
;
020,0,Adaptation Channels 035 && 037
020,1,Adaptation,Channel
020,2,Engine Speed,Threshold,See Adaptation Channel 035
020,3,Adaptation,Channel
020,4,Breake Wear,Indicator Install.,See Adaptation Channel 037
;
021,0,Adaptation Channels 038 && 039
021,1,Adaptation,Channel
021,2,Oil Minimum,Detection Sensor,See Adaptation Channel 038
021,3,Adaptation,Channel
021,4,TOG,Installation,See Adaptation Channel 039
;
022,0,Adaptation Channels 018 && 020
022,1,Adaptation,Channel
022,2,Auxiliary,Heating,See Adaptation Channel 018
022,3,Adaptation,Channel
022,4,Configuration,,See Adaptation Channel 020
;
023,0,Adaptation Channels 080 && 081
023,1,Adaptation,Channel
023,2,Day/Month,of Delivery,See Adaptation Channel 080
023,3,Adaptation,Channel
023,4,Year,of Delivery,See Adaptation Channel 081
;
024,0,Adaptation Channels 082 && 033
024,1,Adaptation,Channel
024,2,Comfort Menu,,See Adaptation Channel 082
024,3,Adaptation,Channel
024,4,Full Calibration,,See Adaptation Channel 033
;
026,0,Fuel Level Sender
026,1,Fuel Sender 1,(Resistance)
026,2,Fuel Sender 1,(Tank Content)
026,3,Fuel Sender 2,(Resistance)
026,4,Fuel Sender 2,(Tank Content)
;
050,1,Mileage
050,2,Engine Speed
050,3,Coolant,Temperature
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
082,0,Advanced Control Module Identification III
;
120,0,Connector Status I
120,1,Brake Fluid,Connector
120,2,Washer Fluid,Connector
120,3,Coolant Level,Connector
120,4,Oil Level,Connector
;
121,0,Connector Status II
121,1,Brake Pad Waer,Indicator Connect.
121,2,Parking Brake
121,3,Learned Keys
121,4,S-Contact,Status
;
122,0,Seat Belt Inquiry
122,1,Seat Belt Inquiry,Driver,Display Range: Open/Closed
122,2,Seat Belt Inquiry,Passenger,Display Range: Open/Closed
;
125,0,CAN-Databus Communication (Powertrain)
125,1,CAN-Gateway,,Specification: Gateway 1
;
;
;---------------------------------------------------
;
; security access informations
;
;---------------------------------------------------
;
;
S0,Instrument Cluster (J285) Security Access
S1,13861 - General Adaptation "Enabling"
;
;
;---------------------------------------------------
;
; adaptation informations
;
;---------------------------------------------------
;
;
A2,0,Service Reminder
A2,5,Service Reminder
A2,6,0 - Service NOT Due
A2,7,1 - Service Due
A2,8, 
A2,9,To reset the service reminder save 00000 as new value.
;
A3,0,Consumption Correction
A3,5,Consumption Correction
A3,6,Standard Value: 100 %
A3,7,Display Range: 85...115 %
A3,8,Increments: 5 %
A3,9, 
A3,10,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
;
A4,0,Language
A4,5,Language
A4,6,00001 - German
A4,7,00002 - English (also Japan and Arabic States)
A4,8,00003 - French
A4,9,00004 - Italian
A4,10,00005 - Spanish (also Mexico)
A4,11,00006 - Portuguese/Brazil 
;
A038,0,Oil Minimum Detection
A038,5,Oil Minimum Detection
A038,6,With this function the oil-minimum-warning at
A038,7,low oil level can be deactivated or activated.
A038,8, 
A038,9,NOTE: Perform Security Access with "13861" first.
;
A039,0,Oil Level Sensor Adaptation
A039,5,Oil Level Sensor Adaptation
A039,6,Determines if the TOG Sensor is installed or not.
A039,7, 
A039,8,NOTE: Perform Security Access with "13861" first.
;
A40,0,Mileage since Service
A40,5,Mileage since Service
A40,6,Increments: 1 = 100 km
A40,7, 
A40,8,NOTE: Adaptation channels 40-49 must be
A40,9,entered and stored in the following order:
A40,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A41,0,Time since Service
A41,5,Time since Service
A41,6,Increments: 1 = 1 day(s)
A41,7, 
A41,8,NOTE: Adaptation channels 40-49 must be
A41,9,entered and stored in the following order:
A41,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A42,0,Minimum Mileage to Service
A42,5,Minimum Mileage to Service
A42,6,Increments: 1 = 100 km
A42,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A42,8,00150 - flexible Service Intervals (15.000 km - with Longlife)
A42,9,or (if coded to miles)
A42,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A42,11,00090 - flexible Service Intervals (9.000 mi - with Longlife)
A42,12, 
A42,13,NOTE: Adaptation channels 40-49 must be
A42,14,entered and stored in the following order:
A42,15,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A43,0,Maximum Mileage to Service
A43,5,Maximum Mileage to Service
A43,6,Increments: 1 = 100 km
A43,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A43,8,00300 - flexible Service Intervals (30.000 km - with Longlife)
A43,9,or (if coded to miles)
A43,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A43,11,00190 - flexible Service Intervals (19.000 mi - with Longlife)
A43,12, 
A43,13,NOTE: Adaptation channels 40-49 must be
A43,14,entered and stored in the following order:
A43,15,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A44,0,Maximum Time to Service
A44,5,Maximum Time to Service
A44,6,Increments: 1 = 1 day(s)
A44,7,00365 - fixed Service Intervals (w/o Longlife)
A44,8,00730 - flexible Service Intervals (with Longlife)
A44,9, 
A44,10,NOTE: Adaptation channels 40-49 must be
A44,11,entered and stored in the following order:
A44,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A45,0,Oil Quality
A45,5,Oil Quality
A45,6,1 - fixed Service Intervals (w/o Longlife)
A45,7,2 - flexible Service Intervals (with Longlife)
A45,8, 
A45,9,NOTE: Adaptation channels 40-49 must be
A45,10,entered and stored in the following order:
A45,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A46,0,Total Consumption
A46,5,Total Consumption
A46,6,This value does not represent the actual consumption
A46,7,but is rather an arithmetic value for the service interval display
A46,8, 
A46,9,NOTE: Adaptation channels 40-49 must be
A46,10,entered and stored in the following order:
A46,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A47,0,Soot Entry
A47,5,Soot Entry
A47,6,Arithmetic value used to calculate the amount of soot in
A47,7,the engine oil referenced to a distance of 100 km and used
A47,8,as comparison value for the service interval display.
A47,9, 
A47,10,NOTE: Adaptation channels 40-49 must be
A47,11,entered and stored in the following order:
A47,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A48,0,Thermal Load
A48,5,Thermal Load
A48,6,Arithmetic value used to calculate the thermal stress of
A48,7,the engine oil referenced to a distance of 100 km and used
A48,8,as comparison value for the service interval display.
A48,9, 
A48,10,NOTE: Adaptation channels 40-49 must be
A48,11,entered and stored in the following order:
A48,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A49,0,Minimum Time to Service
A49,5,Minimum Time to Service
A49,6,Increments: 1 = 1 day(s)
A49,7,00365 - fixed Service Intervals (w/o Longlife)
A49,8,00365 - flexible Service Intervals (gasoline engines with Longlife)
A49,9,00730 - flexible Service Intervals (diesel engines with Longlife)
A49,10, 
A49,11,NOTE: Adaptation channels 40-49 must be
A49,12,entered and stored in the following order:
A49,13,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
;
;---------------------------------------------------
;
; coding informations
;
;---------------------------------------------------
;
;
C0,Instrument Cluster (J285) Coding
C1,??xxx: Equipment
C2,+01 = 2nd Fuel Tank Characteristic (All-Wheel Drive)
C3,+02 = Highline without DIS (for Midline variant 9Q3 - Automatic without DIS)
C4,+04 = Manual Transmission (not midline variant 9Q3)
C5,+08 = 2nd tire circumference pair (e.g. winter tires)
C5,+32 = AFS (Advanced Front Lighting System (cornering lights)
C6,xx?xx: Country
C7,0 = Germany / 1 = Rest of World (RoW - Left Hand Steering) / 2 = USA / 3 = Canada
C8,4 = Great Britain (Right Hand Steering) / 5 = Japan (Left Hand Steering) / 6 = Arabien States
C9,7 = Australia / 8 = Rest of World (RoW - Right Hand Steering) / 9 = Japan (Right Hand Steering)
C10,xxx?x: Seat Belt Warning
C11,0 - No Seat Belt Warning
C12,1 = Europe-NCAP (permanent visual warning and acoustic warning active for 91 seconds)	
C13,2 = USA and Canada OLD (visual and acoustic warning for 6 seconds)	
C14,3 = USA and Canada NAR-NEW (permanent visual warning and acoustic warning active every 30 seconds)
C15,4 = Europe-NCAP (including passenger - permanent visual warning and acoustic warning active for 91 seconds)	
C16,5 = USA and Canada OLD (including passenger - visual and acoustic warning for 6 seconds)	
C17,6 = USA and Canada NAR-NEW (including passenger - permanent visual warning and acoustic warning active every 30 seconds)
;
