;
; VAG-COM label file
;
; VW Golf IV / Bora / Jetta IV (1J)
;
; component: J285 - instrument cluster (#17)
;
; p/n: 1J?-920-??0-???
;      1J?-920-??1-???
;      1J?-920-??2-???
;      1J?-920-??5-???
;
; tested with: 1J0 920 900 K
;              1J0 920 825 C
;              1J5 920 845 A
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1J-17.LBL
; 1J0-919-xxx.LBL
; 1J0-920-xx0.LBL
; 1J0-920-xx6.LBL
; 1J0-920-xx7.LBL
;
; created on 10/Aug/2004 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 15/Apr/2005
;
; requires VAG-COM 405.0 or newer
;
;---------------------------------------------------
;
; Measuring block informations
;
;---------------------------------------------------
;
001,0,Speed / Engine speed / Oil pressure / Time
001,1,Speed
001,2,Engine Speed
001,3,Oil pressure, 0.9 bar
001,4,Time
;
002,0,Distance / Fuel / Ambient temperature
002,1,Odometer
002,2,Fuel level (l)
002,3,Fuel Sender,Resistance
002,4,Ambient,temperature,MFD only
;
003,0,Coolant and Oil
003,1,Coolant Temp
003,2,Oil level,(Ok/n.Ok)
003,3,Oil,temperature
003,4,[N/A]
;
020,0,Immobilizer - ID Block 1
020,1,Digit 1 && 2
020,2,Digit 3 && 4
020,3,Digit 5 && 6
020,4,Digit 7 && 8
;
021,0,Immobilizer - ID Block 2
021,1,Digit 9 && 10
021,2,Digit 11 && 12
021,3,Digit 13 && 14
021,4,[N/A]
;
022,0,Immobilizer
022,1,Starting,permitted
022,2,Engine (ECM),responds
022,3,Key condition,OK
022,4,Number of,keys coded
;
023,0,Immobilizer
023,1,Variable code,authorized
023,2,Key status,(transponder)
023,3,Fixed code,authorized
023,4,Immobilizer,status,see labelfile
; 4 - new customer service - delivery condition (replacement part instrument cluster)
; 5 - customer service locked - adaptation data programmed in customer service
; 6 - immobilizer adapted - normal function condition
; 7 - key adaptation active - key adaptation via tester
;
050,0,Misc
050,1,Odometer
050,2,Engine Speed
050,3,Oil,temperature
050,4,Coolant,temperature
;
125,0,CAN-Databus communication (Powertrain)
125,1,Engine
125,2,Transmission
125,3,ABS
125,4,[N/A]
;
126,0,CAN-Databus communication (Powertrain)
126,1,Steering,sensor
126,2,Airbag
126,3,[N/A]
126,4,[N/A]
;
;
;---------------------------------------------------
;
; Adaptation informations
;
;---------------------------------------------------
;
;
A2,0,Service reminder
A2,5,Service reminder reset
A2,6,displayed values:
A2,7,0 - no service
A2,8,1 - service
A2,9, 
A2,10,reset:
A2,11,0 - Service reminder reset
;
A3,0,Consumption display
A3,5,consumption display adaption
A3,6,Basic value: 100
A3,7,Range: 85 - 115
A3,8,Unit: 5 % (percent)
;
A4,0,Language for error messages and navigation (MFD only)
A4,5,Language for error messages and navigation
A4,6,1 - German
A4,7,2 - English
A4,8,3 - French
A4,9,4 - Italian
A4,10,5 - Spanish
A4,11,6 - Portuguese
A4,12,8 - Czech
;
A9,0,Dinstance (in 10km)
A9,1,Distance
A9,2,in 10
A9,3,km
A9,5,Distance changing
A9,6,Before the cluster accepts the new
A9,7,distance you have to login using 13861.
A9,8, 
A9,9,The distance can only be changed until
A9,10,the current value is not over 100km.
;
A16,0,Distance impulse identifier (read only)
;
A21,0,Key count (Immobilizer)
A21,1,Old Key
A21,2,count
A21,3,[count]
;
A30,0,Fuel gauge adaption
A30,1,Current,value
A30,5,Fuel gauge adaption
A30,6,Basic value: 100
A30,7,Range: 120 - 136
A30,8,Unit: 1 Ohm
;
A35,0,Engine speed threshold
A35,5,Engine speed threshold adaption
A35,6,Basic value: 0
A35,7,Range: 0 - 1000
A35,8,Unit: 250 U/min
;
A40,0,Distance from inspection
A40,5,Distance from inspection
A40,6,Resolution: 1 = 100 km
A40,7, 
A40,8,NOTE: Adaptation channels 40-44 must be
A40,9,entered and stored in the following order:
A40,10,42 > 43 > 44 > 40 > 41
;
A41,0,Time from inspection
A41,5,Time from inspection
A41,6, 
A41,7,NOTE: Adaptation channels 40-44 must be
A41,8,entered and stored in the following order:
A41,9,42 > 43 > 44 > 40 > 41
;
A42,0,Minimum value mileage
A42,5,Minimum value mileage
A42,6,Resolution: 1 = 1000 km
A42,7, 
A42,8,NOTE: Adaptation channels 40-44 must be
A42,9,entered and stored in the following order:
A42,10,42 > 43 > 44 > 40 > 41
;
A43,0,Maximum value mileage
A43,5,Maximum value mileage
A43,6,Resolution: 1 = 1000 km
A43,7, 
A43,8,NOTE: Adaptation channels 40-44 must be
A43,9,entered and stored in the following order:
A43,10,42 > 43 > 44 > 40 > 41
;
A44,0,Maximum time interval
A44,5,Maximum time interval
A44,6, 
A44,7,NOTE: Adaptation channels 40-44 must be
A44,8,entered and stored in the following order:
A44,9,42 > 43 > 44 > 40 > 41
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,Instrument Cluster (J285) Coding
C1,??xxx - Additional equipment
C2,+00 - Without additional equipment
C3,+01 - Brake pad warning
C4,+02 - Seatbelt warning
C5,+04 - Washer fluid level warning
C6,+16 - Radio/Navigation
C7,xx?xx - Country version
C8,1 - Europe / 2 - USA / 3 - Canada/Mexico/Latin America
C9,4 - England / 5 - Japan / 6 - Saudi Arabia / 7 - Australia
C10,xxx?x - Service intervals
C11,0 - mini-service intervals without oil level/temperature sensor
C12,1 - flexible service intervals with oil level/temperature sensor
C13,2 - fixed service intervals with oil level/temperature sensor
C14,3 - without service intervals (USA/Canada)
C15,xxxx? - Distance impulse number (K-value)
C16,1 - 4358 (1,4l/55kW AHW/AKQ with manual transmission)
C17,2 - 3538 (all other engine  codes and/or automatic transmission)
C18,3 - 4146 (1,6l/74-77kW and 1,9l/50kW-SDI with manual transmission)
C19,4 - 3648 (unknown)
;
