;
; VAG-COM Labelfile
;
; Audi A6 (4F)
;
; Component: J540 - Parking Brake (#53)
;
; P/N: 4F0-910-801-???
;
; includes measuring blocks, coding and selective output test
;
; created on 16/Oct/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 16/oct/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Parking Brake (J540) Coding
C01,000??xx: Engine
C02,01 - 2.0l TDI (Diesel)
C03,03 - 3.0l TDI (Diesel)
C04,05 - 2.7l TDI (Diesel)
C05,10 - 2.0l TFSI (Gasoline)
C06,20 - 2.4l MPI (Gasoline)
C07,30 - 2.8l FSI (Gasoline)
C08,40 - 3.0l MPI (Gasoline)
C09,50 - 3.2l FSI (Gasoline)
C10,60 - 4.2l MPI (Gasoline)
C11,70 - 4.2l FSI (Gasoline)
C12,000xx?x: Transmission 		
C13,1 - Manual Transmission
C14,2 - Automatic Transmission (09L/09E)
C15,3 - Multitronic (01J)
C16,000xxx?: Country
C17,1 - Rest of World (RoW)
C18,2 - USA/Canada
C19,3 - Japan
;
;
;---------------------------------------------------
;
; selective output test information
;
;---------------------------------------------------
;
;
T401,Acoustic Signal Sensor
T2440,Function Display in Instrument Cluster (P)
; 2417 aftwards necessary to deactivate
T2441,Yellow Malfunction Lamp in Instrument Cluster
; 2417 aftwards necessary to deactivate
T2442,Function Lamp in Control Head
; 2417 aftwards necessary to deactivate
T2417,Lights Switched Off
T2573,Control Circuit for Left Actuator
; 2576 to activate that output
T2575,Control Circuit for Right Actuator
; 2576 to activate that output
T2576,Actuator(s) being Opened
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,General
001,1,System,Configuration
; xxxxxxx? = Readiness Bit "Assembly Check" (0 = OK / 1 = not OK)
; xxxxxx?x = Readiness Bit "System Calibration" (0 = OK / 1 = not OK)
; xxxxx?xx = Airbag Belt Lock "DAA" (0 = OFF / 1 = ON "Standard")
; xxxx?xxx = Auto-Hold (0 = active / 1 = inactive)
; xxx?xxxx = Pad Replacement Mode (1 = Standard)
; xx?xxxxx = RWU-ECD Functionality (0 = ECD active / 1 = RWU active)
; x?xxxxxx = Opening with Brake Pedal (0 = Opening w/o Brake Pedal / 1 = No Opening w/o Brake Pedal)
; ?xxxxxxx = Readiness Bit "End-Of-Line" (0 = Successfully coded / 1 = EOL not completed)
001,2,Brake Pad,Replacement Mode,
; x111xxx? = Left Brake Open
; x111xx?x = Right Brake Open
; x111x?xx = Left Fuse removed
; x111?xxx = Right Fuse removed
; ?111xxxx = Maintenance Mode active
;11111111,Bin. Bits,
001,3,Maximum ECD,Deceleration,Specification: 2.0...8.0 m/s²
001,4,Transmission,Type,?1111111 = Transmission Type (0 = Manual / 1 = Automatic)
;
002,0,General
002,1,Internal Battery,Voltage,Specification: min. 10 V
002,2,Pressure Switch,,Display Range: Open/Closed/Not Oper.
002,3,Current Vehicle,Inclination Angle
002,4,Brake Temperature,(Calculated),Specification: max. 500.0 °C
;
003,0,Brake Status
003,1,Shut-Off Current,Left (Calculated),Specification: min. 15.0 A
003,2,Shut-Off Current,Right (Calculated),Specification: min. 15.0 A
003,3,Brake Status,(Left),0 = Open\n8 = Closed\n11 = Faulty
003,4,Brake Status,(Right),0 = Open\n8 = Closed\n11 = Faulty
;
007,0,Operating Counter
;
008,0,Clutch Pedal Travel
008,2,Clutch Pedal,Travel,Display Range: 0...250 (0...100 %)\n255 = Invalid Value (or Automatic Transmission)
;
099,0,Versions
099,1,Software
099,2,Software Version
099,3,Hardware
099,4,Hardware Version
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Brake,Electronics (J104),Specification: ABS 1\nDisplay Range: ABS 1/ABS 0
125,2,Airbag System,(J255),Specification: Airbag 1\nDisplay Range: Airbag 1/Airbag 0
125,3,Transmission,Electronics,Specification: Transm. 1\nDisplay Range: Transm. 1/Transm. 0
125,4,Engine,Electronics,Specification: Engine 1\nDisplay Range: Engine 1/Engine 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,CAN-Gateway,(J533),Specification: Gateway 1\nDisplay Range: Gateway 1/Gateway 0
126,2,Instrument Cluster,(J285),Specification: Instruments 1\nDisplay Range: Instruments 1/Instruments 0
126,3,Electrical,Ignition Lock,Specification: El.Ign.Lock 1\nDisplay Range: El.Ign.Lock 1/El.Ign.Lock 0
;
225,0,CAN-Databus Powertrain (Timeout)
225,1,Brake,Electronics (J104)
225,2,Airbag System,(J255)
225,3,Transmission,Electronics
225,4,Engine,Electronics
;
226,0,CAN-Databus Powertrain (Timeout)
226,1,CAN-Gateway,(J533)
226,2,Instrument Cluster,(J285)
226,3,Electrical,Ignition Lock
;
