;
; VAG-COM Labelfile
;
; Seat Altea/Toledo (5P) / Skoda Octavia II (1Z)
; VW Caddy (2K) / VW Fox (5Z) / VW Golf/Jetta (1K) / VW Touran (1T)
;
; Component: R - Radio (#56)
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-56.LBL
; 1Z-56.LBL
; 5M-56.LBL
; 5P-56.LBL
; 5Z-56.LBL
; 1K0-035-1xx-56.LBL
;
; created on 23/Mar/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 15/Nov/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,1,Supply Voltage,(Terminal 30),Specification: 5...18 V
001,2,Amplifier,Output,only if Amplifier installed
001,3,Dimming of,Radio Illumination,CAN-Message (Specification: ca. 29...98 %
001,4,S-Contact,Input Condition,CAN-Message
;
002,0,Telephone
002,1,Component
002,2,Mute Status
002,4,Status
;
003,0,Speaker/Line-Out (Front Left)
003,1,Location/Type
003,2,Status
;
004,0,Speaker/Line-Out (Front Right)
004,1,Location/Type
004,2,Status
;
005,0,Speaker/Line-Out (Rear Left)
005,1,Location/Type
005,2,Status
;
006,0,Speaker/Line-Out (Rear Right)
006,1,Location/Type
006,2,Status
;
007,0,Remote Feed Antenna I
007,1,Type
007,2,Component
007,3,Status
;
008,0,Signal Strength
008,1,Signal Strength
008,2,Signal Strength,Tuner I
008,3,Signal Strength
008,4,Signal Strength,Tuner II
;
010,0,Remote Feed Antenna II
010,1,Type
010,2,Component
010,3,Status
;
011,0,Communication Status CD-Changer (R41)
011,1,Component
011,2,Status
;
016,0,CAN Connection Satelite Radio Receiver (SDARS)
;
025,0,Internal Control Module Malfunctions
025,1,Control Module,Status
; 01 = Button(s) Jam
; 02 = Checksum Error ROM/EPROM/Flash-ROM
; 03 = Writing Error EEPROM
; 04 = CC-Drive (Casette) Error
; 05 = CD/DVD-Drive Error
; 09 = Malfunction at CD/DVD-Drive
; 0A = Internal Communication (BUS)
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A01,0,Reception Optimization
A01,5,Reception Optimization
A01,6,This channel allows optimization of the reception
A01,7,behavior for areas with strong FM interference.
A01,8, 
A01,9,0 - Normal reception
A01,10,1 - Optimized reception
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,Radio (R) Coding
C1,?xxxx - Treble Speaker Monitoring
C2,1 - front and rear monitoring inactive
C3,2 - front monitoring active - rear monitoring inactive
C4,4 - front and rear monitoring active
C5,x?xxx - Telephone Control
C6,0 - no CAN-Telephone Control
C7,2 - CAN-Telephone Control
C8,xx?xx - Speaker channels
C9,0 - no passive speakers (sound system)
C10,2 - 2 passive speakers front and 0 passive speakers rear
C11,4 - 4 passive speakers
C12,xxx?x - Sound system correction
C13,0 - No sound system (no correction)
C14,1 - Sound system with cloth interior equipment
C15,2 - Sound system with leather interior equipment
C16,xxxx? - Radio configuration
C17,+2 - CD-Changer
C18,+4 - CAN-Secondary Display (Board Computer/large Display)
;
