; For Audi A3 (8P), no guaranties
Byte 00 Bit 0 Fog light installed
Byte 00 Bit 1 Xenon head lights with shutter installed
Byte 00 Bit 2 Footwell light installed
Byte 00 Bit 3 Daytime driving lights (Scandinavia) active
Byte 00 Bit 4 Daytime driving lights (North America) active
Byte 00 Bit 5 Assistance driving light with Leaving-Home
Byte 00 Bit 6 Rain-/Light sensor installed
Byte 00 Bit 7 Coming-Home installed
Byte 01 Bit 0 Rear seat recognition installed
Byte 01 Bit 1 Front Head light washer installed
Byte 01 Bit 2 Electronic fuelpump relay installed
Byte 01 Bit 3 Rear wiper installed
Byte 01 Bit 4 Heated side mirror installed
Byte 01 Bit 5 Rear hatch remote opening
Byte 01 Bit 6 Rear hatch remote opening allowed - active
Byte 01 Bit 7 Rear Wiper active when driving backwards with continuesly wiper in front
Byte 02 Bit 0 Rear Wiper active when driving backwards with intermit wiper in front
Byte 02 Bit 1 Automatic turn signal on Highway when changing lane (press turn signal arm light)
Byte 02 Bit 2 Cold lamp diagnostics (no light on) (mandatory)
Byte 02 Bit 3 Loadmanagement (mandatory)
Byte 02 Bit 4 Coming-Home Mode by		(0 = Adaption / 1 = Potentiometer)
Byte 02 Bit 5 Rear lid remote openening	(0 = impuls activated / 1 = contact activated)
Byte 02 Bit 6 Side turn signal lights installed 
Byte 02 Bit 7 Seat heating installed
Byte 03 Bit 0 Relay pin 15 inside installed
Byte 03 Bit 1 Rear fog light active (0 = 2 rear fog lights / 1 = 1 rear fog lights)
Byte 03 Bit 2 Reverse driving light active (0 = 2 reverse driving lights / 1 = 1 reverse driving lights)
Byte 03 Bit 3 Reverse driving light switched off when rear lid is open
Byte 03 Bit 4 Xenon head lights without shutter installed
Byte 03 Bit 5 Rear Wiper on, one time after normal wiper cycle (drip function)
Byte 03 Bit 6 Second battery installed
Byte 03 Bit 7 Rear light activation (0 = rear light dimmed / 1= rear light/Brake light dimmed)
Byte 04 Bit 0 Cabinheater installed
Byte 04 Bit 1 Extra airheater installed
Byte 04 Bit 2 Trailer Connection Unit installed
Byte 04 Bit 3 Electrical seat adjustment with memory
Byte 04 Bit 4 Activation of both rear fog lights installed
Byte 04 Bit 5 0 = Right hand drive (PR-L0R) / 1 = Left hand drive (PR-L0L)
Byte 04 Bit 6 Rear fog light not active
Byte 04 Bit 7 Automatic airconditioning installed
Byte 05 Bit 0 Front light cleaning delay - Resolution 50ms
Byte 05 Bit 1 - Decimal value multiply resolution
Byte 05 Bit 2 - For example: Byte decimal value: 20 is 20 x 50 = 1000 ms
Byte 05 Bit 3 
Byte 05 Bit 4 
Byte 05 Bit 5 
Byte 05 Bit 6 
Byte 05 Bit 7 
Byte 06 Bit 0 Front light cleaning activation time - Resolution 50ms
Byte 06 Bit 1 - Decimal value multiply resolution
Byte 06 Bit 2 - For example: Byte decimalvalue: 16 is 16 x 50 = 800 ms
Byte 06 Bit 3 
Byte 06 Bit 4 
Byte 06 Bit 5 
Byte 06 Bit 6 
Byte 06 Bit 7 
Byte 07 Bit 0 Extra function turn signal front left/right as parkinglight front left/right (USA and Canada)
Byte 07 Bit 1 - Decimalvalue (Resolution 1%)
Byte 07 Bit 2 
Byte 07 Bit 3 
Byte 07 Bit 4 
Byte 07 Bit 5 
Byte 07 Bit 6 
Byte 07 Bit 7 
Byte 08 Bit 0 Day light dimming
Byte 08 Bit 1 - Decimalvalue (Resolution 1%)
Byte 08 Bit 2 
Byte 08 Bit 3 
Byte 08 Bit 4 
Byte 08 Bit 5 
Byte 08 Bit 6 
Byte 08 Bit 7 
Byte 09 Bit 0 Extra function Brake light left/right as rear parkinglight
Byte 09 Bit 1 - Decimalvalue (Resolution 1%)
Byte 09 Bit 2 
Byte 09 Bit 3 
Byte 09 Bit 4 
Byte 09 Bit 5 
Byte 09 Bit 6 
Byte 09 Bit 7 
Byte 10 Bit 0 Extra function rear fog light left/right as parkinglight
Byte 10 Bit 1 - Decimalvalue (Resolution 1%)
Byte 10 Bit 2 
Byte 10 Bit 3 
Byte 10 Bit 4 
Byte 10 Bit 5 
Byte 10 Bit 6 
Byte 10 Bit 7 
Byte 11 Bit 0 Extra function front parking light left/right
Byte 11 Bit 1 - Decimalvalue (Resolution 1%)
Byte 11 Bit 2 
Byte 11 Bit 3 
Byte 11 Bit 4 
Byte 11 Bit 5 
Byte 11 Bit 6 
Byte 11 Bit 7 
Byte 12 Bit 0 Parking light left/right dimming
Byte 12 Bit 1 - Decimalvalue (Resolution 1%)
Byte 12 Bit 2 
Byte 12 Bit 3 
Byte 12 Bit 4 
Byte 12 Bit 5 
Byte 12 Bit 6 
Byte 12 Bit 7 
Byte 13 Bit 0 Replacement function front Side turn signal left/right as front Parking light left/right
Byte 13 Bit 1 - Decimalvalue (Resolution 1%)
Byte 13 Bit 2 
Byte 13 Bit 3 
Byte 13 Bit 4 
Byte 13 Bit 5 
Byte 13 Bit 6 
Byte 13 Bit 7 
Byte 14 Bit 0 Replacement function front Parking light left/right as front Side turn signal left/right
Byte 14 Bit 1 - Decimalvalue (Resolution 1%)
Byte 14 Bit 2 
Byte 14 Bit 3 
Byte 14 Bit 4 
Byte 14 Bit 5 
Byte 14 Bit 6 
Byte 14 Bit 7 
Byte 15 Bit 0 Replacement function Back light left/right as rear Side turn signal left/right
Byte 15 Bit 1 - Decimalvalue (Resolution 1%)
Byte 15 Bit 2 
Byte 15 Bit 3 
Byte 15 Bit 4 
Byte 15 Bit 5 
Byte 15 Bit 6 
Byte 15 Bit 7 
Byte 16 Bit 0 Replacement function fog head light left/right as head light low beam left/right
Byte 16 Bit 1 - Decimalvalue (Resolution 1%)
Byte 16 Bit 2 
Byte 16 Bit 3 
Byte 16 Bit 4 
Byte 16 Bit 5 
Byte 16 Bit 6 
Byte 16 Bit 7 
Byte 17 Bit 0 Ermergency brake flash light active
Byte 17 Bit 1 Deactivation of High beam light with Bi-Xenon
Byte 17 Bit 2 Heated frontwindow installed
Byte 17 Bit 3 Diagnostics pin 50 active
Byte 17 Bit 4 Day light driving with dimmed Head light low beam
Byte 17 Bit 5 Fog light deactivated when Head light high beam
Byte 17 Bit 6 Park light function USA/Canada active
Byte 17 Bit 7 Free
Byte 18 Bit 0 Cold diagnostics License plate light active
Byte 18 Bit 1 Cold diagnostics Brake light active
Byte 18 Bit 2 Cold diagnostics Fog headlight active
Byte 18 Bit 3 Cold diagnostics Rear Foglight active
Byte 18 Bit 4 Cold diagnostics Head light high beam active
Byte 18 Bit 5 Cold diagnostics Turn signal active
Byte 18 Bit 6 Cold diagnostics Back light active
Byte 18 Bit 7 Cold diagnostics Side turn signal active
Byte 19 Bit 0 Cold diagnostics Head light low beam active
Byte 19 Bit 1 Cold diagnostics Front Parking light active
Byte 19 Bit 2 Cold diagnostics Rear Parking light active
Byte 19 Bit 3 Diagnostic Rear Parking light active
Byte 19 Bit 4 Relay pin 75 mounted
Byte 19 Bit 5 Relay pin 15 engine room installed
Byte 19 Bit 6 Free
Byte 19 Bit 7 Free
Byte 20 Bit 0 Fog light dimming
Byte 20 Bit 1 - Decimalvalue (Resolution 1%)
Byte 20 Bit 2 
Byte 20 Bit 3 
Byte 20 Bit 4 
Byte 20 Bit 5 
Byte 20 Bit 6 
Byte 20 Bit 7 
Byte 21 Bit 0 Front light variant
Byte 21 Bit 1 Front light variant
Byte 21 Bit 2 Front light variant
Byte 21 Bit 3 Reserved (Front light variant)
Byte 21 Bit 4 Rear fog light active as Brake light
Byte 21 Bit 5 Free
Byte 21 Bit 6 Free
Byte 21 Bit 7 Free
Byte 22 Bit 0 Free
Byte 22 Bit 1 Free
Byte 22 Bit 2 Free
Byte 22 Bit 3 Free
Byte 22 Bit 4 Free
Byte 22 Bit 5 Free
Byte 22 Bit 6 Free
Byte 22 Bit 7 Free
