;
; VAG-COM label file
;
; Seat Leon/Toledo / (1M) Skoda Octavia (1U)
; VW Golf/Jetta (1J) / VW Passat (3B)
;
; component: J136 - Driver's Seat Adjustment (#36)
;
; p/n: 3B1 959 760 ?
;
; includes measuring blocks
;
; created on 15/April/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Basic Informations
001,1,Individual,Switch Positions,Display Range: 0 = not pressed/1 = pressed (?xx = P1/x?x = P2/xx? = P3)
001,2,MEM-OFF Button,Door Contact,Display Range 0 = off / 1 = on (?x = MEM-OFF Button/x? = Door Contact)
001,3,Key-Number
;
002,0,Actual Status
002,1,Seat Fore/Aft,Adjustment Button,Display Range: forward/backward/not operated/implausible
002,2,Actual Seat Fore/Aft,Adjustment,Display Range: 0...65535 | Central Position: 32767 | Not Initialised: 30000
002,3,Backrest Angle,Adjustment Button,Display Range: forward/backward/not operated/implausible
002,4,Actual Backrest,Angle Adjustment,Display Range: 0...65535 | Central Position: 32767 | Not Initialised: 30000
;
003,0,Actual Status
003,1,Seat Height,Adjustment Button,Display Range: raise/lower/not operated/implausible
003,2,Actual Seat Height,Adjustment,Display Range: 0...65535 | Central Position: 32767 | Not Initialised: 30000
003,3,Seat Angle,Adjustment Button,Display Range: raise/lower/not operated/implausible
003,4,Actual Seat Angle,Adjustment,Display Range: 0...65535 | Central Position: 32767 | Not Initialised: 30000
;
004,0,Mirrors
004,1,Driver's Side,Potentiom. X-Pos.,Display Range: 1...99 %
004,2,Driver's Side,Potentiom. Y-Pos.,Display Range: 1...99 %
004,3,Passenger's Side,Potentiom. X-Pos.,Display Range: 1...99 %
004,4,Passenger's Side,Potentiom. Y-Pos.,Display Range: 1...99 %
;
005,0,Switch Positions
005,1,Voltage,(Terminal 30)
005,2,Inputs and,Initialisation,Display Range: 0 = off/1 = on (?xx = Terminal X/x?x = Reversing Switch/xx? = Init Mode)
005,3,Last Reason,for switch-off,Display Range: 0 = off/1 = on (?xx = Block/x?x = Soft Stop/xx? = Running Period)
;
006,0,Databus Communication (Comfort)
006,1,Status,Databus Comfort
;
