;
; VAG-COM label file
;
; Seat Ibiza (6K)
;
; component: Radio system (#56)
;
; p/n: 6K0-035-156
;
; includes measuring blocks, coding information and adaption information
;
; created on 27/Nov/2005 by Jose Carlos Fernandez (josecarlosfernandez@terra.es)
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
1,0,,
1,1,-
1,2,Voltage BNE 30,(voltage),– Measurement after filtering 
1,3,Light on,display (%),Reduction in light on display- by means of panel lighting regulator\n– Minimum 20%\n– Maximum 100%
1,4,S contact,status 
;
2,0,Speakers,
2,1,Front speaker
2,2,State of,front speaker,- OK\n- Short-circuit\n- Break
2,3,Rear speakers
2,4,State of,rear speaker,- OK\n- Short-circuit\n- Break
;
3,0,Aerial,
3,1,Aerial type,,– Passive \n– Active (e.g. Aerial on rear window)
3,2,Aerial
3,3,State of,the aerial,- OK\n- Short-circuit\n- Break
;
4,0,Amplifier / Telephone
4,1,State of,active amplifier,State of active amplifier control outlet\n– 0 = State OK\n– 1 = Shorting with ground
4,2,,-
4,3,Telephone
4,4,State of muter,for telephone,State of muter inlet for telephone \n– Telephone working = “ON”\n– Telephone not working = “OFF”
;
5,0,CD connection
5,1,CD connection
5,2,State of,CD connection,State of the connection for CD\n– OK\n– Not OK
;
6,0,,
6,1,,-
6,2,,- 
;
7,0,Remote control from steering wheel
7,1,Steering wheel,remote control,Remote control from steering wheel in operative reception mode\n– The number of each key activated is visualised
7,2,Statate of,signal 
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C0,Radio system
C1,?0xxx: Country identification
C2,0 - Europe / 1 - USA 
C3, 
C4,x0?xx: Number of passive speakers
C5,0 - 0 No passive speakers                                    
C6,1 - 1 passive speaker - front left                           
C7,2 - 2 passive speakers - front right                         
C8,3 - 3 passive speakers - rear                                
C9,4 - 4 passive speakers                                       
C10,5 - 2 passive speakers - front and no active speakers in rear
C11, 
C12,x0x?x: Correction of the sound system
C13,0 - No correction
C14,1 - BOSE
C15,2 - DSP
C16, 
C17,x0xx?: Radio set-up
C18,+1 - Aerial with remote supply installed
C19,+2 - CD changer installed
C20,+4 - Second display installed
;
;
;---------------------------------------------------
;
; Adaptation informations
;
;---------------------------------------------------
;
;
;No adaption channel available
;
